R=Reserve resistor or capcitor







AVS\_VDDFB is the output of the Ethernet switch IC.