("FILE_TYPE"	"PMAP File"
    ("devices"
        ("R")
        ("C")
        ("ES1A")
        ("L")
        ("VPULSE")
        ("TPS61086")
    )
    ("instances"
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"50k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C6"
            ("device_name"	"C")
            ("pspice_path"	"C_C6")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1n")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C11"
            ("device_name"	"C")
            ("pspice_path"	"C_C11")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"20p")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("D1"
            ("device_name"	"ES1A")
            ("pspice_path"	"D_D1")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("L1"
            ("device_name"	"L")
            ("pspice_path"	"L_L1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
            )
        )
        ("C7"
            ("device_name"	"C")
            ("pspice_path"	"C_C7")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C8"
            ("device_name"	"C")
            ("pspice_path"	"C_C8")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C9"
            ("device_name"	"C")
            ("pspice_path"	"C_C9")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("R4"
            ("device_name"	"R")
            ("pspice_path"	"R_R4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"147K")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"13.3K")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C4"
            ("device_name"	"C")
            ("pspice_path"	"C_C4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"33n")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("V1"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_V1")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PW"
                    ("value"	"1")
                    ("pspice_param"	"PW")
                )
                ("TF"
                    ("value"	"10u")
                    ("pspice_param"	"TF")
                )
                ("TD"
                    ("value"	"50u")
                    ("pspice_param"	"TD")
                )
                ("V2"
                    ("value"	"6")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("TR"
                    ("value"	"200u")
                    ("pspice_param"	"TR")
                )
                ("PER"
                    ("value"	"2")
                    ("pspice_param"	"PER")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("RL1"
            ("device_name"	"R")
            ("pspice_path"	"R_RL1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"25m")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("V2"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_V2")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PW"
                    ("value"	"1")
                    ("pspice_param"	"PW")
                )
                ("TF"
                    ("value"	"10u")
                    ("pspice_param"	"TF")
                )
                ("TD"
                    ("value"	"400u")
                    ("pspice_param"	"TD")
                )
                ("V2"
                    ("value"	"3.3")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"3.3")
                    ("pspice_param"	"V1")
                )
                ("TR"
                    ("value"	"10u")
                    ("pspice_param"	"TR")
                )
                ("PER"
                    ("value"	"2")
                    ("pspice_param"	"PER")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("C1"
            ("device_name"	"C")
            ("pspice_path"	"C_C1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C2"
            ("device_name"	"C")
            ("pspice_path"	"C_C2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C3"
            ("device_name"	"C")
            ("pspice_path"	"C_C3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("RLoad"
            ("device_name"	"R")
            ("pspice_path"	"R_RLoad")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"150")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("U1"
            ("device_name"	"TPS61086")
            ("pspice_path"	"X_U1")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"-104.1e-30W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C12"
            ("device_name"	"C")
            ("pspice_path"	"C_C12")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("D2"
            ("device_name"	"ES1A")
            ("pspice_path"	"D_D2")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("D3"
            ("device_name"	"ES1A")
            ("pspice_path"	"D_D3")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("D4"
            ("device_name"	"ES1A")
            ("pspice_path"	"D_D4")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("RLoad1"
            ("device_name"	"R")
            ("pspice_path"	"R_RLoad1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("RLoad2"
            ("device_name"	"R")
            ("pspice_path"	"R_RLoad2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("RLoad3"
            ("device_name"	"R")
            ("pspice_path"	"R_RLoad3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"150")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
    )
)
