("FILE_TYPE"	"PMAP File"
    ("devices"
        ("C")
        ("CESR_0")
        ("VPULSE")
        ("LDCR_0")
        ("R")
        ("TPS61372YKB_TRANS")
    )
    ("instances"
        ("C3"
            ("device_name"	"C")
            ("pspice_path"	"C_C3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("C2"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C2")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"150u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"0.05")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("V1"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_V1")
            ("level"	"0")
            ("model_params"
                ("PW"
                    ("value"	"3m")
                    ("pspice_param"	"PW")
                )
                ("TR"
                    ("value"	"10u")
                    ("pspice_param"	"TR")
                )
                ("V2"
                    ("value"	"3.6")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("TD"
                    ("value"	"200u")
                    ("pspice_param"	"TD")
                )
                ("TF"
                    ("value"	"10u")
                    ("pspice_param"	"TF")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"")
                    ("pspice_param"	"PER")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("L1"
            ("device_name"	"LDCR_0")
            ("pspice_path"	"X_L1")
            ("level"	"0")
            ("model_params"
                ("L"
                    ("value"	"2.2u")
                    ("pspice_param"	"L")
                )
                ("DCR"
                    ("value"	"0.066")
                    ("pspice_param"	"DCR")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C1"
            ("device_name"	"C")
            ("pspice_path"	"C_C1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.1u")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("C5"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C5")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"1.572u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C6"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C6")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"1.572u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C4"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C4")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"1.572u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("R4"
            ("device_name"	"R")
            ("pspice_path"	"R_R4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"49.9")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"909k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1MEG")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("R5"
            ("device_name"	"R")
            ("pspice_path"	"R_R5")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"61.9k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("C7"
            ("device_name"	"C")
            ("pspice_path"	"C_C7")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"680p")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("R6"
            ("device_name"	"R")
            ("pspice_path"	"R_R6")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("RLOAD"
            ("device_name"	"R")
            ("pspice_path"	"R_RLOAD")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{12/0.6}")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("U1"
            ("device_name"	"TPS61372YKB_TRANS")
            ("pspice_path"	"X_U1")
            ("level"	"0")
            ("model_params"
                ("SS"
                    ("value"	"0")
                    ("pspice_param"	"SS")
                )
                ("BiasValue Power"
                    ("value"	"-1.800pW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PackageName"
                    ("value"	"TPS61372YKBR")
                    ("pspice_param"	"PackageName")
                )
                ("IsHeterogeneous"
                    ("value"	"False")
                    ("pspice_param"	"IsHeterogeneous")
                )
                ("DevicesInView"
                    ("value"	"1")
                    ("pspice_param"	"DevicesInView")
                )
                ("DevicesInPackage"
                    ("value"	"1")
                    ("pspice_param"	"DevicesInPackage")
                )
                ("DeviceDesignator"
                    ("value"	"A")
                    ("pspice_param"	"DeviceDesignator")
                )
                ("DeviceNumbering"
                    ("value"	"Alpha")
                    ("pspice_param"	"DeviceNumbering")
                )
                ("Manufacturer"
                    ("value"	"Texas Instruments")
                    ("pspice_param"	"Manufacturer")
                )
                ("PartNumber"
                    ("value"	"TPS61372YKBR")
                    ("pspice_param"	"PartNumber")
                )
                ("< Value >"
                    ("value"	"TPS61372YKBR")
                    ("pspice_param"	"< Value >")
                )
                ("OriginalSymbolOrigin"
                    ("value"	"(-50000,90000)")
                    ("pspice_param"	"OriginalSymbolOrigin")
                )
            )
        )
        ("V2"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_V2")
            ("level"	"0")
            ("model_params"
                ("TF"
                    ("value"	"10u")
                    ("pspice_param"	"TF")
                )
                ("TD"
                    ("value"	"10u")
                    ("pspice_param"	"TD")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("V2"
                    ("value"	"5")
                    ("pspice_param"	"V2")
                )
                ("TR"
                    ("value"	"10u")
                    ("pspice_param"	"TR")
                )
                ("PW"
                    ("value"	"3m")
                    ("pspice_param"	"PW")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"")
                    ("pspice_param"	"PER")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
    )
)
