Thank you for your answer. I changed the resistance of s-conf pin on the original board from 42.2k to 18.2k, and retested the ripple. The measurement method is the same as before.

Here are some pictures of my measurements. They are all measured under no-load condition.















