
|  |  |  |
| --- | --- | --- |
| Module1 | Output1: 5V | 1.5A |
| Output2: Not used |  |
| Module2 | Output1: 2V5 | 1.5A |
| Output2: 3V3 | 3.5A |


5V\_top




Connect the BP5 cap on top level. BP5 capacitor is the supply voltage for the device.

The EN2 resistor connect on bottom or further away

5V\_bot



3v3+2v5 top



Connect the BP5 cap on top level. BP5 capacitor is the supply voltage for the device.

3v3+2v5 bot

