

Figure VIN at Normal operation



Figure Lx at Normal operation with Normal Load



Figure Vout put at Min load 3.3V



Figure Normal readings with 3.3V@ Normal load



Figure Vin at Peak load



Figure Lx showing when at Max load



Figure Voutput at max load



Figure Reading showing Voutput and Max Load current

