

Figure VIN at Normal operation




Figure Lx at Normal operation with Normal Load




Figure Vout put at Min load 3.3V



Figure Normal readings with 3.3V@ Normal load




Figure Vin at Peak load




Figure Lx showing when at Max load




Figure Voutput at max load




Figure Reading showing Voutput and Max Load current

