The power-on waveform of the new screen is as follows:



CH 1-- +11V\_AVDD\_LCD

CH1-- +20V\_VGH\_LCD



CH1-- +9.6V\_VCC\_LCD



CH1-- +3.3V\_VDD\_LCD



CH1-- - 6V\_VGL\_LCD

power-on waveform of Hanchuan Public Security Bureau is as follows:



CH1 -- +11V\_AVDD\_LCD 

CH1-- +20V\_VGH\_LCD



CH1-- +3.3V\_VDD\_LCD



CH1-- - 6V\_VGL\_LCD



 CH1-- +9.6V\_VCC\_LCD