


The power-on waveform of the new screen is as follows:




CH 1-- +11V\_AVDD\_LCD


CH1-- +20V\_VGH\_LCD



CH1-- +9.6V\_VCC\_LCD





CH1-- +3.3V\_VDD\_LCD




CH1-- - 6V\_VGL\_LCD

power-on waveform of Hanchuan Public Security Bureau is as follows:




CH1 -- +11V\_AVDD\_LCD 


CH1-- +20V\_VGH\_LCD



CH1-- +3.3V\_VDD\_LCD



CH1-- - 6V\_VGL\_LCD



CH1-- +9.6V\_VCC\_LCD