

Variable 15 ohm heater drive controlled by signal HCV.

When HCV goes slightly above internal 1V reference of U1 output goes to zero V.

Fan is not operating while heater is driven.

