

We have changed from PFM to COT that helps a lot concerning the sound but some was still left.

So my focus is now to change C3 and C9 from ceramic capacitor aluminum polymer.

On C9 I will use Würth:





But on C3 I haven’t found an Aluminum Polymer with 2,2uF