[Header]
bq EVSW Version = 0.9.90	
DeviceName = bq34z950 v0.02
Time = 23.09.2019 9:28:10	


[Voltage(1st Level Safety)]
COV Threshold = 4250
COV Recovery = 4000
CUV Threshold = 2500
CUV Recovery = 2800
[Current(1st Level Safety)]
OC (1st Tier) Chg = 1500
OC (1st Tier) Dsg = 1500
Current Recovery Time = 8
AFE OC Dsg = 12
AFE OC Dsg Time = 0F
AFE SC Chg Cfg = 77
AFE SC Dsg Cfg = 77
[Temperature(1st Level Safety)]
Over Temp Chg = 55.0
OT Chg Recovery = 50.0
Over Temp Dsg = 60.0
OT Dsg Recovery = 55.0

[Voltage(2nd Level Safety)]
SOV Threshold = 15000
SOV Time = 0
Cell Imbalance Current = 5
Cell Imbalance Fail Voltage = 1000
Cell Imbalance Time = 0
Battery Rest Time = 1800
[Current(2nd Level Safety)]
SOC Chg = 3000
SOC Chg Time = 0
SOC Dsg = 3000
SOC Dsg Time = 0
[Temperature(2nd Level Safety)]
SOT Chg = 65.0
SOT Chg Time = 0
SOT Dsg = 75.0
SOT Dsg Time = 0
[FET Verification(2nd Level Safety)]
FET Fail Time = 0
[AFE Verification(2nd Level Safety)]
AFE Fail Limit = 10

[Charge Inhibit Cfg(Charge Control)]
Chg Inhibit Temp Low = 0.0
Chg Inhibit Temp High = 45.0
[Pre-Charge Cfg(Charge Control)]
Pre-chg Current = 250
Pre-chg Temp = 12.0
Pre-chg Voltage = 3000
Recovery Voltage = 3100
[Fast Charge Cfg(Charge Control)]
Fast Charge Current = 1000
Charging Voltage = 12600
Suspend Low Temp = -5.0
Suspend High Temp = 55.0
[Termination Cfg.(Charge Control)]
Taper Current = 150
Taper Voltage = 300
TCA Clear % = 95
FC Set % = -1
FC Clear % = 98
[Cell Balancing Cfg(Charge Control)]
Min Cell Deviation = 1750
[Charging Faults(Charge Control)]
Over Charge Capacity = 300

[Data(SBS Configuration)]
Rem Cap Alarm = 300
Rem Energy Alarm = 4320
Rem Time Alarm = 10
Init Battery Mode = 0081
Design Voltage = 11800
Spec Info = 0031
Manuf Date = 22-рту-2019
Ser. Num. = 0001
Cycle Count = 0
CC Threshold = 4400
CF MaxError Limit = 100
Design Capacity = 3400
Design Energy = 12240
Manuf Name = Texas Inst.
Device Name = bq34z950
Device Chemistry = LION
[Configuration(SBS Configuration)]
TDA Set % = 6
TDA Clear % = 8
FD Set % = 2
FD Clear % = 5
TDA Set Volt Threshold = 5000
TDA Set Volt Time = 0
TDA Clear Volt = 5500

[Integrity Data(System Data)]
Reset Counter Partial = 0
Reset Counter Full = 28
[Manufacturer Info(System Data)]
Manuf. Info = 0123456789ABCDEF0123

[Registers(Configuration)]
Operation Cfg A = 0229
Operation Cfg B = 2448
Operation Cfg C = 0000
Permanent Fail Cfg = 0000
Non-Removable Cfg = 0000
[AFE(Configuration)]
AFE PMS Threshold = 5500

[LED Cfg(LED Support)]
LED Flash Period = 512
LED Blink Period = 1024
LED Delay = 100
LED Hold Time = 4
CHG Flash Alarm = 10
CHG Thresh 1 = 0
CHG Thresh 2 = 20
CHG Thresh 3 = 40
CHG Thresh 4 = 60
CHG Thresh 5 = 80
DSG Flash Alarm = 10
DSG Thresh 1 = 0
DSG Thresh 2 = 20
DSG Thresh 3 = 40
DSG Thresh 4 = 60
DSG Thresh 5 = 80
Sink Current = 3

[Power(Power)]
Flash Update OK Voltage = 7500
Shutdown Voltage = 7000
Charger Present = 3000
Wake Current Reg = 00

[IT Cfg(Gas Gauging)]
Load Select = 3
Load Mode = 1
Term Voltage = 7800
User Rate-mA = 0
User Rate-mW = 0
Reserve Cap-mAh = 0
Reserve Cap-mWh = 0
[Current Thresholds(Gas Gauging)]
Dsg Current Threshold = 100
Chg Current Threshold = 90
Quit Current = 25
[State(Gas Gauging)]
Qmax Cell 0 = 3645
Qmax Cell 1 = 3658
Qmax Cell 2 = 3664
Qmax Cell 3 = 3400
Qmax Pack = 3645
Update Status = 06
Delta Voltage = 16

[R_a0(Ra Table)]
Cell0 R_a flag = 0000
Cell0 R_a 0 = 549
Cell0 R_a 1 = 369
Cell0 R_a 2 = 207
Cell0 R_a 3 = 336
Cell0 R_a 4 = 235
Cell0 R_a 5 = 207
Cell0 R_a 6 = 688
Cell0 R_a 7 = 2057
Cell0 R_a 8 = 1966
Cell0 R_a 9 = 2805
Cell0 R_a 10 = 4807
Cell0 R_a 11 = 8008
Cell0 R_a 12 = 10614
Cell0 R_a 13 = 11458
Cell0 R_a 14 = 12438
[R_a1(Ra Table)]
Cell1 R_a flag = 0000
Cell1 R_a 0 = 525
Cell1 R_a 1 = 349
Cell1 R_a 2 = 188
Cell1 R_a 3 = 320
Cell1 R_a 4 = 230
Cell1 R_a 5 = 201
Cell1 R_a 6 = 601
Cell1 R_a 7 = 1709
Cell1 R_a 8 = 1619
Cell1 R_a 9 = 2243
Cell1 R_a 10 = 3886
Cell1 R_a 11 = 6798
Cell1 R_a 12 = 9341
Cell1 R_a 13 = 10111
Cell1 R_a 14 = 11843
[R_a2(Ra Table)]
Cell2 R_a flag = 0000
Cell2 R_a 0 = 573
Cell2 R_a 1 = 400
Cell2 R_a 2 = 243
Cell2 R_a 3 = 370
Cell2 R_a 4 = 271
Cell2 R_a 5 = 254
Cell2 R_a 6 = 612
Cell2 R_a 7 = 1862
Cell2 R_a 8 = 1796
Cell2 R_a 9 = 2539
Cell2 R_a 10 = 4285
Cell2 R_a 11 = 7333
Cell2 R_a 12 = 10035
Cell2 R_a 13 = 11023
Cell2 R_a 14 = 14709
[R_a3(Ra Table)]
Cell3 R_a flag = FF55
Cell3 R_a 0 = 432
Cell3 R_a 1 = 384
Cell3 R_a 2 = 375
Cell3 R_a 3 = 417
Cell3 R_a 4 = 426
Cell3 R_a 5 = 415
Cell3 R_a 6 = 520
Cell3 R_a 7 = 778
Cell3 R_a 8 = 1148
Cell3 R_a 9 = 1864
Cell3 R_a 10 = 3302
Cell3 R_a 11 = 5677
Cell3 R_a 12 = 6336
Cell3 R_a 13 = 7216
Cell3 R_a 14 = 11938
[R_a0x(Ra Table)]
xCell0 R_a flag = 0055
xCell0 R_a 0 = 555
xCell0 R_a 1 = 387
xCell0 R_a 2 = 219
xCell0 R_a 3 = 351
xCell0 R_a 4 = 232
xCell0 R_a 5 = 184
xCell0 R_a 6 = 684
xCell0 R_a 7 = 2742
xCell0 R_a 8 = 1832
xCell0 R_a 9 = 2669
xCell0 R_a 10 = 4573
xCell0 R_a 11 = 7884
xCell0 R_a 12 = 10802
xCell0 R_a 13 = 11661
xCell0 R_a 14 = 12658
[R_a1x(Ra Table)]
xCell1 R_a flag = 0055
xCell1 R_a 0 = 551
xCell1 R_a 1 = 366
xCell1 R_a 2 = 199
xCell1 R_a 3 = 332
xCell1 R_a 4 = 227
xCell1 R_a 5 = 175
xCell1 R_a 6 = 592
xCell1 R_a 7 = 2270
xCell1 R_a 8 = 1510
xCell1 R_a 9 = 2101
xCell1 R_a 10 = 3626
xCell1 R_a 11 = 6606
xCell1 R_a 12 = 9425
xCell1 R_a 13 = 10083
xCell1 R_a 14 = 11810
[R_a2x(Ra Table)]
xCell2 R_a flag = 0055
xCell2 R_a 0 = 596
xCell2 R_a 1 = 416
xCell2 R_a 2 = 255
xCell2 R_a 3 = 385
xCell2 R_a 4 = 265
xCell2 R_a 5 = 222
xCell2 R_a 6 = 595
xCell2 R_a 7 = 2419
xCell2 R_a 8 = 1697
xCell2 R_a 9 = 2309
xCell2 R_a 10 = 3899
xCell2 R_a 11 = 6975
xCell2 R_a 12 = 9951
xCell2 R_a 13 = 10867
xCell2 R_a 14 = 14501
[R_a3x(Ra Table)]
xCell3 R_a flag = FFFF
xCell3 R_a 0 = 432
xCell3 R_a 1 = 384
xCell3 R_a 2 = 375
xCell3 R_a 3 = 417
xCell3 R_a 4 = 426
xCell3 R_a 5 = 415
xCell3 R_a 6 = 520
xCell3 R_a 7 = 778
xCell3 R_a 8 = 1148
xCell3 R_a 9 = 1864
xCell3 R_a 10 = 3302
xCell3 R_a 11 = 5677
xCell3 R_a 12 = 6336
xCell3 R_a 13 = 7216
xCell3 R_a 14 = 11938

[Device Status Data(PF Status)]
PF Flags 1 = 0000
PF Flags 2 = 0000

[Data(Calibration)]
CC Gain = 0
CC Delta = 0
Ref Voltage = 1225.00
AFE Pack Gain = 672.91
CC Offset = -0.279
Board Offset = -42.4
Int Temp Offset = 0.0
Ext1 Temp Offset = 0.0
Ext2 Temp Offset = 0.0
[Config(Calibration)]
CC Current = 3000
Voltage Signal = 16800
Temp Signal = 298.0
CC Offset Time = 250
ADC Offset Time = 32
CC Gain Time = 250
Voltage Time = 1984
Temperature Time = 32
Cal Mode Timeout = 300
[Temp Model(Calibration)]
Ext Coef 1 = -28285
Ext Coef 2 = 20848
Ext Coef 3 = -7537
Ext Coef 4 = 401.2
Ext Min AD = 0
Ext Max Temp = 401.2
Int Coef 1 = 0
Int Coef 2 = 0
Int Coef 3 = -11136
Int Coef 4 = 575.4
Int Min AD = 0
Int Max Temp = 575.4
[Current(Calibration)]
Filter = 239
Deadband = 3
CC Deadband = 10.0

[bq2050 Config(DQ Communication)]
bq20z753 Configuration = 10
Pins Pulled Down = 20
Pins Pulled Up = 05
Resistor Divider Gain = 6
mV to mAhr Scale = 640
AutoCal per Sleep = 0
BR_Low = 2700
BR_RC = 1000
Wr0_Low = 1775
Wr0_RC = 1225
Wr1_Low = 550
Wr1_RC = 2451
Rd0_Low = 1150
Rd1_Low = 1100
Rd_TO = 0
RD_RS = 300
Wr_0_to_1_Delay = 100
SlaveRsp_Delay = 3020
