


Hi sir ,



Scope captures for LDRV and HDRV when MOSFETs are not connected


LDRV (MOSFETs are not connected)



LDRV (MOSFETs are connected)


 

HDRV (MOSFETs) not connected




HDRV (MOSFETs are connected)


Here is the scope capture for all pins




REGN




SRP




SRN




Term Enable




Vref




State 2




State 1



TS



MPPSet



VCC