###
C2 Compliance Test Report

# Power Delivery 3.1 Tests- Result Summary

Sl No | Test ID | Test Name | Test Result
--- | --- | --- | ---
1 | InitialBringUpCapture | InitialBringUpCapture | NA

# Power Delivery 3.1 Tests - Detailed Test Result

Test Status | Test Description
--- | ---
NA | 1. InitialBringUpCapture

# Packet List

Index | Start time(s.ms.μs.ns) | Stop time(s.ms.μs.ns) | Message Origin | Message |  | Secondary Message | SOP | Port Type | Msg ID | PDO | Header(MSB to LSB) | Payload(LSB to MSB)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Get_Cap_PDMer |
Port A Packet Details
1 | 1,710 S | 1,710 S | T-> | Ra_Asserted |  |  | NONE | NONE/NONE/R- | 0 | Ra_CC2 | 0x0000 |
6 | 1,915 S | 1,915 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Disabled -> FSM_State_Unattached_SRC | 0x0000 |
7 | 1,915 S | 1,915 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
8 | 1,917 S | 1,917 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
9 | 1,917 S | 1,917 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
10 | 2,127 S | 2,127 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
12 | 2,183 S | 2,184 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 0 | FS: 5V ,1A; | 0x11A1 | 0x0A-0x90-0x01-0x3B-
13 | 2,184 S | 2,184 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 0 |  | 0x0041 |
14 | 2,188 S | 2,189 S | <-D |  | Request |  | SOP | UFP/Sink/R3 | 0 | PDO#1 Fixed; OpCurrent = 0,1A; MaxCurrent = 3A | 0x1082 | 0x2C-0x29-0x80-0x15-
15 | 2,189 S | 2,189 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 0 |  | 0x0121 |
16 | 2,191 S | 2,191 S | T-> | Accept |  |  | SOP | DFP/Source/R3 | 1 |  | 0x03A3 |
17 | 2,192 S | 2,192 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 1 |  | 0x0241 |
19 | 2,292 S | 2,292 S | T-> | PS_RDY |  |  | SOP | DFP/Source/R3 | 2 |  | 0x05A6 |
20 | 2,293 S | 2,293 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 2 |  | 0x0441 |
22 | 2,293 S | 2,293 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
23 | 2,396 S | 2,396 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
25 | 2,396 S | 2,396 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
27 | 2,415 S | 2,416 S | T-> | VendorDefined |  |  | SOP | DFP/Source/R3/VdmR2/ | 3 | Discover ID;Initiator; | 0x17AF | 0x01-0xA0-0x00-0xFF-
28 | 2,416 S | 2,416 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 3 |  | 0x0641 |
29 | 2,417 S | 2,418 S | <-D |  | VendorDefined |  | SOP | UFP/Sink/R3/VdmR2/ | 1 | Discover ID;ACK; | 0x428F | 0x41-0xA8-0x00-0xFF-0xCF-0x19-0x40-0x18-0x18-0x2E-0x00-0x00-0x14-0x07-0x00-0x64-
30 | 2,419 S | 2,419 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 1 |  | 0x0321 |
32 | 2,419 S | 2,419 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
33 | 2,462 S | 2,462 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
35 | 2,462 S | 2,462 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
37 | 2,470 S | 2,471 S | T-> | VendorDefined |  |  | SOP | DFP/Source/R3/VdmR2/ | 4 | Discover SVID;Initiator; | 0x19AF | 0x02-0xA0-0x00-0xFF-
38 | 2,471 S | 2,471 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 4 |  | 0x0841 |
39 | 2,475 S | 2,476 S | <-D |  | VendorDefined |  | SOP | UFP/Sink/R3/VdmR2/ | 2 | Discover SVID;NAK; | 0x148F | 0x82-0xA8-0x00-0xFF-
40 | 2,476 S | 2,476 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 2 |  | 0x0521 |
42 | 2,476 S | 2,476 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
44 | 2,579 S | 2,579 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
45 | 2,579 S | 2,579 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
47 | 2,587 S | 2,587 S | T-> | Get_Sink_Cap |  |  | SOP | DFP/Source/R3 | 5 |  | 0x0BA8 |
48 | 2,588 S | 2,588 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 5 |  | 0x0A41 |
49 | 2,592 S | 2,593 S | <-D |  | SinkCap |  | SOP | UFP/Sink/R3 | 3 | FS: 5V ,9A; VS: (9~20)V 3A; | 0x2684 | 0x5A-0x90-0x01-0x10-0x2C-0xD1-0x02-0x99-
50 | 2,593 S | 2,593 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 3 |  | 0x0721 |
52 | 2,593 S | 2,593 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
53 | 2,696 S | 2,696 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
55 | 2,696 S | 2,696 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
57 | 2,704 S | 2,704 S | T-> | Get_Sink_Cap_Ext |  |  | SOP | DFP/Source/R3 | 6 |  | 0x0DB6 |
58 | 2,705 S | 2,705 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 6 |  | 0x0C41 |
59 | 2,709 S | 2,710 S | <-D |  | Sink_Cap_Extended |  | SOP | UFP/Sink/R3 | 4 | UnChunked | 0x888F | 0x18-0x00-0xCF-0x19-0x00-0x64-0x18-0x2E-0x00-0x00-0xFF-0x06-0x01-0x00-0x00-0x00-0x00-0x00-0x02-0x1A-0x00-0x00-0x00-0x00-0x00-0x00-
60 | 2,711 S | 2,711 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 4 |  | 0x0921 |
62 | 2,711 S | 2,711 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
64 | 12.34 S | 12.34 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Disabled | 0x0000 |
65 | 12.34 S | 12.34 S | T-> | Detach |  |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |

# AMS Summary

AMS Index | AMS Name | AMS Start | AMS Stop | AMS Status | Child AMS Count
--- | --- | --- | --- | --- | ---

# DUT Information

Manufacturer | Parrot
Model Number | MPPUA2
Serial Number | 1

# Test Information

Test Lab |
Test_Engineer | Test_Engineer
Remarks | Remarks
Date_and_Time | 14/10/2025 17:32:52

# Controller and Instrument Information

Parameter | Value
--- | ---
GRL_USB_PD_Controller_Serial_No | 397.409.397.077.376.
GRL_USB_PD_Software_Version | 1.6.28.0
GRL_USB_PD_Firmware_Version | 2.2.65
GRL USB-PD Ethernet Buffer Size | 62K
GRL USB-PD Eload Firmware Version | 9.8 / 9.8
Calibration | Calibration Success
RX mask Power selection | Neutral Power
Device_Type | Consumer Only
Cable Type | GRL_SPL_CABLE_1
Impedance (milli ohm) | 0
PD_Merged CTS Version | v.Q4-2024
USB_PD_Spec Version | Rev3.2 Ver1.1RC2
USB_Type_C_Spec Version | v2.3 Oct-2023
VIF_File_Name | Parrot__MPPUA2__1__0_14_10_2025.xml
Noise Pattern Generation: | Two-Tone Noise
Application mode | Informational
Disabled all Pop-up during test execution | False
Pop-up Timer | 0
Rerun Enabled | False
Rerun Count | 1
Rerun Iteration | 0
UI Live Update | False
Execution Time(In Minutes) | 0

# Power Delivery 3.1 Tests Information

Parameter | Value
--- | ---
Connect EPR Test Fixture | False
FR_Swap AUTO Box Connected | False