##########C:\GRL\USBPD-C2-Browser-App\Report\TempReport\C2\MPPUA2_2025_10_14-16_06_47\New_Run18_Rep0_2025_10_14-05_20_05\GRL_USB_PD_Report_Run_18_2025_10_14.html
Test res file is available
Test res file is not null
Not DP AUX
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:32:25.940 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0xD5, 
Application Type C2 decoded value is 1
StartTime Exec :2025_10_14-05_32_25
SW_BuildPurpose :DebugMode
10 /14/2025 05:32:25.973  Write Ethernet :FW Write:0x16, 0x22, 0x04, 0x01,  , API description - PD interrupts
10 /14/2025 05:32:25.987  Write Ethernet :FW Write:0x16, 0x10, 0x01, 0x00, 0x00, 
Port A VBUS Resistance: 114
Port A CC2 Resistance: 930
Port A CC1 Resistance: 930
Port B VBUS Resistance: 114
Port B CC2 Resistance: 930
Port B CC1 Resistance: 930
IRDropVBUSValue0
IRDropCC1Value0
IRDropCC1Value0
10 /14/2025 05:32:26.002  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
##########C:\GRL\USBPD-C2-Browser-App\Report\TempReport\C2\MPPUA2_2025_10_14-16_06_47\New_Run18_Rep0_2025_10_14-05_20_05\GRL_USB_PD_Report_Run_18_2025_10_14.html
10 /14/2025 05:32:27.230  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:32:27.403  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:32:27.573  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:32:27.588  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:32:27.602  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:32:27.617  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:32:27.632  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:32:27.646  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:32:27.661  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:32:27.675  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:32:27.690  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:32:27.705  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:32:27.719  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:32:27.734  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:32:27.748  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:32:27.763  Write Ethernet :FW Write:0x6F, 0x02,  , API description - Setting Controller Configuaton :RA_CC2
10 /14/2025 05:32:27.937  Write Ethernet :FW Write:0x16, 0x00, 0x80, 0x01,  , API description - Set revision number
10 /14/2025 05:32:27.951  Write Ethernet :FW Write:0x16, 0x02, 0x20, 0x01,  , API description - Set VDM revision number
10 /14/2025 05:32:27.965  Write Ethernet :FW Write:0x3E, 0x00,  , API description - Initiate DR_Swap
10 /14/2025 05:32:28.030  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:32:28.045  Write Ethernet :FW Write:0x3F, 0x00, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:32:28.060  Write Ethernet :FW Write:0x16, 0x0C, 0x05, 0x00, 0x0B, 0x00, 0x00, 0x80, 0x00, 0x00, 
10 /14/2025 05:32:28.075  Write Ethernet :FW Write:0x54,  , API description - Setting Controller Configuaton :VDM_DiscovIdAck_All_SOP
10 /14/2025 05:32:28.229  Write Ethernet :FW Write:0x16, 0x01, 0x00, 0x01,  , API description - Enable unchunked message support
10 /14/2025 05:32:28.243  Write Ethernet :FW Write:0x5E, 0xC1, 0x3D, 0x00, 0x0A, 
10 /14/2025 05:32:28.258  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:32:28.272  Write Ethernet :FW Write:0x18, 0x00,  , API description - Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:32:28.433  Write Ethernet :FW Write:0x18, 0x09,  , API description - Setting Controller Configuaton :SimulateDetach_CC1_CC2
10 /14/2025 05:32:28.604  Write Ethernet :FW Write:0x0E,  , API description - Setting Controller Configuaton :PHY_RESET
ResetDataManager - End of Reset all RTDataChunk

---------------------------------------------------------------------------------------------------------
17:32:28 Test Name(Start): InitialBringUpCapture
Tester cable drop compensation : False
10 /14/2025 05:32:28.799  Write Ethernet :FW Write:0x16, 0x21, 0x07, 0x00, 0x00, 0x00, 0x00, 0x01, 
DataStreamerSertvice -->>StartStreamer()-->> SubSampleRatio -->>500
Reset board API start
10 /14/2025 05:32:28.814  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:32:28.839  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:32:28.853  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x10,  , API description - Enable LSADC
10 /14/2025 05:32:28.867  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:28.882  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:28.896  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:32:28.911  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x00,  , API description - Reset DMA :DMA0_CCLinePortA
10 /14/2025 05:32:28.926  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x01,  , API description - Reset DMA :DMA1_CCLinePortB
10 /14/2025 05:32:28.941  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x02,  , API description - Reset DMA :DMA2_LSADC_Port_A_B
10 /14/2025 05:32:28.955  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:32:29.073  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:32:29.088  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:29.103  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:29.118  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:32:29.132  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:32:29.146  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:32:29.160  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:32:29.206  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x40, 0x02, 0x00, 0x00, 0x00, 0x00,  , API description - Configure LSADC Sub Sampling
###LSADC channel debug
Without adding dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

With dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

10 /14/2025 05:32:29.221  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x04, 0x02, 0x00, 0x00, 0x15, 0x33, 0x00, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:32:29.236  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x08, 0x02, 0x00, 0x00, 0x88, 0xC6, 0x02, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:32:29.250  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x0C, 0x02, 0x00, 0x00, 0x88, 0x00, 0x00, 0x0A,  , API description - Configure Port A Channels
10 /14/2025 05:32:29.264  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x20, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.279  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x24, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.294  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x28, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.308  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x2C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.323  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x30, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.337  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x34, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.352  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x38, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.366  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x3C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0x00, 0x00,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:29.381  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x1C, 0x02, 0x00, 0x00, 0x3F, 0x00,  , API description - Configure LSADC Sub Sampling
10 /14/2025 05:32:29.396  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x10, 0x02, 0x00, 0x00, 0xFB, 0x00, 0x00, 0xF0,  , API description - Time stamp configuration
10 /14/2025 05:32:29.410  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x09,  , API description - Enable LSADC
10 /14/2025 05:32:29.424  Write Ethernet :FW Write:0x6B, 0x01, 0x23, 0x04, 0x06, 0x02, 0xFF, 0xFF,  , API description - Switch LSADC Ch8 Path
10 /14/2025 05:32:29.453 Read Ethernet :FW Read:0xFE, 0x00, 0x05, 0xE4, 0x02, 0x00, 0x00, 
C2Lib: StartStreamer(): 17_17_32_29_455
10 /14/2025 05:32:29.455  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:32:29.481  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
17_17_32_29_496: WorkerThreadLSADC start
17_17_32_29_496: WorkerThread_CCline start
10 /14/2025 05:32:29.496  Write Ethernet :FW Write:0x16, 0x24, 0x0B, 0x01, 0x00, 0x00, 0x00,  , API description - Enable/Disable Configure
10 /14/2025 05:32:30.174 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.205 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.237 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.268 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.299 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.331 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.362 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.395 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.426 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.457 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.503 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.536 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.568 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.598 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.631 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.661 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.707 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.739 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.770 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:32:30.803 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
Configured message: 0->Setting Controller Configuaton :RA_CC2
Configured message: 1->Setting Controller Configuaton :SimulateAttach
Configured message: 2->Setting Controller Configuaton :Source
Configured message: 3->Setting Controller Configuaton :Source
Configured message: 4->VDM
Configured message: 5->VDM
Configured message: 6->
Configured message: 7->
10 /14/2025 05:32:30.836  Write Ethernet :FW Write:0x6E, 0x66, 0x00, 0x00, 0x08, 0x00, 0x00, 0x09, 0x00, 0x04, 0x00, 0x05, 0x00, 0x05, 0x00, 0x00, 0x6F, 0x02, 0x09, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x18, 0x00, 0x09, 0x00, 0x04, 0x00, 0x05, 0x00, 0x05, 0x00, 0x00, 0x14, 0x03, 0x09, 0x00, 0x06, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x18, 0x01, 0x0D, 0x00, 0x03, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x4F, 0x10, 0x01, 0x80, 0x00, 0xFF, 0x0D, 0x00, 0x03, 0x00, 0x64, 0x00, 0x28, 0x00, 0x00, 0x4F, 0x10, 0x02, 0x80, 0x00, 0xFF, 0x0C, 0x00, 0x07, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x2C, 0x03, 0x00, 0x48, 0x00, 0x0C, 0x00, 0x07, 0x00, 0x64,  ..... , API description - Group Configuration Command
10 /14/2025 05:32:30.850  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:32:31.009 
10 /14/2025 05:32:32.024 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:32:32.024 
10 /14/2025 05:32:35.026  Write Ethernet :FW Write:0x6E, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Group Configuration Command
10 /14/2025 05:32:35.041  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
CCLine Read Started :14/10/2025 17:32:35
Configured message: 0->Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:32:41.368  Write Ethernet :FW Write:0x6E, 0x0B, 0x00, 0x00, 0x01, 0x00, 0x00, 0x09, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x18, 0x00,  , API description - Group Configuration Command
10 /14/2025 05:32:41.382  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:32:41.541 
10 /14/2025 05:32:42.556 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:32:42.556 
StreamStSpData_LA
TimeStamp 26391583, TicksPerSample 123246, ValidSample 502
TimeStamp 36621176, TicksPerSample 123246, ValidSample 502
TimeStamp 46973469, TicksPerSample 123246, ValidSample 502
TimeStamp 1593710769, TicksPerSample 123246, ValidSample 502

10 /14/2025 05:32:45.558  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:32:50.579 :InteruptLasdcRead triggered
17_17_32_50_739: WorkerThread_CCline end
17_17_32_51_738: WorkerThreadLSADC end
InteruptLasdcRead:  m_LSADCthread: thread Aborted()
InteruptLasdcRead:  m_CClinethread: thread Aborted()
10 /14/2025 05:32:51.807  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
StopStreamer:  m_LSADCthread: thread Aborted()
StopStreamer:  m_CClinethread: thread Aborted()
StreamStSpData_LA
TimeStamp 26391583, TicksPerSample 123246, ValidSample 502
TimeStamp 36621176, TicksPerSample 123246, ValidSample 502
TimeStamp 46973469, TicksPerSample 123246, ValidSample 502
TimeStamp 2222635641, TicksPerSample 123246, ValidSample 502

StopTime Exec :14/10/2025 17:32:52
CreateHtmlDoc -->> New change
SPR_Adjustable_Voltage_Supply is not supported by UUT
10 /14/2025 05:32:52.157  Write Ethernet :FW Write:0x16, 0x36, 0x00, 0x02, 0x01, 0x00, 0x00, 0x01, 0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x02, 0x04, 0x00,  , API description - PDMVIFData
10 /14/2025 05:32:52.172  Write Ethernet :FW Write:0x16, 0x36, 0x01,  , API description - VIFSrcPDOInfo
10 /14/2025 05:32:52.186  Write Ethernet :FW Write:0x16, 0x36, 0x02, 0x00, 0x64, 0x00, 0x5A, 0x00, 0x00, 0x00, 0x02, 0xB4, 0x00, 0x90, 0x01, 0x2C, 0x01,  , API description - VIFSnkPDOInfo
10 /14/2025 05:32:52.201  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:32:52.381  Write Ethernet :FW Write:0x6F, 0x02,  , API description - Setting Controller Configuaton :RA_CC2
10 /14/2025 05:32:52.542  Write Ethernet :FW Write:0x16, 0x00, 0x80, 0x01,  , API description - Set revision number
10 /14/2025 05:32:52.557  Write Ethernet :FW Write:0x16, 0x02, 0x20, 0x01,  , API description - Set VDM revision number
10 /14/2025 05:32:52.571  Write Ethernet :FW Write:0x3E, 0x00,  , API description - Initiate DR_Swap
10 /14/2025 05:32:52.651  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:32:52.665  Write Ethernet :FW Write:0x3F, 0x00, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:32:52.680  Write Ethernet :FW Write:0x16, 0x0C, 0x05, 0x00, 0x0B, 0x00, 0x00, 0x80, 0x00, 0x00, 
10 /14/2025 05:32:52.695  Write Ethernet :FW Write:0x54,  , API description - Setting Controller Configuaton :VDM_DiscovIdAck_All_SOP
10 /14/2025 05:32:52.855  Write Ethernet :FW Write:0x16, 0x01, 0x00, 0x01,  , API description - Enable unchunked message support
10 /14/2025 05:32:52.870  Write Ethernet :FW Write:0x5E, 0xC1, 0x3D, 0x00, 0x0A, 
10 /14/2025 05:32:52.884  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:32:52.899  Write Ethernet :FW Write:0x3E, 0x02,  , API description - Initiate DR_Swap
10 /14/2025 05:32:52.979  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:32:52.994  Write Ethernet :FW Write:0x3F, 0x02, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:32:53.009  Write Ethernet :FW Write:0x18, 0x00,  , API description - Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:32:53.179  Write Ethernet :FW Write:0x18, 0x09,  , API description - Setting Controller Configuaton :SimulateDetach_CC1_CC2
10 /14/2025 05:32:53.336  Write Ethernet :FW Write:0x0E,  , API description - Setting Controller Configuaton :PHY_RESET
ResetDataManager - End of Reset all RTDataChunk

---------------------------------------------------------------------------------------------------------
17:32:53 Test Name(Start): TEST.PD.PROT.SNK.3 SinkWaitCapTimer Deadline
Tester cable drop compensation : False
10 /14/2025 05:32:53.526  Write Ethernet :FW Write:0x16, 0x21, 0x07, 0x00, 0x00, 0x00, 0x00, 0x01, 
DataStreamerSertvice -->>StartStreamer()-->> SubSampleRatio -->>500
Reset board API start
10 /14/2025 05:32:53.540  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:32:53.572  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:32:53.586  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x10,  , API description - Enable LSADC
10 /14/2025 05:32:53.601  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:53.615  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:53.629  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:32:53.644  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x00,  , API description - Reset DMA :DMA0_CCLinePortA
10 /14/2025 05:32:53.658  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x01,  , API description - Reset DMA :DMA1_CCLinePortB
10 /14/2025 05:32:53.673  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x02,  , API description - Reset DMA :DMA2_LSADC_Port_A_B
10 /14/2025 05:32:53.687  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:32:53.809  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:32:53.824  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:53.839  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:32:53.853  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:32:53.867  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:32:53.882  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:32:53.897  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:32:53.950  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x40, 0x02, 0x00, 0x00, 0x00, 0x00,  , API description - Configure LSADC Sub Sampling
###LSADC channel debug
Without adding dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

With dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

10 /14/2025 05:32:53.965  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x04, 0x02, 0x00, 0x00, 0x15, 0x33, 0x00, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:32:53.980  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x08, 0x02, 0x00, 0x00, 0x88, 0xC6, 0x02, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:32:53.995  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x0C, 0x02, 0x00, 0x00, 0x88, 0x00, 0x00, 0x0A,  , API description - Configure Port A Channels
10 /14/2025 05:32:54.009  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x20, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.023  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x24, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.038  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x28, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.053  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x2C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.067  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x30, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.082  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x34, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.097  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x38, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.112  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x3C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0x00, 0x00,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:32:54.127  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x10, 0x02, 0x00, 0x00, 0xFB, 0x00, 0x00, 0xF0,  , API description - Time stamp configuration
10 /14/2025 05:32:54.141  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x09,  , API description - Enable LSADC
10 /14/2025 05:32:54.156  Write Ethernet :FW Write:0x6B, 0x01, 0x23, 0x04, 0x06, 0x02, 0xFF, 0xFF,  , API description - Switch LSADC Ch8 Path
10 /14/2025 05:32:54.184 Read Ethernet :FW Read:0xFE, 0x00, 0x05, 0xE4, 0x02, 0x00, 0x00, 
C2Lib: StartStreamer(): 17_17_32_54_188
10 /14/2025 05:32:54.188  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:32:54.219  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
17_17_32_54_234: WorkerThreadLSADC start
17_17_32_54_234: WorkerThread_CCline start
Present Test case TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline EPR Flag Status False and enableForNonTestCases False
Consolidate message group
0 -> 0x16, 0x24, 0x15, 0x01, 0x00,  PDM Mode setting RxTimer:50 and TxTimer:50
1 -> 0x16, 0x35, 0x00, 0x4F, 0x00, 0x00, 0x01,  Start PDM test case 79 RxTimer:100 and TxTimer:100
10 /14/2025 05:32:54.235  Write Ethernet :FW Write:0x16, 0x24, 0x0B, 0x01, 0x00, 0x00, 0x00,  , API description - Enable/Disable Configure
Configured message: 0->PDM Mode setting
Configured message: 1->Start PDM test case 79
10 /14/2025 05:32:54.250  Write Ethernet :FW Write:0x6E, 0x1E, 0x00, 0x00, 0x02, 0x00, 0x00, 0x0C, 0x00, 0x04, 0x00, 0x32, 0x00, 0x32, 0x00, 0x00, 0x16, 0x24, 0x15, 0x01, 0x00, 0x0E, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x16, 0x35, 0x00, 0x4F, 0x00, 0x00, 0x01,  , API description - Group Configuration Command
10 /14/2025 05:32:54.265  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:32:54.438 
10 /14/2025 05:32:55.453 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:32:55.458 
Start : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:32:56 
Read_All_Packets_Dynamic_Delay StAssertion Found :970292354-->> 14/10/2025 17:33:04 
 LastADCTimeStamp before ADCRead 1022599238
 LastADCTimeStamp before ADCRead 1022599238
Stop : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:33:04 
DUT Behaviour -- Index: 14, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 35, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
DUT Behaviour -- Index: 57, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 84, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS merge Bef
AMS merge Aft
DUT role after Swap or PDC
14 Pow:Sink Dat:UFP Vconn Src:False
35 Pow:Sink Dat:UFP Vconn Src:False
57 Pow:Sink Dat:UFP Vconn Src:False
84 Pow:Sink Dat:UFP Vconn Src:False

TEST_PD_PROT_SNK_3_SinkWaitCapTimer_DeadlineExpected TestCondition:Rev2Snk and Configured TestCondition:Rev2Snk
TEST_PD_PROT_SNK_3_SinkWaitCapTimer_DeadlineExpected TestCondition:Rev3ChkdSnk and Configured TestCondition:Rev3ChkdSnk
Test conditions
StInd:6 StAMS:0 AftStInd:23 AftAMS:1 SpInd:47 SpAMS:1
StInd:48 StAMS:2 AftStInd:70 AftAMS:3 SpInd:100 SpAMS:3
#PD merged debug desc: Start of common field check validation : 17:33:04.4721350
StartTime :0,83064523, StopTime :0,83058023ObtainedTime :0,0649999999999817
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :0,83941947, StopTime :0,83935467ObtainedTime :0,064800000000087
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :1,16064688, StopTime :1,16058208ObtainedTime :0,064800000000087
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :4,21294097, StopTime :4,21287617ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :4,21928341, StopTime :4,21921861ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :4,54049483, StopTime :4,54043002ObtainedTime :0,0648099999995821
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :5,86257549, StopTime :5,86251749ObtainedTime :0,0580000000001135
Obtained time difference is 0,058ms, Expected time limit 0,025ms to 0,195ms
StartTime :5,87045114, StopTime :5,87038634ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :6,19245296, StopTime :6,19238816ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :9,24857683, StopTime :9,24852543ObtainedTime :0,0514000000002568
Obtained time difference is 0,051ms, Expected time limit 0,025ms to 0,195ms
StartTime :9,25645608, StopTime :9,25639108ObtainedTime :0,0649999999993156
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :9,57945931, StopTime :9,57939451ObtainedTime :0,0648000000005311
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
Time Difference of GoodCRC of SourceCap and Request is 4,09502000000006ms at AMS Index : 0
Time Difference of GoodCRC of SourceCap and Request is 4,08782999999957ms at AMS Index : 1
Time Difference of GoodCRC of SourceCap and Request is 4,09124000000016ms at AMS Index : 2
Time Difference of GoodCRC of SourceCap and Request is 4,08779999999886ms at AMS Index : 3
Skipped: Power_Negotiation Index: 2
Validated: 0 packets
No Discover ID in TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline test case
Validated: 0 VCONN_Swap packets
Validated: 0 packets
#PD merged debug desc: Stop of common field check validation : 17:33:04.4741340
###Test condition validation: Assert count is not integrated
#PD Merged: Critical error - BU test result count is 1, Test case validation count 2
Read_All_Packets_Dynamic_Delay StAssertion Found :970292354-->> 14/10/2025 17:33:04 
 LastADCTimeStamp before ADCRead 1022599238
 LastADCTimeStamp before ADCRead 1022599238
StreamStSpData_CC First Message StTime0,4329107 , SpTime0,4329107
StreamStSpData_CC Last Message StTime9,70292354 , SpTime9,70292354
StreamStSpData_LA
TimeStamp 25903739, TicksPerSample 123246, ValidSample 502
TimeStamp 36133332, TicksPerSample 123246, ValidSample 502
TimeStamp 46485871, TicksPerSample 123246, ValidSample 340
TimeStamp 1022599238, TicksPerSample 123246, ValidSample 502

10 /14/2025 05:33:04.474  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:33:09.498 :InteruptLasdcRead triggered
17_17_33_9_630: WorkerThread_CCline end
17_17_33_9_660: WorkerThreadLSADC end
InteruptLasdcRead:  m_LSADCthread: thread Aborted()
InteruptLasdcRead:  m_CClinethread: thread Aborted()
10 /14/2025 05:33:09.714  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
StopStreamer:  m_LSADCthread: thread Aborted()
StopStreamer:  m_CClinethread: thread Aborted()
StreamStSpData_LA
TimeStamp 25903739, TicksPerSample 123246, ValidSample 502
TimeStamp 36133332, TicksPerSample 123246, ValidSample 502
TimeStamp 46485871, TicksPerSample 123246, ValidSample 340
TimeStamp 1249494999, TicksPerSample 123246, ValidSample 502

StopTime Exec :14/10/2025 17:33:10
CreateHtmlDoc -->> New change
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - Updated
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - Updated
COMMON.PROC.BU.2 - Updated
Rev2Snk - Updated
Rev3ChkdSnk - Updated
TEST.PD.PROT.SNK.3 SinkWaitCapTimer Deadline - Updated
Packet and signal mapping list PD_Merged -> TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline
TEST.PD.PROT.SNK.3 SinkWaitCapTimer Deadline - 0
COMMON.PROC.BU.2 - -1
Packet Index is missing
Signal start or stop time is missing
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - 14
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 16
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - 57
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 59
Rev2Snk - -1
Packet Index is missing
Signal start or stop time is missing
Hard_Reset check - TEST.PD.PROT.SNK.3#1 - 35
Rev3ChkdSnk - -1
Packet Index is missing
Signal start or stop time is missing
Hard_Reset check - TEST.PD.PROT.SNK.3#1 - 84
CCline Thread State : (STOP)
LSADC Thread State : (STOP)
HSADC Thread State : (NONE)
QD Thread State : (NONE)

17:33:10     | Test Name(Stop): TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline
---------------------------------------------------------------------------------------------------------
10 /14/2025 05:33:10.065  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:33:10.227  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:33:10.398  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:33:10.412  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:33:10.426  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:33:10.440  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:33:10.455  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:33:10.469  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:33:10.484  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:33:10.499  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:33:10.514  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:33:10.529  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:33:10.544  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:33:10.558  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:33:10.573  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:33:10.589  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:33:10.759  Write Ethernet :FW Write:0x6F, 0x02,  , API description - Setting Controller Configuaton :RA_CC2
10 /14/2025 05:33:10.917  Write Ethernet :FW Write:0x16, 0x00, 0x80, 0x01,  , API description - Set revision number
10 /14/2025 05:33:10.931  Write Ethernet :FW Write:0x16, 0x02, 0x20, 0x01,  , API description - Set VDM revision number
10 /14/2025 05:33:10.946  Write Ethernet :FW Write:0x3E, 0x00,  , API description - Initiate DR_Swap
10 /14/2025 05:33:11.011  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:33:11.026  Write Ethernet :FW Write:0x3F, 0x00, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:33:11.040  Write Ethernet :FW Write:0x16, 0x0C, 0x05, 0x00, 0x0B, 0x00, 0x00, 0x80, 0x00, 0x00, 
10 /14/2025 05:33:11.055  Write Ethernet :FW Write:0x54,  , API description - Setting Controller Configuaton :VDM_DiscovIdAck_All_SOP
10 /14/2025 05:33:11.214  Write Ethernet :FW Write:0x16, 0x01, 0x00, 0x01,  , API description - Enable unchunked message support
10 /14/2025 05:33:11.228  Write Ethernet :FW Write:0x5E, 0xC1, 0x3D, 0x00, 0x0A, 
10 /14/2025 05:33:11.242  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:33:11.257  Write Ethernet :FW Write:0x3E, 0x02,  , API description - Initiate DR_Swap
10 /14/2025 05:33:11.322  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:33:11.336  Write Ethernet :FW Write:0x3F, 0x02, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:33:11.351  Write Ethernet :FW Write:0x18, 0x00,  , API description - Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:33:11.510  Write Ethernet :FW Write:0x18, 0x09,  , API description - Setting Controller Configuaton :SimulateDetach_CC1_CC2
10 /14/2025 05:33:11.680  Write Ethernet :FW Write:0x0E,  , API description - Setting Controller Configuaton :PHY_RESET
ResetDataManager - End of Reset all RTDataChunk

---------------------------------------------------------------------------------------------------------
17:33:11 Test Name(Start): TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout
Tester cable drop compensation : False
10 /14/2025 05:33:11.857  Write Ethernet :FW Write:0x16, 0x21, 0x07, 0x00, 0x00, 0x00, 0x00, 0x01, 
DataStreamerSertvice -->>StartStreamer()-->> SubSampleRatio -->>500
Reset board API start
10 /14/2025 05:33:11.872  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:33:11.898  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:33:11.913  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x10,  , API description - Enable LSADC
10 /14/2025 05:33:11.927  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:33:11.942  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:33:11.957  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:33:11.972  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x00,  , API description - Reset DMA :DMA0_CCLinePortA
10 /14/2025 05:33:11.987  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x01,  , API description - Reset DMA :DMA1_CCLinePortB
10 /14/2025 05:33:12.001  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x02,  , API description - Reset DMA :DMA2_LSADC_Port_A_B
10 /14/2025 05:33:12.015  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:33:12.133  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:33:12.147  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:33:12.162  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:33:12.177  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:33:12.191  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:33:12.206  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:33:12.220  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:33:12.269  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x40, 0x02, 0x00, 0x00, 0x00, 0x00,  , API description - Configure LSADC Sub Sampling
###LSADC channel debug
Without adding dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

With dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

10 /14/2025 05:33:12.284  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x04, 0x02, 0x00, 0x00, 0x15, 0x33, 0x00, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:33:12.298  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x08, 0x02, 0x00, 0x00, 0x88, 0xC6, 0x02, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:33:12.313  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x0C, 0x02, 0x00, 0x00, 0x88, 0x00, 0x00, 0x0A,  , API description - Configure Port A Channels
10 /14/2025 05:33:12.328  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x20, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.343  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x24, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.357  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x28, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.371  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x2C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.386  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x30, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.401  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x34, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.416  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x38, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.430  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x3C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0x00, 0x00,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:33:12.445  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x10, 0x02, 0x00, 0x00, 0xFB, 0x00, 0x00, 0xF0,  , API description - Time stamp configuration
10 /14/2025 05:33:12.459  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x09,  , API description - Enable LSADC
10 /14/2025 05:33:12.474  Write Ethernet :FW Write:0x6B, 0x01, 0x23, 0x04, 0x06, 0x02, 0xFF, 0xFF,  , API description - Switch LSADC Ch8 Path
10 /14/2025 05:33:12.504 Read Ethernet :FW Read:0xFE, 0x00, 0x05, 0xE4, 0x02, 0x00, 0x00, 
C2Lib: StartStreamer(): 17_17_33_12_507
10 /14/2025 05:33:12.507  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:33:12.543  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
17_17_33_12_558: WorkerThreadLSADC start
17_17_33_12_559: WorkerThread_CCline start
Present Test case TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout EPR Flag Status False and enableForNonTestCases False
Consolidate message group
0 -> 0x16, 0x24, 0x15, 0x01, 0x00,  PDM Mode setting RxTimer:50 and TxTimer:50
1 -> 0x16, 0x35, 0x00, 0x50, 0x00, 0x00, 0x01,  Start PDM test case 80 RxTimer:100 and TxTimer:100
10 /14/2025 05:33:12.559  Write Ethernet :FW Write:0x16, 0x24, 0x0B, 0x01, 0x00, 0x00, 0x00,  , API description - Enable/Disable Configure
Configured message: 0->PDM Mode setting
Configured message: 1->Start PDM test case 80
10 /14/2025 05:33:12.574  Write Ethernet :FW Write:0x6E, 0x1E, 0x00, 0x00, 0x02, 0x00, 0x00, 0x0C, 0x00, 0x04, 0x00, 0x32, 0x00, 0x32, 0x00, 0x00, 0x16, 0x24, 0x15, 0x01, 0x00, 0x0E, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x16, 0x35, 0x00, 0x50, 0x00, 0x00, 0x01,  , API description - Group Configuration Command
10 /14/2025 05:33:12.589  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:33:12.763 
10 /14/2025 05:33:13.778 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:33:13.778 
Start : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:33:14 
Read_All_Packets_Dynamic_Delay StAssertion Found :1283308517-->> 14/10/2025 17:33:25 
 LastADCTimeStamp before ADCRead 1321609663
 LastADCTimeStamp before ADCRead 1321609663
Stop : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:33:25 
DUT Behaviour -- Index: 14, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 43, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
DUT Behaviour -- Index: 65, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 103, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS merge Bef
AMS merge Aft
DUT role after Swap or PDC
14 Pow:Sink Dat:UFP Vconn Src:False
43 Pow:Sink Dat:UFP Vconn Src:False
65 Pow:Sink Dat:UFP Vconn Src:False
103 Pow:Sink Dat:UFP Vconn Src:False

TEST_PD_PROT_SNK_4_SinkWaitCapTimer_TimeoutExpected TestCondition:Rev2Snk and Configured TestCondition:Rev2Snk
TEST_PD_PROT_SNK_4_SinkWaitCapTimer_TimeoutExpected TestCondition:Rev3ChkdSnk and Configured TestCondition:Rev3ChkdSnk
Test conditions
StInd:7 StAMS:0 AftStInd:22 AftAMS:1 SpInd:55 SpAMS:3
StInd:56 StAMS:4 AftStInd:78 AftAMS:5 SpInd:119 SpAMS:7
SNK_4: vSafe5V min start time:3,912672
SNK_4: vSafe5V min start time:10,505616
#PD merged debug desc: Start of common field check validation : 17:33:25.7952546
Pkt Index: 25 skipped in Common_Check_PD_5_Check_Unexpected_Messages_And_Signals. HR/CR: False, SR: False, GC Not Exp: False, Not PDC AMS: False,PDC Reject:False, Skip AMS:NONE, Skip MsgTy:Hard_Reset PDO Ele:
Pkt Index: 34 skipped in Common_Check_PD_5_Check_Unexpected_Messages_And_Signals. HR/CR: False, SR: False, GC Not Exp: False, Not PDC AMS: False,PDC Reject:False, Skip AMS:NONE, Skip MsgTy:Hard_Reset PDO Ele:
Pkt Index: 81 skipped in Common_Check_PD_5_Check_Unexpected_Messages_And_Signals. HR/CR: False, SR: False, GC Not Exp: False, Not PDC AMS: False,PDC Reject:False, Skip AMS:NONE, Skip MsgTy:Hard_Reset PDO Ele:
Pkt Index: 92 skipped in Common_Check_PD_5_Check_Unexpected_Messages_And_Signals. HR/CR: False, SR: False, GC Not Exp: False, Not PDC AMS: False,PDC Reject:False, Skip AMS:NONE, Skip MsgTy:Hard_Reset PDO Ele:
StartTime :0,84016181, StopTime :0,84009681ObtainedTime :0,0649999999999817
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :0,84650084, StopTime :0,84643604ObtainedTime :0,064799999999976
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :1,16769625, StopTime :1,16763145ObtainedTime :0,064800000000087
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :5,86527803, StopTime :5,86521322ObtainedTime :0,0648099999995821
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :5,87163646, StopTime :5,87157166ObtainedTime :0,0648000000005311
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :6,19281907, StopTime :6,19275427ObtainedTime :0,0648000000005311
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :7,40573433, StopTime :7,40567633ObtainedTime :0,0580000000001135
Obtained time difference is 0,058ms, Expected time limit 0,025ms to 0,195ms
StartTime :7,41361018, StopTime :7,41354518ObtainedTime :0,0650000000002038
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :7,7356086, StopTime :7,7355438ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :12,46375843, StopTime :12,46369363ObtainedTime :0,0648000000005311
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :12,47161787, StopTime :12,47155287ObtainedTime :0,065000000001092
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :12,7936291, StopTime :12,7935643ObtainedTime :0,0648000000005311
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
Time Difference of GoodCRC of SourceCap and Request is 4,09062000000004ms at AMS Index : 0
Time Difference of GoodCRC of SourceCap and Request is 4,11181999999943ms at AMS Index : 3
Time Difference of GoodCRC of SourceCap and Request is 4,09122000000028ms at AMS Index : 4
Time Difference of GoodCRC of SourceCap and Request is 4,09601999999865ms at AMS Index : 7
Skipped: Power_Negotiation Index: 4
Skipped: Hard_Reset Index: 5
Skipped: Hard_Reset Index: 6
Validated: 0 packets
No Discover ID in TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout test case
Validated: 0 VCONN_Swap packets
Validated: 0 packets
#PD merged debug desc: Stop of common field check validation : 17:33:25.7962535
###Test condition validation: Assert count is not integrated
#PD Merged: Critical error - BU test result count is 1, Test case validation count 2
Read_All_Packets_Dynamic_Delay StAssertion Found :1283308517-->> 14/10/2025 17:33:25 
 LastADCTimeStamp before ADCRead 1321609663
 LastADCTimeStamp before ADCRead 1321609663
StreamStSpData_CC First Message StTime0,43305482 , SpTime0,43305482
StreamStSpData_CC Last Message StTime12,83308517 , SpTime12,83308517
StreamStSpData_LA
TimeStamp 25304959, TicksPerSample 123246, ValidSample 0
TimeStamp 53407985, TicksPerSample 123246, ValidSample 502
TimeStamp 63637617, TicksPerSample 123246, ValidSample 502
TimeStamp 1321609663, TicksPerSample 123246, ValidSample 502

10 /14/2025 05:33:25.796  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:33:30.822 :InteruptLasdcRead triggered
17_17_33_30_881: WorkerThread_CCline end
17_17_33_32_45: WorkerThreadLSADC end
InteruptLasdcRead:  m_LSADCthread: thread Aborted()
InteruptLasdcRead:  m_CClinethread: thread Aborted()
10 /14/2025 05:33:32.146  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
StopStreamer:  m_LSADCthread: thread Aborted()
StopStreamer:  m_CClinethread: thread Aborted()
StreamStSpData_LA
TimeStamp 25304959, TicksPerSample 123246, ValidSample 0
TimeStamp 53407985, TicksPerSample 123246, ValidSample 502
TimeStamp 63637617, TicksPerSample 123246, ValidSample 502
TimeStamp 1558858007, TicksPerSample 123246, ValidSample 502

StopTime Exec :14/10/2025 17:33:32
CreateHtmlDoc -->> New change
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - Updated
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - Updated
COMMON.PROC.BU.2 - Updated
Rev2Snk - Updated
Rev3ChkdSnk - Updated
TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout - Updated
Packet and signal mapping list PD_Merged -> TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout
TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout - 0
COMMON.PROC.BU.2 - -1
Packet Index is missing
Signal start or stop time is missing
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - 14
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 16
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - 65
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 67
Rev2Snk - -1
Packet Index is missing
Signal start or stop time is missing
SinkWaitCapTimer Timeout - TEST.PD.PROT.SNK.4#1 - -1
Packet Index is missing
Signal start or stop time is missing
Rev3ChkdSnk - -1
Packet Index is missing
Signal start or stop time is missing
SinkWaitCapTimer Timeout - TEST.PD.PROT.SNK.4#1 - -1
Packet Index is missing
Signal start or stop time is missing
CCline Thread State : (STOP)
LSADC Thread State : (STOP)
HSADC Thread State : (NONE)
QD Thread State : (NONE)

17:33:32     | Test Name(Stop): TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout
---------------------------------------------------------------------------------------------------------
10 /14/2025 05:33:32.525  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:33:32.690  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:33:32.844  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:33:32.858  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:33:32.873  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:33:32.887  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:33:32.902  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:33:32.916  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:33:32.931  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:33:32.945  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:33:32.960  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:33:32.974  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:33:32.989  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:33:33.004  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:33:33.018  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
AddTest - test result is null
10 /14/2025 05:33:33.034  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:33:33.205  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:33:33.375  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:33:33.389  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:33:33.404  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:33:33.418  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:33:33.432  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:33:33.447  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:33:33.462  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:33:33.477  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:33:33.491  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:33:33.505  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:33:33.520  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:33:33.535  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:33:33.550  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:33:34.565  Write Ethernet :FW Write:0x16, 0x24, 0x15, 0x00, 0x00,  , API description - PDM Mode setting
StopTime Exec :14/10/2025 17:33:35
CreateHtmlDoc -->> New change
CreateHtmlDoc -->> New change
<--TesterInfoStore--> 
GRL_USB_PD_Controller_Serial_No - Value : 397.409.397.077.376.
GRL_USB_PD_Software_Version - Value : 1.6.28.0
GRL_USB_PD_Firmware_Version - Value : 2.2.65
GRL USB-PD Ethernet Buffer Size - Value : 62K
GRL USB-PD Eload Firmware Version - Value : 9.8 / 9.8
Calibration - Value : Calibration Success
RX mask Power selection - Value : Neutral Power
Device_Type - Value : Consumer Only
Cable Type - Value : GRL_SPL_CABLE_1
Impedance (milli ohm) - Value : 0
PD_Merged CTS Version - Value : v.Q4-2024
USB_PD_Spec Version - Value : Rev3.2 Ver1.1RC2
USB_Type_C_Spec Version - Value : v2.3 Oct-2023
VIF_File_Name - Value : Parrot__MPPUA2__1__0_14_10_2025.xml
Noise Pattern Generation: - Value : Two-Tone Noise
Application mode - Value : Informational
Disabled all Pop-up during test execution - Value : False
Pop-up Timer - Value : 0
Rerun Enabled - Value : False
Rerun Count - Value : 1
Rerun Iteration - Value : 0
UI Live Update - Value : False
<--MOIsInfoStore--> 
Connect EPR Test Fixture - Value : False
FR_Swap AUTO Box Connected - Value : False
StopTime Exec :14/10/2025 17:33:35
CreateHtmlDoc -->> New change
