###
C2 Compliance Test Report

# Power Delivery 3.1 Tests- Result Summary

Sl No | Test ID | Test Name | Test Result
--- | --- | --- | ---
1 | InitialBringUpCapture | InitialBringUpCapture | NA

# Power Delivery 3.1 Tests - Detailed Test Result

Test Status | Test Description
--- | ---
NA | 1. InitialBringUpCapture

# Packet List

Index | Start time(s.ms.μs.ns) | Stop time(s.ms.μs.ns) | Message Origin | Message |  | Secondary Message | SOP | Port Type | Msg ID | PDO | Header(MSB to LSB) | Payload(LSB to MSB)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Get_Cap_PDMer |
Port A Packet Details
1 | 1,693 S | 1,693 S | T-> | Ra_Asserted |  |  | NONE | NONE/NONE/R- | 0 | Ra_CC2 | 0x0000 |
5 | 1,898 S | 1,898 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
7 | 1,899 S | 1,899 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Disabled -> FSM_State_Unattached_SRC | 0x0000 |
8 | 1,900 S | 1,900 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
9 | 1,900 S | 1,900 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
10 | 2,110 S | 2,110 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
12 | 2,167 S | 2,167 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 0 | FS: 5V ,1A; | 0x11A1 | 0x0A-0x90-0x01-0x3B-
13 | 2,169 S | 2,170 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 0 | FS: 5V ,1A; | 0x11A1 | 0x0A-0x90-0x01-0x3B-
14 | 2,172 S | 2,172 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 0 | FS: 5V ,1A; | 0x11A1 | 0x0A-0x90-0x01-0x3B-
16 | 2,277 S | 2,277 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 1 | FS: 5V ,1A; | 0x13A1 | 0x0A-0x90-0x01-0x3B-
17 | 2,279 S | 2,280 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 1 | FS: 5V ,1A; | 0x13A1 | 0x0A-0x90-0x01-0x3B-
18 | 2,282 S | 2,282 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 1 | FS: 5V ,1A; | 0x13A1 | 0x0A-0x90-0x01-0x3B-
20 | 2,387 S | 2,387 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 2 | FS: 5V ,1A; | 0x15A1 | 0x0A-0x90-0x01-0x3B-
21 | 2,389 S | 2,390 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 2 | FS: 5V ,1A; | 0x15A1 | 0x0A-0x90-0x01-0x3B-
22 | 2,392 S | 2,392 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 2 | FS: 5V ,1A; | 0x15A1 | 0x0A-0x90-0x01-0x3B-
24 | 2,497 S | 2,497 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 3 | FS: 5V ,1A; | 0x17A1 | 0x0A-0x90-0x01-0x3B-
25 | 2,497 S | 2,498 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 3 |  | 0x0641 |
26 | 2,502 S | 2,502 S | <-D |  | Request |  | SOP | UFP/Sink/R3 | 0 | PDO#1 Fixed; OpCurrent = 0,1A; MaxCurrent = 3A | 0x1082 | 0x2C-0x29-0x80-0x15-
27 | 2,502 S | 2,503 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 0 |  | 0x0121 |
28 | 2,505 S | 2,505 S | T-> | Accept |  |  | SOP | DFP/Source/R3 | 4 |  | 0x09A3 |
29 | 2,505 S | 2,506 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 4 |  | 0x0841 |
31 | 2,607 S | 2,607 S | T-> | PS_RDY |  |  | SOP | DFP/Source/R3 | 5 |  | 0x0BA6 |
32 | 2,607 S | 2,608 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 5 |  | 0x0A41 |
34 | 2,608 S | 2,608 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
35 | 2,710 S | 2,710 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
37 | 2,711 S | 2,711 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
39 | 2,730 S | 2,730 S | T-> | VendorDefined |  |  | SOP | DFP/Source/R3/VdmR2/ | 6 | Discover ID;Initiator; | 0x1DAF | 0x01-0xA0-0x00-0xFF-
40 | 2,730 S | 2,731 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 6 |  | 0x0C41 |
41 | 2,732 S | 2,733 S | <-D |  | VendorDefined |  | SOP | UFP/Sink/R3/VdmR2/ | 1 | Discover ID;ACK; | 0x428F | 0x41-0xA8-0x00-0xFF-0xCF-0x19-0x40-0x18-0x18-0x2E-0x00-0x00-0x14-0x07-0x00-0x64-
42 | 2,733 S | 2,734 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 1 |  | 0x0321 |
44 | 2,734 S | 2,734 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
46 | 2,777 S | 2,777 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
47 | 2,777 S | 2,777 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
49 | 2,785 S | 2,785 S | T-> | VendorDefined |  |  | SOP | DFP/Source/R3/VdmR2/ | 7 | Discover SVID;Initiator; | 0x1FAF | 0x02-0xA0-0x00-0xFF-
50 | 2,785 S | 2,786 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 7 |  | 0x0E41 |
51 | 2,790 S | 2,790 S | <-D |  | VendorDefined |  | SOP | UFP/Sink/R3/VdmR2/ | 2 | Discover SVID;NAK; | 0x148F | 0x82-0xA8-0x00-0xFF-
52 | 2,790 S | 2,791 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 2 |  | 0x0521 |
54 | 2,791 S | 2,791 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
55 | 2,893 S | 2,893 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
57 | 2,894 S | 2,894 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
59 | 2,902 S | 2,902 S | T-> | Get_Sink_Cap |  |  | SOP | DFP/Source/R3 | 0 |  | 0x01A8 |
60 | 2,902 S | 2,903 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 0 |  | 0x0041 |
61 | 2,907 S | 2,907 S | <-D |  | SinkCap |  | SOP | UFP/Sink/R3 | 3 | FS: 5V ,9A; VS: (9~20)V 3A; | 0x2684 | 0x5A-0x90-0x01-0x10-0x2C-0xD1-0x02-0x99-
62 | 2,907 S | 2,908 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 3 |  | 0x0721 |
64 | 2,908 S | 2,908 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
66 | 3,011 S | 3,011 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
67 | 3,011 S | 3,011 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
69 | 3,019 S | 3,019 S | T-> | Get_Sink_Cap_Ext |  |  | SOP | DFP/Source/R3 | 1 |  | 0x03B6 |
70 | 3,019 S | 3,020 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 1 |  | 0x0241 |
71 | 3,024 S | 3,025 S | <-D |  | Sink_Cap_Extended |  | SOP | UFP/Sink/R3 | 4 | UnChunked | 0x888F | 0x18-0x00-0xCF-0x19-0x00-0x64-0x18-0x2E-0x00-0x00-0xFF-0x06-0x01-0x00-0x00-0x00-0x00-0x00-0x02-0x1A-0x00-0x00-0x00-0x00-0x00-0x00-
72 | 3,025 S | 3,026 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 4 |  | 0x0921 |
74 | 3,026 S | 3,026 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
76 | 13.34 S | 13.34 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Disabled | 0x0000 |
77 | 13.34 S | 13.34 S | T-> | Detach |  |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |

# AMS Summary

AMS Index | AMS Name | AMS Start | AMS Stop | AMS Status | Child AMS Count
--- | --- | --- | --- | --- | ---

# DUT Information

Manufacturer | Parrot
Model Number | MPPUA2
Serial Number | 1

# Test Information

Test Lab |
Test_Engineer | Test_Engineer
Remarks | Remarks
Date_and_Time | 14/10/2025 17:20:32

# Controller and Instrument Information

Parameter | Value
--- | ---
GRL_USB_PD_Controller_Serial_No | 397.409.397.077.376.
GRL_USB_PD_Software_Version | 1.6.28.0
GRL_USB_PD_Firmware_Version | 2.2.65
GRL USB-PD Ethernet Buffer Size | 62K
GRL USB-PD Eload Firmware Version | 9.8 / 9.8
Calibration | Calibration Success
RX mask Power selection | Neutral Power
Device_Type | Consumer Only
Cable Type | GRL_SPL_CABLE_1
Impedance (milli ohm) | 0
PD_Merged CTS Version | v.Q4-2024
USB_PD_Spec Version | Rev3.2 Ver1.1RC2
USB_Type_C_Spec Version | v2.3 Oct-2023
VIF_File_Name | Parrot__MPPUA2__1__0_14_10_2025.xml
Noise Pattern Generation: | Two-Tone Noise
Application mode | Informational
Disabled all Pop-up during test execution | False
Pop-up Timer | 0
Rerun Enabled | False
Rerun Count | 1
Rerun Iteration | 0
UI Live Update | False
Execution Time(In Minutes) | 0

# Power Delivery 3.1 Tests Information

Parameter | Value
--- | ---
Connect EPR Test Fixture | False
FR_Swap AUTO Box Connected | False