###
C2 Compliance Test Report

# Power Delivery 3.1 Tests- Result Summary

Sl No | Test ID | Test Name | Test Result
--- | --- | --- | ---
1 | TEST.PD.PROT.SNK.4 | TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout | WARNING

# Power Delivery 3.1 Tests - Detailed Test Result

Test Status | Test Description
--- | ---
WARNING | 1. TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout
PASS | COMMON.PROC.BU.2:
PASS | COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk:
| SourceCap Packet14
PASS | UUT should respond with request - - COMMON.PROC.BU.2#1:
| Request Packet16
PASS | COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk:
| SourceCap Packet65
PASS | UUT should respond with request - - COMMON.PROC.BU.2#1:
| Request Packet67
WARNING | Rev2Snk:
WARNING | SinkWaitCapTimer Timeout - TEST.PD.PROT.SNK.4#1:
| Measured tTypeCSinkWaitCap value is 641.8 mS which is more than expected limit[310ms ~ 620ms]
WARNING | Rev3ChkdSnk:
WARNING | SinkWaitCapTimer Timeout - TEST.PD.PROT.SNK.4#1:
| Measured tTypeCSinkWaitCap value is 639.2 mS which is more than expected limit[310ms ~ 620ms]

# Packet List (Click to View AMS Summary)

Index | Start time(s.ms.μs.ns) | Stop time(s.ms.μs.ns) | Message Origin | Message |  | Secondary Message | SOP | Port Type | Msg ID | PDO | Header(MSB to LSB) | Payload(LSB to MSB)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout |
Port A Packet Details
4 | 636.4 mS | 636.4 mS | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
5 | 636.7 mS | 636.7 mS | T-> | Ra_Asserted |  |  | NONE | NONE/NONE/R- | 0 | Ra_CC2 | 0x0000 |
10 | 636.8 mS | 636.8 mS | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Disabled -> FSM_State_Unattached_SRC | 0x0000 |
11 | 638.1 mS | 638.1 mS | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
12 | 638.1 mS | 638.1 mS | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
13 | 788.2 mS | 788.2 mS | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
14 | 839.5 mS | 840.1 mS | T-> | SourceCap |  |  | SOP | DFP/Source/R2 | 0 | FS: 5V ,1A; | 0x1161 | 0x0A-0x90-0x01-0x28-
15 | 840.2 mS | 840.7 mS | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 0 |  | 0x0041 |
16 | 844.7 mS | 845.4 mS | <-D |  | Request |  | SOP | UFP/Sink/R2 | 0 | PDO#1 Fixed; OpCurrent = 0,1A; MaxCurrent = 3A | 0x1042 | 0x2C-0x29-0x00-0x15-
17 | 845.4 mS | 845.9 mS | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 0 |  | 0x0121 |
18 | 846.0 mS | 846.4 mS | T-> | Accept |  |  | SOP | DFP/Source/R2 | 1 |  | 0x0363 |
19 | 846.5 mS | 847.0 mS | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 1 |  | 0x0241 |
20 | 1,167 S | 1,168 S | T-> | PS_RDY |  |  | SOP | DFP/Source/R2 | 2 |  | 0x0566 |
21 | 1,168 S | 1,168 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 2 |  | 0x0441 |
25 | 2,639 S | 2,639 S | T-> | Hard_Reset |  |  | HARD_RESET | NONE/NONE/R- | 0 |  | 0x0000 |
27 | 2,761 S | 2,761 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Unattached_SRC | 0x0000 |
28 | 2,761 S | 2,761 S | T-> |  | Detach |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |
29 | 2,761 S | 2,761 S | <-D |  | NONE | LOAD_CURRENT | NONE | NONE/NONE/R- | 0 | LOAD_CURRENT:0A | 0x0000 |
30 | 3,760 S | 3,760 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
31 | 3,762 S | 3,762 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
32 | 3,762 S | 3,762 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
33 | 3,912 S | 3,912 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
34 | 4,554 S | 4,555 S | <-D |  | Hard_Reset |  | HARD_RESET | NONE/NONE/R- | 0 |  | 0x0000 |
36 | 4,672 S | 4,672 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Unattached_SRC | 0x0000 |
37 | 4,672 S | 4,672 S | T-> |  | Detach |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |
38 | 4,673 S | 4,673 S | <-D |  | NONE | LOAD_CURRENT | NONE | NONE/NONE/R- | 0 | LOAD_CURRENT:0A | 0x0000 |
39 | 5,671 S | 5,671 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
40 | 5,673 S | 5,673 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
41 | 5,673 S | 5,673 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
42 | 5,823 S | 5,823 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
43 | 5,865 S | 5,865 S | T-> | SourceCap |  |  | SOP | DFP/Source/R2 | 0 | FS: 5V ,1A; | 0x1161 | 0x0A-0x90-0x01-0x3A-
44 | 5,865 S | 5,866 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 0 |  | 0x0041 |
45 | 5,870 S | 5,871 S | <-D |  | Request |  | SOP | UFP/Sink/R2 | 0 | PDO#1 Fixed; OpCurrent = 0,1A; MaxCurrent = 3A | 0x1042 | 0x2C-0x29-0x00-0x15-
46 | 5,871 S | 5,871 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 0 |  | 0x0121 |
47 | 5,871 S | 5,872 S | T-> | Accept |  |  | SOP | DFP/Source/R2 | 1 |  | 0x0363 |
48 | 5,872 S | 5,872 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 1 |  | 0x0241 |
49 | 6,192 S | 6,193 S | T-> | PS_RDY |  |  | SOP | DFP/Source/R2 | 2 |  | 0x0566 |
50 | 6,193 S | 6,193 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 2 |  | 0x0441 |
51 | 6,204 S | 6,204 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Disabled | 0x0000 |
52 | 6,204 S | 6,204 S | T-> | Detach |  |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |
53 | 6,206 S | 6,206 S | <-D |  | NONE | LOAD_CURRENT | NONE | NONE/NONE/R- | 0 | LOAD_CURRENT:0A | 0x0000 |
54 | 7,206 S | 7,206 S | T-> | Ra_Asserted |  |  | NONE | NONE/NONE/R- | 0 | Ra_CC2 | 0x0000 |
59 | 7,206 S | 7,206 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Disabled -> FSM_State_Unattached_SRC | 0x0000 |
60 | 7,206 S | 7,206 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
61 | 7,207 S | 7,207 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
62 | 7,207 S | 7,207 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
63 | 7,358 S | 7,358 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
65 | 7,405 S | 7,406 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 0 | FS: 5V ,1A; | 0x11A1 | 0x0A-0x90-0x01-0x28-
66 | 7,406 S | 7,406 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 0 |  | 0x0041 |
67 | 7,410 S | 7,411 S | <-D |  | Request |  | SOP | UFP/Sink/R3 | 0 | PDO#1 Fixed; OpCurrent = 0,1A; MaxCurrent = 3A | 0x1082 | 0x2C-0x29-0x80-0x15-
68 | 7,411 S | 7,411 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 0 |  | 0x0121 |
69 | 7,413 S | 7,414 S | T-> | Accept |  |  | SOP | DFP/Source/R3 | 1 |  | 0x03A3 |
70 | 7,414 S | 7,414 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 1 |  | 0x0241 |
71 | 7,735 S | 7,736 S | T-> | PS_RDY |  |  | SOP | DFP/Source/R3 | 2 |  | 0x05A6 |
72 | 7,736 S | 7,736 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 2 |  | 0x0441 |
74 | 7,736 S | 7,736 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
76 | 9,207 S | 9,207 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
77 | 9,207 S | 9,207 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
81 | 9,227 S | 9,227 S | T-> | Hard_Reset |  |  | HARD_RESET | NONE/NONE/R- | 0 |  | 0x0000 |
84 | 9,352 S | 9,352 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Unattached_SRC | 0x0000 |
85 | 9,352 S | 9,352 S | T-> |  | Detach |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |
86 | 9,352 S | 9,352 S | <-D |  | NONE | LOAD_CURRENT | NONE | NONE/NONE/R- | 0 | LOAD_CURRENT:0A | 0x0000 |
87 | 10.35 S | 10.35 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
88 | 10.35 S | 10.35 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
89 | 10.35 S | 10.35 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
90 | 10.50 S | 10.50 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
92 | 11.14 S | 11.15 S | <-D |  | Hard_Reset |  | HARD_RESET | NONE/NONE/R- | 0 |  | 0x0000 |
95 | 11.27 S | 11.27 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Unattached_SRC | 0x0000 |
96 | 11.27 S | 11.27 S | T-> |  | Detach |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |
97 | 11.27 S | 11.27 S | <-D |  | NONE | LOAD_CURRENT | NONE | NONE/NONE/R- | 0 | LOAD_CURRENT:0A | 0x0000 |
98 | 12.27 S | 12.27 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
99 | 12.27 S | 12.27 S | T-> | Attach |  | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
100 | 12.27 S | 12.27 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Unattached_SRC -> FSM_State_AttachWait_SRC | 0x0000 |
101 | 12.42 S | 12.42 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_AttachWait_SRC -> FSM_State_Attached_SRC | 0x0000 |
103 | 12.46 S | 12.46 S | T-> | SourceCap |  |  | SOP | DFP/Source/R3 | 0 | FS: 5V ,1A; | 0x11A1 | 0x0A-0x90-0x01-0x3A-
104 | 12.46 S | 12.46 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 0 |  | 0x0041 |
105 | 12.47 S | 12.47 S | <-D |  | Request |  | SOP | UFP/Sink/R3 | 0 | PDO#1 Fixed; OpCurrent = 0,1A; MaxCurrent = 3A | 0x1082 | 0x2C-0x29-0x80-0x15-
106 | 12.47 S | 12.47 S | T-> | GoodCRC |  |  | SOP | DFP/Source/R1 | 0 |  | 0x0121 |
107 | 12.47 S | 12.47 S | T-> | Accept |  |  | SOP | DFP/Source/R3 | 1 |  | 0x03A3 |
108 | 12.47 S | 12.47 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 1 |  | 0x0241 |
109 | 12.79 S | 12.79 S | T-> | PS_RDY |  |  | SOP | DFP/Source/R3 | 2 |  | 0x05A6 |
110 | 12.79 S | 12.79 S | <-D |  | GoodCRC |  | SOP | UFP/Sink/R2 | 2 |  | 0x0441 |
112 | 12.79 S | 12.79 S | T-> |  | Rp_Asserted | Rp_4_7k_3A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_4_7k_3A_Asserted | 0x0000 |
114 | 12.80 S | 12.80 S | T-> |  | Rp_Asserted | Rp_12k_1_5A_Asserted | NONE | NONE/NONE/R- | 0 | Rp_12k_1_5A_Asserted | 0x0000 |
115 | 12.80 S | 12.80 S | <-D |  | Rd_Detected |  | NONE | NONE/NONE/R- | 0 | Rd in CC1; | 0x0000 |
116 | 12.82 S | 12.82 S | T-> | FSM_State_Transition |  |  | NONE | NONE/NONE/R- | 0 | FSM_State_Attached_SRC -> FSM_State_Disabled | 0x0000 |
117 | 12.82 S | 12.82 S | T-> | Detach |  |  | NONE | NONE/NONE/- | 0 | NONE | 0x0000 |
118 | 12.83 S | 12.83 S | <-D |  | NONE | LOAD_CURRENT | NONE | NONE/NONE/R- | 0 | LOAD_CURRENT:0A | 0x0000 |

# AMS Summary

AMS Index | AMS Name | AMS Start | AMS Stop | AMS Status | Child AMS Count
--- | --- | --- | --- | --- | ---
0 | Power_Negotiation | 14 | 21 | COMPLETE | 0
1 | Hard_Reset | 25 | 25 | COMPLETE | 0
2 | Hard_Reset | 34 | 34 | COMPLETE | 0
3 | Power_Negotiation | 43 | 50 | COMPLETE | 0
4 | Power_Negotiation | 65 | 72 | COMPLETE | 0
5 | Hard_Reset | 81 | 81 | COMPLETE | 0
6 | Hard_Reset | 92 | 92 | COMPLETE | 0
7 | Power_Negotiation | 103 | 110 | COMPLETE | 0

# DUT Information

Manufacturer | Parrot
Model Number | MPPUA2
Serial Number | 1

# Test Information

Test Lab |
Test_Engineer | Test_Engineer
Remarks | Remarks
Date_and_Time | 14/10/2025 17:33:32

# Controller and Instrument Information

Parameter | Value
--- | ---
GRL_USB_PD_Controller_Serial_No | 397.409.397.077.376.
GRL_USB_PD_Software_Version | 1.6.28.0
GRL_USB_PD_Firmware_Version | 2.2.65
GRL USB-PD Ethernet Buffer Size | 62K
GRL USB-PD Eload Firmware Version | 9.8 / 9.8
Calibration | Calibration Success
RX mask Power selection | Neutral Power
Device_Type | Consumer Only
Cable Type | GRL_SPL_CABLE_1
Impedance (milli ohm) | 0
PD_Merged CTS Version | v.Q4-2024
USB_PD_Spec Version | Rev3.2 Ver1.1RC2
USB_Type_C_Spec Version | v2.3 Oct-2023
VIF_File_Name | Parrot__MPPUA2__1__0_14_10_2025.xml
Noise Pattern Generation: | Two-Tone Noise
Application mode | Informational
Disabled all Pop-up during test execution | False
Pop-up Timer | 0
Rerun Enabled | False
Rerun Count | 1
Rerun Iteration | 0
UI Live Update | False
Execution Time(In Minutes) | 1

# Power Delivery 3.1 Tests Information

Parameter | Value
--- | ---
Connect EPR Test Fixture | False
FR_Swap AUTO Box Connected | False