##########C:\GRL\USBPD-C2-Browser-App\Report\TempReport\C2\MPPUA2_2025_10_14-16_06_47\New_Run17_Rep0_2025_10_14-05_17_53\GRL_USB_PD_Report_Run_17_2025_10_14.html
Test res file is available
Test res file is not null
Not DP AUX
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:20:05.868 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0xD5, 
Application Type C2 decoded value is 1
StartTime Exec :2025_10_14-05_20_05
SW_BuildPurpose :DebugMode
10 /14/2025 05:20:05.884  Write Ethernet :FW Write:0x16, 0x22, 0x04, 0x01,  , API description - PD interrupts
10 /14/2025 05:20:05.898  Write Ethernet :FW Write:0x16, 0x10, 0x01, 0x00, 0x00, 
Port A VBUS Resistance: 114
Port A CC2 Resistance: 930
Port A CC1 Resistance: 930
Port B VBUS Resistance: 114
Port B CC2 Resistance: 930
Port B CC1 Resistance: 930
IRDropVBUSValue0
IRDropCC1Value0
IRDropCC1Value0
10 /14/2025 05:20:05.913  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
##########C:\GRL\USBPD-C2-Browser-App\Report\TempReport\C2\MPPUA2_2025_10_14-16_06_47\New_Run17_Rep0_2025_10_14-05_17_53\GRL_USB_PD_Report_Run_17_2025_10_14.html
10 /14/2025 05:20:07.133  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:20:07.305  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:20:07.475  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:20:07.490  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:20:07.504  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:20:07.519  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:20:07.534  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:20:07.548  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:20:07.563  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:20:07.577  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:20:07.592  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:20:07.606  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:20:07.621  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:20:07.636  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:20:07.650  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:20:07.665  Write Ethernet :FW Write:0x6F, 0x02,  , API description - Setting Controller Configuaton :RA_CC2
10 /14/2025 05:20:07.837  Write Ethernet :FW Write:0x16, 0x00, 0x80, 0x01,  , API description - Set revision number
10 /14/2025 05:20:07.852  Write Ethernet :FW Write:0x16, 0x02, 0x20, 0x01,  , API description - Set VDM revision number
10 /14/2025 05:20:07.867  Write Ethernet :FW Write:0x3E, 0x00,  , API description - Initiate DR_Swap
10 /14/2025 05:20:07.946  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:20:07.960  Write Ethernet :FW Write:0x3F, 0x00, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:20:07.975  Write Ethernet :FW Write:0x16, 0x0C, 0x05, 0x00, 0x0B, 0x00, 0x00, 0x80, 0x00, 0x00, 
10 /14/2025 05:20:07.990  Write Ethernet :FW Write:0x54,  , API description - Setting Controller Configuaton :VDM_DiscovIdAck_All_SOP
10 /14/2025 05:20:08.147  Write Ethernet :FW Write:0x16, 0x01, 0x00, 0x01,  , API description - Enable unchunked message support
10 /14/2025 05:20:08.162  Write Ethernet :FW Write:0x5E, 0xC1, 0x3D, 0x00, 0x0A, 
10 /14/2025 05:20:08.176  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:20:08.190  Write Ethernet :FW Write:0x18, 0x00,  , API description - Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:20:08.351  Write Ethernet :FW Write:0x18, 0x09,  , API description - Setting Controller Configuaton :SimulateDetach_CC1_CC2
10 /14/2025 05:20:08.506  Write Ethernet :FW Write:0x0E,  , API description - Setting Controller Configuaton :PHY_RESET
ResetDataManager - End of Reset all RTDataChunk

---------------------------------------------------------------------------------------------------------
17:20:08 Test Name(Start): InitialBringUpCapture
Tester cable drop compensation : False
10 /14/2025 05:20:08.692  Write Ethernet :FW Write:0x16, 0x21, 0x07, 0x00, 0x00, 0x00, 0x00, 0x01, 
DataStreamerSertvice -->>StartStreamer()-->> SubSampleRatio -->>500
Reset board API start
10 /14/2025 05:20:08.707  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:08.743  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:08.758  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x10,  , API description - Enable LSADC
10 /14/2025 05:20:08.773  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:08.787  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:08.801  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:20:08.815  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x00,  , API description - Reset DMA :DMA0_CCLinePortA
10 /14/2025 05:20:08.829  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x01,  , API description - Reset DMA :DMA1_CCLinePortB
10 /14/2025 05:20:08.844  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x02,  , API description - Reset DMA :DMA2_LSADC_Port_A_B
10 /14/2025 05:20:08.859  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:20:08.977  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:20:08.991  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:09.005  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:09.019  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:20:09.034  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:09.048  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:09.063  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:20:09.111  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x40, 0x02, 0x00, 0x00, 0x00, 0x00,  , API description - Configure LSADC Sub Sampling
###LSADC channel debug
Without adding dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

With dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

10 /14/2025 05:20:09.125  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x04, 0x02, 0x00, 0x00, 0x15, 0x33, 0x00, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:20:09.140  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x08, 0x02, 0x00, 0x00, 0x88, 0xC6, 0x02, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:20:09.154  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x0C, 0x02, 0x00, 0x00, 0x88, 0x00, 0x00, 0x0A,  , API description - Configure Port A Channels
10 /14/2025 05:20:09.168  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x20, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.183  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x24, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.197  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x28, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.211  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x2C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.225  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x30, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.240  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x34, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.255  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x38, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.270  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x3C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0x00, 0x00,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:09.285  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x1C, 0x02, 0x00, 0x00, 0x3F, 0x00,  , API description - Configure LSADC Sub Sampling
10 /14/2025 05:20:09.299  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x10, 0x02, 0x00, 0x00, 0xFB, 0x00, 0x00, 0xF0,  , API description - Time stamp configuration
10 /14/2025 05:20:09.314  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x09,  , API description - Enable LSADC
10 /14/2025 05:20:09.328  Write Ethernet :FW Write:0x6B, 0x01, 0x23, 0x04, 0x06, 0x02, 0xFF, 0xFF,  , API description - Switch LSADC Ch8 Path
10 /14/2025 05:20:09.358 Read Ethernet :FW Read:0xFE, 0x00, 0x05, 0xE4, 0x02, 0x00, 0x00, 
C2Lib: StartStreamer(): 17_17_20_9_363
10 /14/2025 05:20:09.363  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:09.388  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
17_17_20_9_402: WorkerThreadLSADC start
17_17_20_9_403: WorkerThread_CCline start
10 /14/2025 05:20:09.403  Write Ethernet :FW Write:0x16, 0x24, 0x0B, 0x01, 0x00, 0x00, 0x00,  , API description - Enable/Disable Configure
10 /14/2025 05:20:10.069 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.102 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.134 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.166 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.196 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.228 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.260 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.290 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.320 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.366 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.414 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.445 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.476 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.506 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.537 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.569 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.599 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.630 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.661 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
10 /14/2025 05:20:10.691 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x03, 
Configured message: 0->Setting Controller Configuaton :RA_CC2
Configured message: 1->Setting Controller Configuaton :SimulateAttach
Configured message: 2->Setting Controller Configuaton :Source
Configured message: 3->Setting Controller Configuaton :Source
Configured message: 4->VDM
Configured message: 5->VDM
Configured message: 6->
Configured message: 7->
10 /14/2025 05:20:10.721  Write Ethernet :FW Write:0x6E, 0x66, 0x00, 0x00, 0x08, 0x00, 0x00, 0x09, 0x00, 0x04, 0x00, 0x05, 0x00, 0x05, 0x00, 0x00, 0x6F, 0x02, 0x09, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x18, 0x00, 0x09, 0x00, 0x04, 0x00, 0x05, 0x00, 0x05, 0x00, 0x00, 0x14, 0x03, 0x09, 0x00, 0x06, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x18, 0x01, 0x0D, 0x00, 0x03, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x4F, 0x10, 0x01, 0x80, 0x00, 0xFF, 0x0D, 0x00, 0x03, 0x00, 0x64, 0x00, 0x28, 0x00, 0x00, 0x4F, 0x10, 0x02, 0x80, 0x00, 0xFF, 0x0C, 0x00, 0x07, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x2C, 0x03, 0x00, 0x48, 0x00, 0x0C, 0x00, 0x07, 0x00, 0x64,  ..... , API description - Group Configuration Command
10 /14/2025 05:20:10.735  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:20:10.893 
10 /14/2025 05:20:11.908 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
10 /14/2025 05:20:12.925 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
14/10/2025 17:20:12 : PD merged: Group command configuration status True and count 0/8
PD merged: End of group command configuration 10 /14/2025 05:20:12.925 
10 /14/2025 05:20:15.928  Write Ethernet :FW Write:0x6E, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Group Configuration Command
10 /14/2025 05:20:15.943  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
CCLine Read Started :14/10/2025 17:20:16
Configured message: 0->Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:20:22.272  Write Ethernet :FW Write:0x6E, 0x0B, 0x00, 0x00, 0x01, 0x00, 0x00, 0x09, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x18, 0x00,  , API description - Group Configuration Command
10 /14/2025 05:20:22.287  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:20:22.459 
10 /14/2025 05:20:23.475 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:20:23.475 
StreamStSpData_LA
TimeStamp 26626425, TicksPerSample 123246, ValidSample 502
TimeStamp 36856018, TicksPerSample 123246, ValidSample 502
TimeStamp 47208557, TicksPerSample 123246, ValidSample 502
TimeStamp 1707332302, TicksPerSample 123246, ValidSample 502

10 /14/2025 05:20:26.478  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:31.504 :InteruptLasdcRead triggered
17_17_20_31_592: WorkerThread_CCline end
17_17_20_32_25: WorkerThreadLSADC end
InteruptLasdcRead:  m_LSADCthread: thread Aborted()
InteruptLasdcRead:  m_CClinethread: thread Aborted()
10 /14/2025 05:20:32.122  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
StopStreamer:  m_LSADCthread: thread Aborted()
StopStreamer:  m_CClinethread: thread Aborted()
StreamStSpData_LA
TimeStamp 26626425, TicksPerSample 123246, ValidSample 502
TimeStamp 36856018, TicksPerSample 123246, ValidSample 502
TimeStamp 47208557, TicksPerSample 123246, ValidSample 502
TimeStamp 2264157730, TicksPerSample 123246, ValidSample 502

StopTime Exec :14/10/2025 17:20:32
CreateHtmlDoc -->> New change
SPR_Adjustable_Voltage_Supply is not supported by UUT
10 /14/2025 05:20:32.491  Write Ethernet :FW Write:0x16, 0x36, 0x00, 0x02, 0x01, 0x00, 0x00, 0x01, 0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x02, 0x04, 0x00,  , API description - PDMVIFData
10 /14/2025 05:20:32.506  Write Ethernet :FW Write:0x16, 0x36, 0x01,  , API description - VIFSrcPDOInfo
10 /14/2025 05:20:32.520  Write Ethernet :FW Write:0x16, 0x36, 0x02, 0x00, 0x64, 0x00, 0x5A, 0x00, 0x00, 0x00, 0x02, 0xB4, 0x00, 0x90, 0x01, 0x2C, 0x01,  , API description - VIFSnkPDOInfo
10 /14/2025 05:20:32.535  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:20:32.704  Write Ethernet :FW Write:0x6F, 0x02,  , API description - Setting Controller Configuaton :RA_CC2
10 /14/2025 05:20:32.865  Write Ethernet :FW Write:0x16, 0x00, 0x80, 0x01,  , API description - Set revision number
10 /14/2025 05:20:32.879  Write Ethernet :FW Write:0x16, 0x02, 0x20, 0x01,  , API description - Set VDM revision number
10 /14/2025 05:20:32.893  Write Ethernet :FW Write:0x3E, 0x00,  , API description - Initiate DR_Swap
10 /14/2025 05:20:32.960  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:20:32.975  Write Ethernet :FW Write:0x3F, 0x00, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:20:32.990  Write Ethernet :FW Write:0x16, 0x0C, 0x05, 0x00, 0x0B, 0x00, 0x00, 0x80, 0x00, 0x00, 
10 /14/2025 05:20:33.004  Write Ethernet :FW Write:0x54,  , API description - Setting Controller Configuaton :VDM_DiscovIdAck_All_SOP
10 /14/2025 05:20:33.163  Write Ethernet :FW Write:0x16, 0x01, 0x00, 0x01,  , API description - Enable unchunked message support
10 /14/2025 05:20:33.177  Write Ethernet :FW Write:0x5E, 0xC1, 0x3D, 0x00, 0x0A, 
10 /14/2025 05:20:33.191  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:20:33.206  Write Ethernet :FW Write:0x3E, 0x02,  , API description - Initiate DR_Swap
10 /14/2025 05:20:33.273  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:20:33.288  Write Ethernet :FW Write:0x3F, 0x02, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:20:33.303  Write Ethernet :FW Write:0x18, 0x00,  , API description - Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:20:33.475  Write Ethernet :FW Write:0x18, 0x09,  , API description - Setting Controller Configuaton :SimulateDetach_CC1_CC2
10 /14/2025 05:20:33.646  Write Ethernet :FW Write:0x0E,  , API description - Setting Controller Configuaton :PHY_RESET
ResetDataManager - End of Reset all RTDataChunk

---------------------------------------------------------------------------------------------------------
17:20:33 Test Name(Start): TEST.PD.PROT.SNK.3 SinkWaitCapTimer Deadline
Tester cable drop compensation : False
10 /14/2025 05:20:33.824  Write Ethernet :FW Write:0x16, 0x21, 0x07, 0x00, 0x00, 0x00, 0x00, 0x01, 
DataStreamerSertvice -->>StartStreamer()-->> SubSampleRatio -->>500
Reset board API start
10 /14/2025 05:20:33.839  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:33.879  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:33.893  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x10,  , API description - Enable LSADC
10 /14/2025 05:20:33.908  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:33.923  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:33.938  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:20:33.953  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x00,  , API description - Reset DMA :DMA0_CCLinePortA
10 /14/2025 05:20:33.968  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x01,  , API description - Reset DMA :DMA1_CCLinePortB
10 /14/2025 05:20:33.983  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x02,  , API description - Reset DMA :DMA2_LSADC_Port_A_B
10 /14/2025 05:20:33.997  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:20:34.114  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:20:34.128  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:34.143  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:34.158  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:20:34.173  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:34.187  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:34.201  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:20:34.252  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x40, 0x02, 0x00, 0x00, 0x00, 0x00,  , API description - Configure LSADC Sub Sampling
###LSADC channel debug
Without adding dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

With dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

10 /14/2025 05:20:34.267  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x04, 0x02, 0x00, 0x00, 0x15, 0x33, 0x00, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:20:34.282  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x08, 0x02, 0x00, 0x00, 0x88, 0xC6, 0x02, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:20:34.297  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x0C, 0x02, 0x00, 0x00, 0x88, 0x00, 0x00, 0x0A,  , API description - Configure Port A Channels
10 /14/2025 05:20:34.311  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x20, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.325  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x24, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.340  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x28, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.354  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x2C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.369  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x30, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.383  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x34, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.398  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x38, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.413  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x3C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0x00, 0x00,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:34.427  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x10, 0x02, 0x00, 0x00, 0xFB, 0x00, 0x00, 0xF0,  , API description - Time stamp configuration
10 /14/2025 05:20:34.441  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x09,  , API description - Enable LSADC
10 /14/2025 05:20:34.456  Write Ethernet :FW Write:0x6B, 0x01, 0x23, 0x04, 0x06, 0x02, 0xFF, 0xFF,  , API description - Switch LSADC Ch8 Path
10 /14/2025 05:20:34.485 Read Ethernet :FW Read:0xFE, 0x00, 0x05, 0xE4, 0x02, 0x00, 0x00, 
C2Lib: StartStreamer(): 17_17_20_34_487
10 /14/2025 05:20:34.487  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:34.523  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
17_17_20_34_538: WorkerThreadLSADC start
17_17_20_34_538: WorkerThread_CCline start
Present Test case TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline EPR Flag Status False and enableForNonTestCases False
Consolidate message group
0 -> 0x16, 0x24, 0x15, 0x01, 0x00,  PDM Mode setting RxTimer:50 and TxTimer:50
1 -> 0x16, 0x35, 0x00, 0x4F, 0x00, 0x00, 0x01,  Start PDM test case 79 RxTimer:100 and TxTimer:100
10 /14/2025 05:20:34.539  Write Ethernet :FW Write:0x16, 0x24, 0x0B, 0x01, 0x00, 0x00, 0x00,  , API description - Enable/Disable Configure
Configured message: 0->PDM Mode setting
Configured message: 1->Start PDM test case 79
10 /14/2025 05:20:34.553  Write Ethernet :FW Write:0x6E, 0x1E, 0x00, 0x00, 0x02, 0x00, 0x00, 0x0C, 0x00, 0x04, 0x00, 0x32, 0x00, 0x32, 0x00, 0x00, 0x16, 0x24, 0x15, 0x01, 0x00, 0x0E, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x16, 0x35, 0x00, 0x4F, 0x00, 0x00, 0x01,  , API description - Group Configuration Command
10 /14/2025 05:20:34.567  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:20:34.730 
10 /14/2025 05:20:35.745 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:20:35.748 
Start : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:20:36 
Read_All_Packets_Dynamic_Delay StAssertion Found :969965280-->> 14/10/2025 17:20:44 
 LastADCTimeStamp before ADCRead 1022271960
 LastADCTimeStamp before ADCRead 1022271960
Stop : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:20:44 
DUT Behaviour -- Index: 14, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 39, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
DUT Behaviour -- Index: 62, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 90, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS merge Bef
AMS merge Aft
DUT role after Swap or PDC
14 Pow:Sink Dat:UFP Vconn Src:False
39 Pow:Sink Dat:UFP Vconn Src:False
62 Pow:Sink Dat:UFP Vconn Src:False
90 Pow:Sink Dat:UFP Vconn Src:False

TEST_PD_PROT_SNK_3_SinkWaitCapTimer_DeadlineExpected TestCondition:Rev2Snk and Configured TestCondition:Rev2Snk
TEST_PD_PROT_SNK_3_SinkWaitCapTimer_DeadlineExpected TestCondition:Rev3ChkdSnk and Configured TestCondition:Rev3ChkdSnk
Test conditions
StInd:6 StAMS:0 AftStInd:34 AftAMS:1 SpInd:52 SpAMS:1
StInd:53 StAMS:2 AftStInd:84 AftAMS:3 SpInd:108 SpAMS:3
#PD merged debug desc: Start of common field check validation : 17:20:44.7622541
StartTime :1,15731805, StopTime :1,15725325ObtainedTime :0,064799999999865
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :1,16366049, StopTime :1,16359569ObtainedTime :0,064800000000087
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :1,48486891, StopTime :1,48480391ObtainedTime :0,0649999999999817
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :3,90132583, StopTime :3,90126083ObtainedTime :0,0650000000002038
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :3,90767447, StopTime :3,90760967ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :4,22837068, StopTime :4,22830588ObtainedTime :0,0648000000005311
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :6,17130975, StopTime :6,17124495ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :6,1791718, StopTime :6,179117ObtainedTime :0,0548000000000215
Obtained time difference is 0,055ms, Expected time limit 0,025ms to 0,195ms
StartTime :6,50117683, StopTime :6,50111883ObtainedTime :0,0580000000001135
Obtained time difference is 0,058ms, Expected time limit 0,025ms to 0,195ms
StartTime :8,9343008, StopTime :8,9342494ObtainedTime :0,0514000000002568
Obtained time difference is 0,051ms, Expected time limit 0,025ms to 0,195ms
StartTime :8,94218285, StopTime :8,94212145ObtainedTime :0,0613999999998782
Obtained time difference is 0,061ms, Expected time limit 0,025ms to 0,195ms
StartTime :9,26418449, StopTime :9,26412329ObtainedTime :0,0611999999993174
Obtained time difference is 0,061ms, Expected time limit 0,025ms to 0,195ms
Time Difference of GoodCRC of SourceCap and Request is 4,0864399999998ms at AMS Index : 0
Time Difference of GoodCRC of SourceCap and Request is 4,10103000000017ms at AMS Index : 1
Time Difference of GoodCRC of SourceCap and Request is 4,10021999999977ms at AMS Index : 2
Time Difference of GoodCRC of SourceCap and Request is 4,10121999999902ms at AMS Index : 3
Skipped: Power_Negotiation Index: 2
Validated: 0 packets
No Discover ID in TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline test case
Validated: 0 VCONN_Swap packets
Validated: 0 packets
#PD merged debug desc: Stop of common field check validation : 17:20:44.7633188
###Test condition validation: Assert count is not integrated
#PD Merged: Critical error - BU test result count is 1, Test case validation count 2
Read_All_Packets_Dynamic_Delay StAssertion Found :969965280-->> 14/10/2025 17:20:44 
 LastADCTimeStamp before ADCRead 1022271960
 LastADCTimeStamp before ADCRead 1022271960
StreamStSpData_CC First Message StTime0,42962891 , SpTime0,42962891
StreamStSpData_CC Last Message StTime9,6996528 , SpTime9,6996528
StreamStSpData_LA
TimeStamp 25401211, TicksPerSample 123246, ValidSample 502
TimeStamp 35630804, TicksPerSample 123246, ValidSample 502
TimeStamp 45983097, TicksPerSample 123246, ValidSample 346
TimeStamp 1022271960, TicksPerSample 123246, ValidSample 502

10 /14/2025 05:20:44.763  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:49.783 :InteruptLasdcRead triggered
17_17_20_49_800: WorkerThread_CCline end
17_17_20_49_911: WorkerThreadLSADC end
InteruptLasdcRead:  m_LSADCthread: thread Aborted()
InteruptLasdcRead:  m_CClinethread: thread Aborted()
10 /14/2025 05:20:50.011  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
StopStreamer:  m_LSADCthread: thread Aborted()
StopStreamer:  m_CClinethread: thread Aborted()
StreamStSpData_LA
TimeStamp 25401211, TicksPerSample 123246, ValidSample 502
TimeStamp 35630804, TicksPerSample 123246, ValidSample 502
TimeStamp 45983097, TicksPerSample 123246, ValidSample 346
TimeStamp 1249167475, TicksPerSample 123246, ValidSample 502

StopTime Exec :14/10/2025 17:20:50
CreateHtmlDoc -->> New change
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - Updated
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - Updated
COMMON.PROC.BU.2 - Updated
Rev2Snk - Updated
Rev3ChkdSnk - Updated
TEST.PD.PROT.SNK.3 SinkWaitCapTimer Deadline - Updated
Packet and signal mapping list PD_Merged -> TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline
TEST.PD.PROT.SNK.3 SinkWaitCapTimer Deadline - 0
COMMON.PROC.BU.2 - -1
Packet Index is missing
Signal start or stop time is missing
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - 14
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 28
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - 62
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 73
Rev2Snk - -1
Packet Index is missing
Signal start or stop time is missing
Hard_Reset check - TEST.PD.PROT.SNK.3#1 - 39
Request message check - TEST.PD.PROT.SNK.3#2 - -1
Packet Index is missing
Signal start or stop time is missing
Rev3ChkdSnk - -1
Packet Index is missing
Signal start or stop time is missing
Hard_Reset check - TEST.PD.PROT.SNK.3#1 - 90
Request message check - TEST.PD.PROT.SNK.3#2 - -1
Packet Index is missing
Signal start or stop time is missing
CCline Thread State : (STOP)
LSADC Thread State : (STOP)
HSADC Thread State : (NONE)
QD Thread State : (NONE)

17:20:50     | Test Name(Stop): TEST_PD_PROT_SNK_3_SinkWaitCapTimer_Deadline
---------------------------------------------------------------------------------------------------------
10 /14/2025 05:20:50.336  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:20:50.499  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:20:50.671  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:20:50.685  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:20:50.699  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:20:50.714  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:20:50.729  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:20:50.744  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:20:50.758  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:20:50.773  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:20:50.787  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:20:50.802  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:20:50.816  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:20:50.831  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:20:50.845  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:20:50.860  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:20:51.028  Write Ethernet :FW Write:0x6F, 0x02,  , API description - Setting Controller Configuaton :RA_CC2
10 /14/2025 05:20:51.190  Write Ethernet :FW Write:0x16, 0x00, 0x80, 0x01,  , API description - Set revision number
10 /14/2025 05:20:51.204  Write Ethernet :FW Write:0x16, 0x02, 0x20, 0x01,  , API description - Set VDM revision number
10 /14/2025 05:20:51.219  Write Ethernet :FW Write:0x3E, 0x00,  , API description - Initiate DR_Swap
10 /14/2025 05:20:51.284  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:20:51.298  Write Ethernet :FW Write:0x3F, 0x00, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:20:51.313  Write Ethernet :FW Write:0x16, 0x0C, 0x05, 0x00, 0x0B, 0x00, 0x00, 0x80, 0x00, 0x00, 
10 /14/2025 05:20:51.328  Write Ethernet :FW Write:0x54,  , API description - Setting Controller Configuaton :VDM_DiscovIdAck_All_SOP
10 /14/2025 05:20:51.489  Write Ethernet :FW Write:0x16, 0x01, 0x00, 0x01,  , API description - Enable unchunked message support
10 /14/2025 05:20:51.504  Write Ethernet :FW Write:0x5E, 0xC1, 0x3D, 0x00, 0x0A, 
10 /14/2025 05:20:51.519  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:20:51.534  Write Ethernet :FW Write:0x3E, 0x02,  , API description - Initiate DR_Swap
10 /14/2025 05:20:51.612  Write Ethernet :FW Write:0x65, 0x00, 0x82, 0x00, 0x00, 0x00,  , API description - initiate PR_Swap
10 /14/2025 05:20:51.626  Write Ethernet :FW Write:0x3F, 0x02, 0x00, 0x00,  , API description - SendVCONNSwap
10 /14/2025 05:20:51.640  Write Ethernet :FW Write:0x18, 0x00,  , API description - Setting Controller Configuaton :SimulateDetach
10 /14/2025 05:20:51.799  Write Ethernet :FW Write:0x18, 0x09,  , API description - Setting Controller Configuaton :SimulateDetach_CC1_CC2
10 /14/2025 05:20:51.954  Write Ethernet :FW Write:0x0E,  , API description - Setting Controller Configuaton :PHY_RESET
ResetDataManager - End of Reset all RTDataChunk

---------------------------------------------------------------------------------------------------------
17:20:52 Test Name(Start): TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout
Tester cable drop compensation : False
10 /14/2025 05:20:52.132  Write Ethernet :FW Write:0x16, 0x21, 0x07, 0x00, 0x00, 0x00, 0x00, 0x01, 
DataStreamerSertvice -->>StartStreamer()-->> SubSampleRatio -->>500
Reset board API start
10 /14/2025 05:20:52.146  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:52.172  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:52.186  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x10,  , API description - Enable LSADC
10 /14/2025 05:20:52.201  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:52.215  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:52.229  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:20:52.244  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x00,  , API description - Reset DMA :DMA0_CCLinePortA
10 /14/2025 05:20:52.261  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x01,  , API description - Reset DMA :DMA1_CCLinePortB
10 /14/2025 05:20:52.276  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x02,  , API description - Reset DMA :DMA2_LSADC_Port_A_B
10 /14/2025 05:20:52.291  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:20:52.409  Write Ethernet :FW Write:0xFE, 0x01, 0x00, 0x03,  , API description - Reset DMA :DMA3_HSADC_AND_LSADC_QD
10 /14/2025 05:20:52.424  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:52.439  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x02,  , API description - CC line timer reset
10 /14/2025 05:20:52.453  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x14, 0x01, 0x00, 0x01,  , API description - CC line timer reset
10 /14/2025 05:20:52.468  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:20:52.482  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:52.497  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
ResetDataManager - End of Reset all RTDataChunk
10 /14/2025 05:20:52.550  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x40, 0x02, 0x00, 0x00, 0x00, 0x00,  , API description - Configure LSADC Sub Sampling
###LSADC channel debug
Without adding dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

With dummy channels
Dp Dn count : 0
Port A channel count : 6
PORTA_CC1_VOLTAGE - 5
PORTA_CC1_CURRENT - 2
PORTA_CC2_VOLTAGE - 4
PORTA_CC2_CURRENT - 1
PORTA_VBUS_VOLTAGE - 3
PORTA_VBUS_CURRENT - 0
Port B channel count : 0

10 /14/2025 05:20:52.565  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x04, 0x02, 0x00, 0x00, 0x15, 0x33, 0x00, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:20:52.579  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x08, 0x02, 0x00, 0x00, 0x88, 0xC6, 0x02, 0x0D,  , API description - Configure Port A Channels
10 /14/2025 05:20:52.594  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x0C, 0x02, 0x00, 0x00, 0x88, 0x00, 0x00, 0x0A,  , API description - Configure Port A Channels
10 /14/2025 05:20:52.608  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x20, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.622  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x24, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.637  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x28, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.652  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x2C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.666  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x30, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.681  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x34, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.695  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x38, 0x02, 0x00, 0x00, 0xF4, 0x01, 0xF4, 0x01,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.710  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x3C, 0x02, 0x00, 0x00, 0xF4, 0x01, 0x00, 0x00,  , API description - Set Sub Sampling Ration for Channel
10 /14/2025 05:20:52.724  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x10, 0x02, 0x00, 0x00, 0xFB, 0x00, 0x00, 0xF0,  , API description - Time stamp configuration
10 /14/2025 05:20:52.738  Write Ethernet :FW Write:0xFE, 0x81, 0x02, 0x18, 0x02, 0x00, 0x00, 0x09,  , API description - Enable LSADC
10 /14/2025 05:20:52.753  Write Ethernet :FW Write:0x6B, 0x01, 0x23, 0x04, 0x06, 0x02, 0xFF, 0xFF,  , API description - Switch LSADC Ch8 Path
10 /14/2025 05:20:52.782 Read Ethernet :FW Read:0xFE, 0x00, 0x05, 0xE4, 0x02, 0x00, 0x00, 
C2Lib: StartStreamer(): 17_17_20_52_783
10 /14/2025 05:20:52.783  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x05,  , API description - CcLine Packet Streaming Start/Stop
10 /14/2025 05:20:52.818  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x01,  , API description -  CCLine Packet Streaming Configuration
17_17_20_52_833: WorkerThreadLSADC start
17_17_20_52_833: WorkerThread_CCline start
Present Test case TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout EPR Flag Status False and enableForNonTestCases False
Consolidate message group
0 -> 0x16, 0x24, 0x15, 0x01, 0x00,  PDM Mode setting RxTimer:50 and TxTimer:50
1 -> 0x16, 0x35, 0x00, 0x50, 0x00, 0x00, 0x01,  Start PDM test case 80 RxTimer:100 and TxTimer:100
10 /14/2025 05:20:52.834  Write Ethernet :FW Write:0x16, 0x24, 0x0B, 0x01, 0x00, 0x00, 0x00,  , API description - Enable/Disable Configure
Configured message: 0->PDM Mode setting
Configured message: 1->Start PDM test case 80
10 /14/2025 05:20:52.849  Write Ethernet :FW Write:0x6E, 0x1E, 0x00, 0x00, 0x02, 0x00, 0x00, 0x0C, 0x00, 0x04, 0x00, 0x32, 0x00, 0x32, 0x00, 0x00, 0x16, 0x24, 0x15, 0x01, 0x00, 0x0E, 0x00, 0x04, 0x00, 0x64, 0x00, 0x64, 0x00, 0x00, 0x16, 0x35, 0x00, 0x50, 0x00, 0x00, 0x01,  , API description - Group Configuration Command
10 /14/2025 05:20:52.864  Write Ethernet :FW Write:0x70,  , API description - Setting Controller Configuaton :Init_Configuration
PD merged: Start of group command configuration 10 /14/2025 05:20:53.036 
10 /14/2025 05:20:54.051 Read Ethernet :FW Read:0xFC, 0x00, 0xE1, 0x06, 0x00, 0x00, 0x00, 0x00, 
PD merged: End of group command configuration 10 /14/2025 05:20:54.051 
Start : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:20:55 
Read_All_Packets_Dynamic_Delay StAssertion Found :1168568057-->> 14/10/2025 17:21:04 
 LastADCTimeStamp before ADCRead 1156565803
 LastADCTimeStamp before ADCRead 1269952451
Stop : Read_All_Packets_Dynamic_Delay -->> 14/10/2025 17:21:05 
DUT Behaviour -- Index: 14, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
DUT Behaviour -- Index: 53, ROLE: EprModeExit DataRole_DUT: UFP IsVconnSource: False PowerRole_DUT: Sink
AMS_Gen#### GC for last valid AMS ele missing
AMS merge Bef
AMS merge Aft
DUT role after Swap or PDC
14 Pow:Sink Dat:UFP Vconn Src:False
53 Pow:Sink Dat:UFP Vconn Src:False

TEST_PD_PROT_SNK_4_SinkWaitCapTimer_TimeoutExpected TestCondition:Rev2Snk and Configured TestCondition:Rev2Snk
TEST_PD_PROT_SNK_4_SinkWaitCapTimer_TimeoutExpected TestCondition:Rev3ChkdSnk and Configured TestCondition:Rev3ChkdSnk
Test conditions
StInd:6 StAMS:0 AftStInd:34 AftAMS:1 SpInd:43 SpAMS:1
StInd:44 StAMS:2 AftStInd:75 AftAMS:3 SpInd:85 SpAMS:4
SNK_4: vSafe5V min start time:3,489768
SNK_4: vSafe5V min start time:9,520246
#PD merged debug desc: Start of common field check validation : 17:21:05.5667341
Pkt Index: 37 skipped in Common_Check_PD_5_Check_Unexpected_Messages_And_Signals. HR/CR: False, SR: False, GC Not Exp: False, Not PDC AMS: False,PDC Reject:False, Skip AMS:NONE, Skip MsgTy:Hard_Reset PDO Ele:
Pkt Index: 78 skipped in Common_Check_PD_5_Check_Unexpected_Messages_And_Signals. HR/CR: False, SR: False, GC Not Exp: False, Not PDC AMS: False,PDC Reject:False, Skip AMS:NONE, Skip MsgTy:Hard_Reset PDO Ele:
StartTime :1,16834203, StopTime :1,16827723ObtainedTime :0,064800000000087
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :1,17468447, StopTime :1,17461966ObtainedTime :0,0648100000000262
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :1,49543209, StopTime :1,49536709ObtainedTime :0,0649999999999817
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :7,17333465, StopTime :7,17326985ObtainedTime :0,0647999999996429
Obtained time difference is 0,065ms, Expected time limit 0,025ms to 0,195ms
StartTime :7,1811967, StopTime :7,1811419ObtainedTime :0,0548000000000215
Obtained time difference is 0,055ms, Expected time limit 0,025ms to 0,195ms
StartTime :7,50420013, StopTime :7,50414213ObtainedTime :0,0580000000001135
Obtained time difference is 0,058ms, Expected time limit 0,025ms to 0,195ms
Time Difference of GoodCRC of SourceCap and Request is 4,08621000000009ms at AMS Index : 0
Time Difference of GoodCRC of SourceCap and Request is 4,08623999999946ms at AMS Index : 2
4 - NONE - NOT_VERIFIED
Skipped: Power_Negotiation Index: 2
Skipped: Hard_Reset Index: 3
Validated: 0 packets
No Discover ID in TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout test case
Validated: 0 VCONN_Swap packets
Validated: 0 packets
#PD merged debug desc: Stop of common field check validation : 17:21:05.5676377
###Test condition validation: Assert count is not integrated
#PD Merged: Critical error - BU test result count is 1, Test case validation count 2
Read_All_Packets_Dynamic_Delay StAssertion Found :1168568057-->> 14/10/2025 17:21:05 
 LastADCTimeStamp before ADCRead 1269952451
 LastADCTimeStamp before ADCRead 1269952451
StreamStSpData_CC First Message StTime0,43165424 , SpTime0,43165424
StreamStSpData_CC Last Message StTime11,68568057 , SpTime11,68568057
StreamStSpData_LA
TimeStamp 25582111, TicksPerSample 123246, ValidSample 0
TimeStamp 53267643, TicksPerSample 123246, ValidSample 502
TimeStamp 63497357, TicksPerSample 123246, ValidSample 502
TimeStamp 1269952451, TicksPerSample 123246, ValidSample 502

10 /14/2025 05:21:05.567  Write Ethernet :FW Write:0xFE, 0x01, 0x06, 0x00,  , API description -  CCLine Packet Streaming Configuration
10 /14/2025 05:21:10.590 :InteruptLasdcRead triggered
17_17_21_10_739: WorkerThread_CCline end
17_17_21_10_850: WorkerThreadLSADC end
InteruptLasdcRead:  m_LSADCthread: thread Aborted()
InteruptLasdcRead:  m_CClinethread: thread Aborted()
10 /14/2025 05:21:10.913  Write Ethernet :FW Write:0xFE, 0x01, 0x02, 0x90, 0x00, 0x00, 0x00, 0x00,  , API description - CcLine Packet Streaming Start/Stop
StopStreamer:  m_LSADCthread: thread Aborted()
StopStreamer:  m_CClinethread: thread Aborted()
StreamStSpData_LA
TimeStamp 25582111, TicksPerSample 123246, ValidSample 0
TimeStamp 53267643, TicksPerSample 123246, ValidSample 502
TimeStamp 63497357, TicksPerSample 123246, ValidSample 502
TimeStamp 1445208469, TicksPerSample 123246, ValidSample 502

StopTime Exec :14/10/2025 17:21:11
CreateHtmlDoc -->> New change
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - Updated
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - Updated
COMMON.PROC.BU.2 - Updated
Rev2Snk - Updated
Rev3ChkdSnk - Updated
TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout - Updated
Packet and signal mapping list PD_Merged -> TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout
TEST.PD.PROT.SNK.4 SinkWaitCapTimer Timeout - 0
COMMON.PROC.BU.2 - -1
Packet Index is missing
Signal start or stop time is missing
COMMON.PROC.BU.2 - REVISION_2_0 Rev2Snk - 14
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 28
COMMON.PROC.BU.2 - REVISION_3_0 Rev3ChkdSnk - 53
UUT should respond with request -  - COMMON.PROC.BU.2#1 - 64
Rev2Snk - -1
Packet Index is missing
Signal start or stop time is missing
SinkWaitCapTimer Timeout - TEST.PD.PROT.SNK.4#1 - -1
Packet Index is missing
Signal start or stop time is missing
Rev3ChkdSnk - -1
Packet Index is missing
Signal start or stop time is missing
SinkWaitCapTimer Timeout - TEST.PD.PROT.SNK.4#1 - -1
Packet Index is missing
Signal start or stop time is missing
CCline Thread State : (STOP)
LSADC Thread State : (STOP)
HSADC Thread State : (NONE)
QD Thread State : (NONE)

17:21:11     | Test Name(Stop): TEST_PD_PROT_SNK_4_SinkWaitCapTimer_Timeout
---------------------------------------------------------------------------------------------------------
10 /14/2025 05:21:11.265  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:21:11.430  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:21:11.601  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:21:11.615  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:21:11.629  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:21:11.644  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:21:11.658  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:21:11.673  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:21:11.688  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:21:11.702  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:21:11.716  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:21:11.731  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:21:11.746  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:21:11.760  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:21:11.775  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
AddTest - test result is null
10 /14/2025 05:21:11.790  Write Ethernet :FW Write:0x36, 0x00, 0x00, 0x01,  , API description - Setting Controller Configuaton :FW_FPGA_FullReset
10 /14/2025 05:21:11.963  Write Ethernet :FW Write:0x60, 0x01,  , API description - Setting Controller Configuaton :Enable_GoodCRC
10 /14/2025 05:21:12.135  Write Ethernet :FW Write:0x5A, 0x00, 0x00, 0x00, 0x00,  , API description - Disable tester packet
10 /14/2025 05:21:12.149  Write Ethernet :FW Write:0x16, 0x24, 0x09, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Packet not to send count
10 /14/2025 05:21:12.164  Write Ethernet :FW Write:0x16, 0x05, 0x00, 0x00, 0x00, 0x00,  , API description - PPS_Auto_Request_Enable
10 /14/2025 05:21:12.179  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x03, 0x00, 0x00, 0x00, 0x80,  , API description - Configure packet delay
10 /14/2025 05:21:12.194  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x42, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:21:12.209  Write Ethernet :FW Write:0x16, 0x24, 0x07, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - Configure to send packet until message ID becomes zero
10 /14/2025 05:21:12.224  Write Ethernet :FW Write:0x60, 0x06, 0x06,  , API description - Enable/Disable Configure
10 /14/2025 05:21:12.239  Write Ethernet :FW Write:0x16, 0x0C, 0x0A, 0x00, 0x00, 
10 /14/2025 05:21:12.253  Write Ethernet :FW Write:0x16, 0x25, 0x03, 0x00,  , API description - FR_Swap AMS goodCRC
10 /14/2025 05:21:12.268  Write Ethernet :FW Write:0x5A, 0x01, 0x00, 0x00, 0x40, 0x00,  , API description - Disable tester messages
10 /14/2025 05:21:12.282  Write Ethernet :FW Write:0x60, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00,  , API description - DisableGoodCRC_IndivdualPDMessage
10 /14/2025 05:21:12.297  Write Ethernet :FW Write:0x60, 0x07,  , API description - Reset All GCRC Delay/Disable Feature
10 /14/2025 05:21:12.312  Write Ethernet :FW Write:0x16, 0x0C, 0x04, 0x08, 0x00, 0x00, 0x00, 0x00,  , API description - Configure packet delay
10 /14/2025 05:21:13.327  Write Ethernet :FW Write:0x16, 0x24, 0x15, 0x00, 0x00,  , API description - PDM Mode setting
StopTime Exec :14/10/2025 17:21:14
CreateHtmlDoc -->> New change
CreateHtmlDoc -->> New change
<--TesterInfoStore--> 
GRL_USB_PD_Controller_Serial_No - Value : 397.409.397.077.376.
GRL_USB_PD_Software_Version - Value : 1.6.28.0
GRL_USB_PD_Firmware_Version - Value : 2.2.65
GRL USB-PD Ethernet Buffer Size - Value : 62K
GRL USB-PD Eload Firmware Version - Value : 9.8 / 9.8
Calibration - Value : Calibration Success
RX mask Power selection - Value : Neutral Power
Device_Type - Value : Consumer Only
Cable Type - Value : GRL_SPL_CABLE_1
Impedance (milli ohm) - Value : 0
PD_Merged CTS Version - Value : v.Q4-2024
USB_PD_Spec Version - Value : Rev3.2 Ver1.1RC2
USB_Type_C_Spec Version - Value : v2.3 Oct-2023
VIF_File_Name - Value : Parrot__MPPUA2__1__0_14_10_2025.xml
Noise Pattern Generation: - Value : Two-Tone Noise
Application mode - Value : Informational
Disabled all Pop-up during test execution - Value : False
Pop-up Timer - Value : 0
Rerun Enabled - Value : False
Rerun Count - Value : 1
Rerun Iteration - Value : 0
UI Live Update - Value : False
<--MOIsInfoStore--> 
Connect EPR Test Fixture - Value : False
FR_Swap AUTO Box Connected - Value : False
StopTime Exec :14/10/2025 17:21:14
CreateHtmlDoc -->> New change
