Rohde & Schwarz
EMI Measurement Test Report
Device Under Test	<click here and enter dut description>
Operating Conditions	<click here and enter temperature, humidity, etc.>
Operator Name	<click here and enter your name>
Test Specification	
Comment	<click here and enter additional information>

Scan Settings ( 1 Range )

Frequencies	Receiver Settings	
Start	Stop	Step	Res BW	M-Time	Atten	Preamp	
30 MHz	1 GHz	40 kHz	120 kHz (6dB)	2 ms	Auto	On	

Previous Measurement

	Detector:	PK+       	Meas Time:	see scan settings 
	Peaks:	20	Acc. Margin:	40 dB

Pre-measurement Graph

Peak Search Results

Trace	Frequency	Level	Limit	Delta Limit	Delta Ref	Comment	
	(MHz)	( dBμV/m)	( dBμV/m)	(dB)	(dB)		
1 PK+	35.04	49.71 *	40.00	9.71			
1 PK+	42.2	55.13 *	40.00	15.13			
1 PK+	44.12	55.25 *	40.00	15.25			
1 PK+	57.68	49.47 *	40.00	9.47			
1 PK+	69.76	48.53 *	40.00	8.53			
1 PK+	84.08	47.15 *	40.00	7.15			
1 PK+	98.0	52.15 *	40.00	12.15			
1 PK+	102.44	52.00 *	40.00	12.00			
1 PK+	143.96	44.33 *	40.00	4.33			
1 PK+	167.08	48.17 *	40.00	8.17			
1 PK+	194.2	52.28 *	40.00	12.28			
1 PK+	221.44	46.24 *	40.00	6.24			
1 PK+	248.72	41.78	47.00	-5.22			
1 PK+	312.36	39.42	47.00	-7.58			
1 PK+	354.92	30.60	47.00	-16.40			
1 PK+	448.8	35.47	47.00	-11.53			
1 PK+	506.52	36.18	47.00	-10.82			
1 PK+	612.76	27.06	47.00	-19.94			
1 PK+	745.28	22.69	47.00	-24.31			
1 PK+	993.8	25.82	47.00	-21.18			

* = limit exceeded