("FILE_TYPE"	"PMAP File"
    ("devices"
        ("K_Linear")
        ("L"
            ("info"
                ("spice_dsg"	"L")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("TERM_IA"	"-1")
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"IND")
                )
                ("max_ops"
                    ("LI"	"CURRENT")
                    ("LV"	"DIELECTRIC")
                )
                ("smoke_tests"
                    ("LI"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_IA")
                    )
                    ("LV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                )
                ("device_max_ops")
            )
        )
        ("R"
            ("info"
                ("spice_dsg"	"R")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("TC1"
                        ("value"	"0")
                    )
                    ("TC2"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"RES")
                )
                ("max_ops"
                    ("RV"	"VOLTAGE")
                    ("PDM"	"POWER")
                    ("SLP"	"SLOPE")
                    ("RBA"	"1/SLP")
                    ("TMAX"	"MAX_TEMP")
                    ("TB"	"TMAX")
                    ("RTKNEE"	"TKNEE")
                    ("RTRISE"	"TRISE")
                )
                ("smoke_tests"
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("RV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("TB"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops")
            )
        )
        ("C"
            ("info"
                ("spice_dsg"	"C")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("IC"
                        ("value"	"0")
                    )
                    ("TC"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("TERM_A"	"-1")
                    ("DERATE_TYPE"	"CAP")
                )
                ("max_ops"
                    ("CV"	"VOLTAGE")
                    ("CI"	"CURRENT")
                    ("SLP"	"SLOPE")
                    ("TBRK"	"KNEE")
                    ("TMAX"	"MAX_TEMP")
                )
                ("smoke_tests"
                    ("CV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("CI"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_A")
                    )
                )
                ("device_max_ops")
            )
        )
        ("NAMS20")
        ("MUR10005CT"
            ("info"
                ("spice_dsg"	"X")
            )
            ("model_params"
                ("level_0"
                    ("IS"
                        ("value"	"0.1f")
                    )
                    ("RS"
                        ("value"	"0")
                    )
                    ("N"
                        ("value"	"0")
                    )
                    ("TT"
                        ("value"	"0")
                    )
                    ("CJO"
                        ("value"	"0")
                    )
                    ("VJ"
                        ("value"	"0")
                    )
                    ("M"
                        ("value"	"0")
                    )
                    ("EG"
                        ("value"	"1.11")
                    )
                    ("XTI"
                        ("value"	"3")
                    )
                    ("KF"
                        ("value"	"0")
                    )
                    ("AF"
                        ("value"	"1")
                    )
                    ("FC"
                        ("value"	"0")
                    )
                    ("BV"
                        ("value"	"100")
                    )
                    ("IBV"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("max_ops_desc"
                    ("IF1"
                        ("description"	"Max forward current of Diode1")
                        ("unit"	"A")
                    )
                    ("IF2"
                        ("description"	"Max forward current of Diode2")
                        ("unit"	"A")
                    )
                    ("VR1"
                        ("description"	"Peak reverse voltage of Diode1 ")
                        ("unit"	"V")
                    )
                    ("VR2"
                        ("description"	"Peak reverse voltage of Diode2")
                        ("unit"	"V")
                    )
                    ("PDM"
                        ("description"	"Max pwr dissipation")
                        ("unit"	"W")
                    )
                    ("TJ"
                        ("description"	"Max junction temp")
                        ("unit"	"C")
                    )
                    ("RJC"
                        ("description"	"J-C thermal resist")
                        ("unit"	"C/W")
                    )
                    ("RCA"
                        ("description"	"C-A thermal resist")
                        ("unit"	"C/W")
                    )
                )
                ("pre_smoke"
                    ("TERM_AC1"	"-1")
                    ("TERM_AC2"	"-3")
                    ("NODE_AC1"	"AC1")
                    ("NODE_AC2"	"AC2")
                    ("NODE_DC"	"DC")
                    ("DERATE_TYPE"	"DIODE_BRIDGE")
                )
                ("max_ops"
                    ("RCA"	"RCA")
                )
                ("smoke_tests"
                    ("IF1"
                        ("test"	"current_test")
                        ("term"	"TERM_AC1")
                    )
                    ("IF2"
                        ("test"	"current_test")
                        ("term"	"TERM_AC2")
                    )
                    ("VR1"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_DC")
                            ("NODE_AC1")
                        )
                    )
                    ("VR2"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_DC")
                            ("NODE_AC2")
                        )
                    )
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("TJ"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops"
                    ("IF1"	"100")
                    ("IF2"	"100")
                    ("IFM"	"200")
                    ("VR1"	"50")
                    ("VR2"	"50")
                    ("PDM"	"76")
                    ("TJ"	"175")
                    ("RJC"	"1")
                )
                ("device_pre_smoke"
                    ("TERM_AC1"	"1")
                    ("TERM_AC2"	"2")
                    ("NODE_AC1"	"1")
                    ("NODE_AC2"	"2")
                    ("NODE_DC"	"3")
                    ("DERATE_TYPE"	"DIODE_BRIDGE")
                )
            )
        )
        ("D1D2C1"
            ("info"
                ("spice_dsg"	"X")
            )
            ("model_params"
                ("level_0"
                    ("IS"
                        ("value"	"0.1f")
                    )
                    ("RS"
                        ("value"	"0")
                    )
                    ("N"
                        ("value"	"0")
                    )
                    ("TT"
                        ("value"	"0")
                    )
                    ("CJO"
                        ("value"	"0")
                    )
                    ("VJ"
                        ("value"	"0")
                    )
                    ("M"
                        ("value"	"0")
                    )
                    ("EG"
                        ("value"	"1.11")
                    )
                    ("XTI"
                        ("value"	"3")
                    )
                    ("KF"
                        ("value"	"0")
                    )
                    ("AF"
                        ("value"	"1")
                    )
                    ("FC"
                        ("value"	"0")
                    )
                    ("BV"
                        ("value"	"100")
                    )
                    ("IBV"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("max_ops_desc"
                    ("IF1"
                        ("description"	"Max forward current of Diode1")
                        ("unit"	"A")
                    )
                    ("IF2"
                        ("description"	"Max forward current of Diode2")
                        ("unit"	"A")
                    )
                    ("VR1"
                        ("description"	"Peak reverse voltage of Diode1 ")
                        ("unit"	"V")
                    )
                    ("VR2"
                        ("description"	"Peak reverse voltage of Diode2")
                        ("unit"	"V")
                    )
                    ("PDM"
                        ("description"	"Max pwr dissipation")
                        ("unit"	"W")
                    )
                    ("TJ"
                        ("description"	"Max junction temp")
                        ("unit"	"C")
                    )
                    ("RJC"
                        ("description"	"J-C thermal resist")
                        ("unit"	"C/W")
                    )
                    ("RCA"
                        ("description"	"C-A thermal resist")
                        ("unit"	"C/W")
                    )
                )
                ("pre_smoke"
                    ("TERM_AC1"	"-1")
                    ("TERM_AC2"	"-3")
                    ("NODE_AC1"	"AC1")
                    ("NODE_AC2"	"AC2")
                    ("NODE_DC"	"DC")
                    ("DERATE_TYPE"	"DIODE_BRIDGE")
                )
                ("max_ops"
                    ("RCA"	"RCA")
                )
                ("smoke_tests"
                    ("IF1"
                        ("test"	"current_test")
                        ("term"	"TERM_AC1")
                    )
                    ("IF2"
                        ("test"	"current_test")
                        ("term"	"TERM_AC2")
                    )
                    ("VR1"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_DC")
                            ("NODE_AC1")
                        )
                    )
                    ("VR2"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_DC")
                            ("NODE_AC2")
                        )
                    )
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("TJ"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops"
                    ("IF1"	"2")
                    ("IF2"	"2")
                    ("VR1"	"200")
                    ("VR2"	"200")
                    ("TJ"	"150")
                )
                ("device_pre_smoke"
                    ("TERM_AC1"	"1")
                    ("TERM_AC2"	"2")
                    ("NODE_AC1"	"1")
                    ("NODE_AC2"	"2")
                    ("NODE_DC"	"3")
                    ("DERATE_TYPE"	"DIODE_BRIDGE")
                )
            )
        )
        ("VPULSE")
        ("UCC28600_0")
    )
    ("instances"
        ("K2"
            ("device_name"	"K_Linear")
            ("pspice_path"	"Kn_K2")
            ("level"	"0")
            ("model_params"
                ("L2"
                    ("value"	"L2")
                    ("pspice_param"	"L2")
                )
                ("COUPLING"
                    ("value"	"0.99")
                    ("pspice_param"	"COUPLING")
                )
                ("L1"
                    ("value"	"L1")
                    ("pspice_param"	"L1")
                )
                ("L3"
                    ("value"	"L3")
                    ("pspice_param"	"L3")
                )
                ("L4"
                    ("value"	"")
                    ("pspice_param"	"L4")
                )
                ("L5"
                    ("value"	"")
                    ("pspice_param"	"L5")
                )
                ("L6"
                    ("value"	"")
                    ("pspice_param"	"L6")
                )
            )
        )
        ("L1"
            ("device_name"	"L")
            ("pspice_path"	"L_L1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"126uH")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("IL2"
                    ("value"	"0")
                    ("pspice_param"	"IL2")
                )
                ("IL1"
                    ("value"	"0")
                    ("pspice_param"	"IL1")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
            ("smoke_vars"
                ("CURRENT"	"5.0")
                ("DIELECTRIC"	"300.0")
            )
        )
        ("L2"
            ("device_name"	"L")
            ("pspice_path"	"L_L2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10uH")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("IL2"
                    ("value"	"0")
                    ("pspice_param"	"IL2")
                )
                ("IL1"
                    ("value"	"0")
                    ("pspice_param"	"IL1")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
            ("smoke_vars"
                ("CURRENT"	"5.0")
                ("DIELECTRIC"	"300.0")
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.1")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"7.891KW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("L3"
            ("device_name"	"L")
            ("pspice_path"	"L_L3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10uH")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"78.97e-30W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("IL2"
                    ("value"	"0")
                    ("pspice_param"	"IL2")
                )
                ("IL1"
                    ("value"	"0")
                    ("pspice_param"	"IL1")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
            ("smoke_vars"
                ("CURRENT"	"5.0")
                ("DIELECTRIC"	"300.0")
            )
        )
        ("C_bulk"
            ("device_name"	"C")
            ("pspice_path"	"C_C_bulk")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"222uH")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("M1"
            ("device_name"	"NAMS20")
            ("pspice_path"	"X_M1")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"13.75KW")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("Rcs"
            ("device_name"	"R")
            ("pspice_path"	"R_Rcs")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.153")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"12.07KW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("Rvdd"
            ("device_name"	"R")
            ("pspice_path"	"R_Rvdd")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4.20")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"265.8pW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("Cbias"
            ("device_name"	"C")
            ("pspice_path"	"C_Cbias")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1n")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("Rsu"
            ("device_name"	"R")
            ("pspice_path"	"R_Rsu")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"3.6k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"227.8nW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("Cvdd"
            ("device_name"	"C")
            ("pspice_path"	"C_Cvdd")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"3.8u")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("Rovp1"
            ("device_name"	"R")
            ("pspice_path"	"R_Rovp1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"97k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("Rovp2"
            ("device_name"	"R")
            ("pspice_path"	"R_Rovp2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"32k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("Rpl"
            ("device_name"	"R")
            ("pspice_path"	"R_Rpl")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1.8k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"3.331pW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"7.6k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"4.205uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("C1"
            ("device_name"	"C")
            ("pspice_path"	"C_C1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1.3n")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("C2"
            ("device_name"	"C")
            ("pspice_path"	"C_C2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100n")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("D5"
            ("device_name"	"MUR10005CT")
            ("pspice_path"	"X_D5")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("CSS"
            ("device_name"	"C")
            ("pspice_path"	"C_CSS")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"5.5n")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("Cout"
            ("device_name"	"C")
            ("pspice_path"	"C_Cout")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"677u")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("Rout"
            ("device_name"	"R")
            ("pspice_path"	"R_Rout")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"200")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1.1m")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("R9"
            ("device_name"	"R")
            ("pspice_path"	"R_R9")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100G")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"235.5pW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("D6"
            ("device_name"	"MUR10005CT")
            ("pspice_path"	"X_D6")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"954.4uW")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("U2"
            ("device_name"	"D1D2C1")
            ("pspice_path"	"X_U2")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"656.5uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"1D2C1")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("R10"
            ("device_name"	"R")
            ("pspice_path"	"R_R10")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100G")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"249.6pW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("V2"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_V2")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"-33.71KW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"100m")
                    ("pspice_param"	"PER")
                )
                ("TF"
                    ("value"	"0")
                    ("pspice_param"	"TF")
                )
                ("TD"
                    ("value"	"0")
                    ("pspice_param"	"TD")
                )
                ("V1"
                    ("value"	"120")
                    ("pspice_param"	"V1")
                )
                ("V2"
                    ("value"	"300")
                    ("pspice_param"	"V2")
                )
                ("TR"
                    ("value"	"100m")
                    ("pspice_param"	"TR")
                )
                ("PW"
                    ("value"	"0")
                    ("pspice_param"	"PW")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("U4"
            ("device_name"	"UCC28600_0")
            ("pspice_path"	"X_U4")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"1.848uW")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
    )
)
