("FILE_TYPE"	"PMAP File"
    ("devices"
        ("R")
        ("CESR_0")
        ("C")
        ("VSIN")
        ("LM61460AFS-Q1RJR_TRANS")
        ("LDCR_0")
        ("VPULSE")
        ("Param")
    )
    ("instances"
        ("R4"
            ("device_name"	"R")
            ("pspice_path"	"R_R4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"249.8uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("R5"
            ("device_name"	"R")
            ("pspice_path"	"R_R5")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("C6"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C6")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"22u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C3"
            ("device_name"	"C")
            ("pspice_path"	"C_C3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.022u")
                    ("pspice_param"	"VALUE")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
            )
        )
        ("C4"
            ("device_name"	"C")
            ("pspice_path"	"C_C4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4.7u")
                    ("pspice_param"	"VALUE")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
            )
        )
        ("V6"
            ("device_name"	"VSIN")
            ("pspice_path"	"V_V6")
            ("level"	"0")
            ("model_params"
                ("AC"
                    ("value"	"0")
                    ("pspice_param"	"AC")
                )
                ("VAMPL"
                    ("value"	"30mv")
                    ("pspice_param"	"VAMPL")
                )
                ("VOFF"
                    ("value"	"0")
                    ("pspice_param"	"VOFF")
                )
                ("FREQ"
                    ("value"	"{freq}")
                    ("pspice_param"	"FREQ")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PHASE"
                    ("value"	"0")
                    ("pspice_param"	"PHASE")
                )
                ("DF"
                    ("value"	"0")
                    ("pspice_param"	"DF")
                )
                ("TD"
                    ("value"	"0")
                    ("pspice_param"	"TD")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("PSpice Model Type"
                    ("value"	"0011")
                    ("pspice_param"	"PSpice Model Type")
                )
            )
        )
        ("C5"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C5")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"1u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("U1"
            ("device_name"	"LM61460AFS-Q1RJR_TRANS")
            ("pspice_path"	"X_U1")
            ("level"	"0")
            ("model_params"
                ("STEADY_STATE"
                    ("value"	"{Steady_state}")
                    ("pspice_param"	"STEADY_STATE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PackageName"
                    ("value"	"LM61460AFSQRJRTQ")
                    ("pspice_param"	"PackageName")
                )
                ("IsHeterogeneous"
                    ("value"	"False")
                    ("pspice_param"	"IsHeterogeneous")
                )
                ("DevicesInView"
                    ("value"	"1")
                    ("pspice_param"	"DevicesInView")
                )
                ("DevicesInPackage"
                    ("value"	"1")
                    ("pspice_param"	"DevicesInPackage")
                )
                ("DeviceDesignator"
                    ("value"	"A")
                    ("pspice_param"	"DeviceDesignator")
                )
                ("DeviceNumbering"
                    ("value"	"Alpha")
                    ("pspice_param"	"DeviceNumbering")
                )
                ("Manufacturer"
                    ("value"	"Texas Instruments")
                    ("pspice_param"	"Manufacturer")
                )
                ("PartNumber"
                    ("value"	"LM61460AFSQRJRRQ1")
                    ("pspice_param"	"PartNumber")
                )
                ("< Value >"
                    ("value"	"LM61460AFSQRJRTQ")
                    ("pspice_param"	"< Value >")
                )
                ("OriginalSymbolOrigin"
                    ("value"	"(-70000,130000)")
                    ("pspice_param"	"OriginalSymbolOrigin")
                )
            )
        )
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"33.2k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"30.12uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("R7"
            ("device_name"	"R")
            ("pspice_path"	"R_R7")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"245.3uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("C16"
            ("device_name"	"C")
            ("pspice_path"	"C_C16")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"22p")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("R8"
            ("device_name"	"R")
            ("pspice_path"	"R_R8")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"24.9k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"91.04nW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("R9"
            ("device_name"	"R")
            ("pspice_path"	"R_R9")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"2.267uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("C11"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C11")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"22u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C13"
            ("device_name"	"C")
            ("pspice_path"	"C_C13")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.1u")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"{3.3*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C10"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C10")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"22u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C1"
            ("device_name"	"C")
            ("pspice_path"	"C_C1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4.7u")
                    ("pspice_param"	"VALUE")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
            )
        )
        ("RLOAD"
            ("device_name"	"R")
            ("pspice_path"	"R_RLOAD")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{VOUT/IOUT}")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"20.00W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("C9"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C9")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"22u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C8"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C8")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"22u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("R10"
            ("device_name"	"R")
            ("pspice_path"	"R_R10")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"255k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"368.8uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("L1"
            ("device_name"	"LDCR_0")
            ("pspice_path"	"X_L1")
            ("level"	"0")
            ("model_params"
                ("L"
                    ("value"	"4.7u")
                    ("pspice_param"	"L")
                )
                ("DCR"
                    ("value"	"14.3m")
                    ("pspice_param"	"DCR")
                )
                ("IC"
                    ("value"	"{IOUT*Steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"-20.87W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C2"
            ("device_name"	"C")
            ("pspice_path"	"C_C2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.022u")
                    ("pspice_param"	"VALUE")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
            )
        )
        ("C7"
            ("device_name"	"CESR_0")
            ("pspice_path"	"X_C7")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"22u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2m")
                    ("pspice_param"	"ESR")
                )
                ("X"
                    ("value"	"1")
                    ("pspice_param"	"X")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("C14"
            ("device_name"	"C")
            ("pspice_path"	"C_C14")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1u")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"{VOUT*steady_state}")
                    ("pspice_param"	"IC")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
            )
        )
        ("R13"
            ("device_name"	"R")
            ("pspice_path"	"R_R13")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"144.6uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
            )
        )
        ("C15"
            ("device_name"	"C")
            ("pspice_path"	"C_C15")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1u")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"{Steady_state*3.7}")
                    ("pspice_param"	"IC")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("V5"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_V5")
            ("level"	"0")
            ("model_params"
                ("PW"
                    ("value"	"1")
                    ("pspice_param"	"PW")
                )
                ("TR"
                    ("value"	"20n")
                    ("pspice_param"	"TR")
                )
                ("V2"
                    ("value"	"{VIn}")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"{VIn*Steady_state}")
                    ("pspice_param"	"V1")
                )
                ("TD"
                    ("value"	"0")
                    ("pspice_param"	"TD")
                )
                ("TF"
                    ("value"	"1n")
                    ("pspice_param"	"TF")
                )
                ("PER"
                    ("value"	"1")
                    ("pspice_param"	"PER")
                )
                ("BiasValue Power"
                    ("value"	"-698.6uW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("PARAM"
            ("device_name"	"Param")
            ("pspice_path"	"")
            ("level"	"0")
            ("model_params"
                ("iout"
                    ("value"	"4")
                    ("pspice_param"	"iout")
                )
                ("vin"
                    ("value"	"13.5")
                    ("pspice_param"	"vin")
                )
                ("steady_state"
                    ("value"	"1")
                    ("pspice_param"	"steady_state")
                )
                ("vout"
                    ("value"	"5")
                    ("pspice_param"	"vout")
                )
            )
        )
    )
)
