
**** 05/24/18 12:33:58 ****** PSpice 17.2.0 (March 2016) ****** ID# 0 ********

 ** Profile: "SCHEMATIC1-TestePspice"  [ C:\Users\GFonseca\Desktop\WavEC\Estudos e Projectos\Symbiotracker\KiCad Sym Project\teste1-p


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "TestePspice.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "C:/Cadence/SPB_17.2/tools/pspice/library/ti_pspice_models/LM74670-Q1_PSPICE_TRANS/LM74670-Q1_TRANS.LIB" 
.LIB "../../../spicemodels/sllm126/csd17308q3.lib" 
.INC "C:/Cadence/SPB_17.2/tools/pspice/library/ti_pspice_models/LM74670-Q1_PSPICE_TRANS/LM74670-Q1_TRANS-PSpiceFiles/LM74670-Q1_Tra"
+ "ns/trans.sim" 
* From [PSPICE NETLIST] section of C:\SPB_Data\cdssetup\OrCAD_PSpice\17.2.0\PSpice.ini file:

**** INCLUDING trans.sim ****
@OrCAD Simulation Server Version: 1.0
----------------------------------$
ERROR(ORPSIM-16015): Unknown parameter.

@Settings: 0 1
--------------$
ERROR -- Missing node
@General:
---------$
ERROR -- Missing node
ProfileName= "trans" 
$
ERROR(ORPSIM-16316): Invalid device
ProfileFile= "trans.sim" 
$
ERROR(ORPSIM-16316): Invalid device
Connectivity= "LM74670-Q1_Trans.net" 
-------------------------------------$
ERROR -- Missing node
NetlistFile= "trans.cir" 
-------------------------$
ERROR -- Missing node
DataFile= "trans.dat" 
----------------------$
ERROR -- Missing node
OutFile= "trans.out" 
---------------------$
ERROR -- Missing node
Notes=
------$
ERROR -- Missing node
@#$BEGINNOTES
--$
ERROR(ORPSIM-16316): Invalid device
@#$ENDNOTES
--$
ERROR(ORPSIM-16316): Invalid device
@End General
------------$
ERROR -- Missing node
@Analysis: 0 1
-$
ERROR(ORPSIM-16316): Invalid device
+0 0 0 0 
+0 "10" 
+1 "" 
+2 "0" 
+3 "100u" 
+4 "" 
+5 "" 
+6 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 1 0
-$
ERROR(ORPSIM-16316): Invalid device
+2 0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 2 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 3 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 0 0
+0 "" 
+1 "" 
+2 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 4 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 0 1 0 0 0 0 0 0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
LoadFile 0 "" 
--------------$
ERROR(ORPSIM-16407): Missing model
SaveFile 0 "" 
--------------$
ERROR -- Missing node
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 5 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 6 0
-$
ERROR(ORPSIM-16316): Invalid device
+1 
+0 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 7 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 8 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 9 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 10 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 11 1
-$
ERROR(ORPSIM-16316): Invalid device
+ 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 
+ ABSTOL "10n"
+ ITL4 "20"
+ RELTOL "0.002"
+ TNOM "25.0"
+ 0 0 0 0 0 0 0 0 0
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 12 0
-$
ERROR(ORPSIM-16316): Invalid device
+8946208 0
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 13 1
-$
ERROR(ORPSIM-16316): Invalid device
+1 1 0 1
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 14 1
-$
ERROR(ORPSIM-16316): Invalid device
+1 1 1 "*" 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 15 0
-$
ERROR(ORPSIM-16316): Invalid device
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 16 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 "0" 
+1 "0" 
+2 "chkpt_default, , ," 
@End Analysis
-------------$
ERROR -- Missing node
@Analysis: 17 0
-$
ERROR(ORPSIM-16316): Invalid device
+0 "-1" 
+1 "-1" 
+2 "-1" 
+3 "-1" 
+4 "1" 
@End Analysis
-------------$
ERROR -- Missing node

**** RESUMING TestePspice.cir ****
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 3ms 1ms 100u SKIPBP 
.OPTIONS ADVCONV
.AUTOCONVERGE ITL1=1000 ITL2=1000 ITL4=1000 RELTOL=0.05 ABSTOL=1.0E-6 VNTOL=.001 PIVTOL=1.0E-10 
.PROBE64 V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source TESTE1
R_R1         N15687 N15680  100 TC=0,0 
C_C1         0 N15687  1u IC=0 TC=0,0 
V_V2         N15680 0  
+SIN 0V 1V 0.5k 0 0 0
C_C2         N26086 N26026  1u  TC=0,0 
C_C3         N26550 N26490  1u  TC=0,0 
C_C4         N26904 N26844  1u  TC=0,0 
C_C5         N27258 N27198  1u  TC=0,0 
R_R2         0 NC  3k TC=0,0 
R_R3         DC- DC+  500 TC=0,0 
V_V3         AC+ AC-  
+SIN 0 5 50 0 0 0
X_X1         DC+ N25968 AC+ CSD17308Q3
X_X2         AC+ N27140 DC- CSD17308Q3
X_X3         AC- N26786 DC- CSD17308Q3
X_X4         DC+ N26432 AC- CSD17308Q3
X_U1         DC- AC- NC N26786 N26786 NC NC N26844 N26904 LM74670-Q1_TRANS
X_U2         AC- DC+ NC N26432 N26432 NC NC N26490 N26550 LM74670-Q1_TRANS
X_U3         AC+ DC+ NC N25968 N25968 NC NC N26026 N26086 LM74670-Q1_TRANS
X_U4         DC- AC+ NC N27140 N27140 NC NC N27198 N27258 LM74670-Q1_TRANS

**** RESUMING TestePspice.cir ****
.END
