# Blind/Buried Via Spacing

#### This group consists of Blind/Buried Via Spacing constraints.
The rules are as follows:

- Blind/Buried Via to Line: Defines the minimum blind/buried via to line spacing.
- Blind/Buried Via to Thru Pin: Defines the minimum blind/buried via to thru pin spacing.
- Blind/Buried Via to SMD Pin: Defines the minimum blind/buried via to SMD pin spacing.
- Blind/Buried Via to Test Pin: Defines the minimum blind/buried via to test pin spacing.
- Blind/Buried Via to Thru Via: Defines the minimum blind/buried via to thru via spacing.
- Blind/Buried Via to BB Via: Defines the minimum blind/buried via to blind/buried via spacing.
- Blind/Buried Via to Test Via: Defines the minimum blind/buried via to test via spacing.
- Blind/Buried Via to Microvia : Defines the minimum blind/buried via to microvia spacing.
- Blind/Buried Via to Shape: Defines the minimum blind/buried via to shape spacing.
- Blind/Buried Via to Bond Finger : Defines the minimum blind/buried via to bond finger spacing.