# Thru Via Spacing

#### This group consists of Thru Via Spacing.
The rules are as follows:

- Thru Via to Line: Defines the minimum thru via to line spacing.
- Thru Via to Thru Pin: Defines the minimum thru via to thru pin spacing.
- Thru Via to SMD Via: Defines the minimum thru via to SMD via spacing.
- Thru Via to Test Pin: Defines the minimum thru via to test pin spacing.
- Thru Via to Thru Via: Defines the minimum thru via to thru via spacing.
- Thru Via to BB Via: Defines the minimum thru via to blind/buried via spacing.
- Thru Via to Test Via: Defines the minimum thru via to test via spacing.
- Thru Via to Microvia : Defines the minimum microvia to thru via spacing.
- Thru Via to Shape: Defines the minimum thru via to shape spacing.
- Thru Via to Bond Finger : Defines the minimum thru via to bond finger spacing.