# Same Net Thru Via Spacing

#### This group consists of Same Net Thru Via Spacing constraints.
The rules are as follows:

- Thru Via to Line: Defines the minimum same net thru via to line spacing.
- Thru Via to Thru Via: Defines the minimum same net thru via to thru via spacing.
- Thru Via to SMD Via: Defines the minimum same net thru via to SMD via spacing.
- Thru Via to Test Via: Defines the minimum same net thru via to test via spacing.
- Thru Via to Thru Via: Defines the minimum same net thru via to thru via spacing.
- Thru Via to BB Via: Defines the minimum same net thru via to blind/buried via spacing.
- Thru Via to Test Via: Defines the minimum same net thru via to test via spacing.
- Thru Via to Microvia : Defines the minimum same net microvia to thru via spacing.
- Thru Via to Shape: Defines the minimum same net thru via to shape spacing.
- Thru Via to Bond Finger : Defines the minimum same net thru via to bond finger spacing.