### Component body to Edge finger

This constraint defines the rule for minimum allowable distance between edge of a component instance to an edge finger. Edge fingers are the pins of a finger connector. A finger connector is detected by the prefix used to define the component class in the symbol classification UI, which essentially assigns value for the attribute named 'DFA_DEV_CLASS'.
If the prefix of the class name is "FCON_", that symbol will be treated as finger connector.

#### DRC Code: %2