### Cutout to Non signal geometry fabrication checks

The Cutout to non-signal geometry category consists of a group of fabrication checks for outermost edge of various non-signal geometry objects to outer edge of any cutout geometry in the design. A non-signal geometry can be one of the following:

- A filled shape which is not on any net in a conducting(ETCH) layer. This includes rectangles and polygons as well.
- Text line in conducting layer
- Line or arc in conducting layer

#### Example checks

- Cutout to non signal shape
- Cutout to text
- Cutout to line