### Tall component to conveyed edge

This constraint defines the rule for minimum allowable distance between edge of a tall component instance to the conveyed edge.
A tall component is defined as a symbol having package height greater than the value specified in the attribute DFA_MIN_HEIGHT_TALLCOMP. This can be defined through 'Design for Assembly' options page in Analysis Mode dialog.
The direction of conveyed edge can be defined through the 'Design for Assembly' options page in Analysis Mode dialog. The possible values are 'North-South' or 'East-West'. If the conveyed edge direction is 'North-South', the distance will be computed against the north and south edge of the design outline extent. Similarly, if the direction is 'East-West', the distance between east or west side of the design outline extent will be checked.

#### DRC Code: %2