### Hole Skip Via

Skip vias span more than two layers to make a connection. The layer(s) contained between the start and end layer should not contain a pad definition. There is also a limit as to the number of layers a skip via can pass through.

- Maximum number of layers for a skip via
- A skip via that has a pad defined and not flagged, will be removed as an unused internal pad definition

#### DRC Code: %2