# Same Net Thru Pin Spacing

#### This group consists of Same Net Thru Pin Spacing constraints.
The rules are as follows:

- Thru Pin to Line: Defines the minimum same net thru pin to line spacing.
- Thru Pin to Thru Pin: Defines the minimum same net thru pin to thru pin spacing.
- Thru Pin to SMD Pin: Defines the minimum same net thru pin to SMD pin spacing.
- Thru Pin to Test Pin: Defines the minimum same net thru pin to test pin spacing.
- Thru Pin to Thru Via: Defines the minimum same net thru pin to thru via spacing.
- Thru Pin to BB Via: Defines the minimum same net thru pin to blind/buried via spacing.
- Thru Pin to Test Via: Defines the minimum same net thru pin to test via spacing.
- Thru Pin to Microvia : Defines the minimum same net microvia to thru pin spacing.
- Thru Pin to Shape: Defines the minimum same net thru pin to shape spacing.
- Thru Pin to Bond Finger : Defines the minimum same net thru pin to bond finger spacing.