### Silkscreen to hole fabrication checks

The Silkscreen to hole category consists of a group of fabrication checks for defining minimum allowable distance between edge of the hole of various types of pin or via objects to any silkscreen geometry in the design. A silkscreen object can be any line, shape or text in a silkscreen subclass.

#### Example checks

- Silkscreen object to thru pin hole
- Silkscreen object to thru via hole
- Silkscreen object to slot hole