### Finger to Component Edge

Bond finger component edge spacing is the minimum separation required between a bond finger and the edge of a component, a die or discrete, on the same edge of the package substrate. This is the clearance required to ensure the capillary clears the component edge when adding wires. To run this online rule, choose Setup — Constraints — Modes and set Bond finger to Component.

#### DRC Code: %2