### Wire End to Wire End

Bond wire end-to-end is the minimum separation between the connection points of two different bond wires. This applies to both ends of the wires.
This value is based on the size of the bonding machine as the machine must clear the first wire's end when placing the second wire.
To run this online rule, choose Setup &emdash; Constraints &emdash; Modes and set Wire end to Wire end to On.

#### DRC Code: %2