# Design Acute Angle Detection

#### This group consists of Design Acute Angle Detection constraints.
The rules are as follows:

- Minimum Shape edge to edge angle: Checks resulting angle between shape segments that are part of the same shape. This angle is created at the outer edges of the shape.
- Minimum Line to Pad angle: Checks resulting angle at the point a cline enters a pad.
- Minimum Line to Shape angle: Checks resulting angle at the point a cline enters a shape.
- Minimum Line to Line angle: Checks resulting angle between cline segments.