### Silkscreen object to via object fabrication checks

The Silkscreen to hole category consists of a group of fabrication checks for defining minimum allowable distance between the edge of the pad of various types of via objects to any silkscreen geometry in the design. A silkscreen object can be any line, shape or text in a silkscreen subclass.

#### Example checks

- Silkscreen object to thru via pad
- Silkscreen object to micro via pad
- Silkscreen object to blind/buried via pad