### Allow overlapping pad/shape on the same net

This is an option to specify that overlapping pad with shape or pad with pad should not be treated as violation in case they are on the same net. The pads can be from via or pin.

In copper spacing checks, if two pads of the same net overlap, or if a pad overlaps with a shape on the same net in case of static shape, fabrication DRC violations are reported with actual value as OVERLAP. This may be perfectly valid case from manufacturing perspective. If this option is set, those DRCs will not be reported.