|  |  |
| --- | --- |
| 1. Connect PC/laptop to USB2ANY | C:\Users\a0762069\Desktop\IMG_0426.JPG |
| 1. Launch GUI |  |
| 1. Click “OK”   Notes: If didn’t see this screen, please jump to step 7 |  |
| 1. Click “Help me locate the BSL Button(S1)” to know S1 location |  |
| 1. Disconnect USB Connector | C:\Users\a0762069\Desktop\IMG_0430.JPG |
| 1. Push S1 and Connect USB Connector together | C:\Users\a0762069\Desktop\IMG_0429.JPG |
| 1. After Step 6 -> screen will show and ready for updating firmware. |  |
| 1. Click Update firmware to update firmware |  |
| 1. After updating firmware Click close. USB2ANY is ready work with DRV10983EVM. |  |