Error Report for  - Users\a0226691\AppData\Local\Temp\ProFCD2.tmp
10/2/2017 4:21:22 PM

Warning arcs were not exported.

Warning pad shape change for U1-3 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-8 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-17 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-12 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U5-21 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-26 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U5-23 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U5-24 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U5-25 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U4-21 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-26 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U4-23 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U4-24 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U4-25 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U6-25 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U6-24 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U6-23 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U6-26 from  to rounded 14.764mil,14.764mil
Warning pad shape change for U6-21 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U2-5 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U3-1 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-32 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-29 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U2-7 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U2-4 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U1-20 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U2-8 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U3-26 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-24 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-28 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-5 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U5-1 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-11 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U4-1 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-12 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U6-1 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-7 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U5-22 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-9 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U4-22 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-14 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U6-22 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U2-1 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U1-10 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-31 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-25 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U1-11 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-13 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-15 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-2 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-4 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-6 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-19 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-1 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U1-9 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-20 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U1-7 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-18 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-16 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U1-5 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-19 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U1-18 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-17 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U1-16 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-15 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U1-14 from rounded 17.716mil,55.118mil to rectangular 17.716mil,37.402mil
Warning pad shape change for U3-22 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U5-18 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-20 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-19 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-8 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U4-14 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-13 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-12 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-14 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-17 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-15 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-13 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-16 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-12 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-18 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-17 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-20 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-19 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-16 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-15 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-20 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-19 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-17 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-16 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-18 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-13 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-12 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-15 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-14 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-30 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for D1-1 from  to rounded 18.504mil,18.504mil
Warning pad shape change for D1-2 from  to rounded 18.504mil,18.504mil
Warning pad shape change for U3-21 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U2-3 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U5-6 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-7 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-5 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-10 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-11 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-8 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-9 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-3 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U5-4 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-6 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-7 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-5 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-10 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-11 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-8 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-9 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-3 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U4-4 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-5 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-6 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-9 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-10 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-7 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-8 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-3 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-4 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U6-11 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-27 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-6 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U5-2 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-10 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U4-2 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U3-13 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U6-2 from  to rectangular 17.717mil,9.842mil
Warning pad shape change for U2-2 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for D1-3 from  to rounded 18.504mil,18.504mil
Warning pad shape change for U2-6 from rounded 23.622mil,57.087mil to rectangular 23.622mil,33.465mil
Warning pad shape change for U3-2 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-4 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U3-23 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U5-27 from  to rounded 129.921mil,129.921mil
Warning pad shape change for U3-3 from rounded 7.874mil,23.622mil to rectangular 7.874mil,15.748mil
Warning pad shape change for U4-27 from  to rounded 129.921mil,129.921mil
Warning pad shape change for U6-27 from  to rounded 129.921mil,129.921mil
