{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["TICSPro","Command Descriptions"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TICSPro","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Step 1",null,"Launch TICSPro"]
[null,null,"TICSPro Path","C:\\Program Files (x86)\\Texas Instruments\\TICS Pro"]
[null,null,"Selected Device","LMX2572"]
[]
[]
[]
["Step 2",null,"Run Commands","See Code for More Details"]
[null,null,"CmdTarget","MASH_ORDER"]
[null,null,"CmdName","SETINDEX"]
[null,null,"Parameter",2]
[]
[]
[null,null,"Return Value"]
[]
[]
[]
[]
[]
[]
[]
["Note that if you have an error in your program, the link to TICSPro is broken"]
["In this case, close whole Excel and restart"]

{"sheet":"Command Descriptions","index":1,"n_rows":33,"n_cols":5,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["CmdName","CmdTarget","Parameter","Return Value","Description"]
["ADDBURST",null,"Burst Command",null,"Burst Mode Tab:  Adds a burst command.  CmdTarget is the reg name or delay time"]
["CLOSETICSPRO",null,null,null,"Closes TICSPro program"]
["DELETEBURST",null,null,null,"Burst Mode Tab:  Deletes all burst commands"]
["ENABLEBURST",null,null,null,"Burst Mode Tab:  Starts the burst and immediately return and not wait until burst is done"]
["GETFIELDVALUE","[FieldName]",null,"[FieldValue]","Returns the value of named field"]
["GETINDEX","[FieldName]",null,"[IndexValue]","Returns the indext value of named field"]
["GETPIN","[PinName]",null,"[PinValue]","Returns pin state"]
["GETTEXT","[FieldName]",null,"[FieldValueText]","Returns the text value represented by named field."]
["LOAD",null,null,null,"Loads all registers"]
["LOADREG",null,null,null,"Performs a write of the specified register by name e.g. R0, R4 etc."]
["PRESSBUTTON","[ButtonName]",null,null,"Presses the flexGUI button specified"]
["READALLREGISTERS",null,null,null,"Reads all registers"]
["READFIELD","[FieldName]",null,"[FieldValue]","Returns the register contents that have been read back from the part"]
["READFIELDVALUE","[FieldName]",null,"[FieldIndex]","Reads the field value and updates the GUI"]
["READINDEX","[FieldName]",null,"[FieldIndex]","Reads the indexed value from the device"]
["READREG_ADD-DATA","[RegisterNumber]",null,"[FullRegisterValue]","Reads the regsiter including the address"]
["READREG_DATA","[RegisterNumber]",null,"[RegisterDataValue]","Reads the regsiter data only"]
["READREGUPDATE","[RegisterNumber]",null,"[RegisterValue]","Reads the regsiter and updates the GUI"]
["READTEXT","[FieldName]",null,"[FieldText]","Reads value from the device and returns the text value"]
["RESTORESETUP",null,"[SetupFile]",null,"Restores a setup file"]
["RUNBURSTONCE",null,null,null,"Burst Mode Tab:  Runs the burst mode one time"]
["SAVESETUP",null,"[SaveFile]",null,"Saves a setup to a *.mac file"]
["SETMODE",null,"[ModeNumber]",null,"Restores saved modes in the TICS Pro restoring a particular state"]
["SETMODETEXT",null,"[ModeName]",null,"Sets the mode as described by a string"]
["SETTEXT","[FieldName]","[TextValue]",null,"Sets the value of a Flex Script Variable"]
["SETFIELDVALUE","[FieldName]","[VieldValue]",null,"Sets the value of the field to a specific value"]
["SETINDEX","[FieldName]","[IndexValue]",null,"Sets a register or smart list to an index"]
["SETPIN","[PinName]","[1 or 0]",null,"The PRGMPINS is similar to the PRGMBITS except that it controls external pins of the parallel port"]
["SETPART",null,"[PartName]",null,"This command will select the desired TICS Pro Part"]
["SETREG",null,"[FullRegisterValue]",null,"Sets the register value that is specified in base 10"]
["STARTBURST",null,null,null,"Burst Mode Tab:  Starts the burst sequence"]
["STOPBURST",null,null,null,"Burst Mode Tab:  Stops the burst sequence"]