i use ClockPro like belows,

then File -> Save TXT file ,i send thru IIC path, have got ACK signals back, but Y2 still only 3V voltage, not 66M pulses,
btw is it necessary to pull down VDD OUTs when i am sending IIC commands ?



