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uints_t valueToCopy;

uints ¢ myDatal4] = {oxaA, OxAA, oxAR, OxAsb

MyData_SetParameter(MYDATA_DATA_ID, sizeof(myData), &myData[1]);
/7 Call to retrieve the value of the third characteristic in the profile
if (SimpleProfile_GetParameter(SINPLEPROFILE_CHARS, &valueToCopy) == SUCCESS.
{
// Call to set that value of the fourth characteristic in the profile.
// Note that if notifications of the fourth characteristic have been
// enabled by a GATT client device, then a notification will be sent
// every time this function is called.
SimpleProfile_SetParameter(SIMPLEPROFILE_CHARG, sizeof(uintd t),
‘svalueToCopy);





The Value on smart phone.
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