PCM5100A no output waveforms

**Ch1:CAPP = 1.536MHz**

Description: pin-CAPP and pin-CAPM have the 1.536MHz with normal sound



**Ch1:CAPP = 899.8kHz**

Description: pin-CAPP and pin-CAPM have the 899.8kHz without normal sound



Ch1:DIN, Ch2:3.3V, Ch3:LRCK, Ch4:BCK



Ch1:DIN, Ch2:XSMT, Ch3:LRCK, Ch4:BCK



Ch1:DIN, Ch2:XSMT, Ch3:LRCK(zoom-in), Ch4:BCK



Ch1:OUTL, Ch2:3.3V, Ch3:LRCK, Ch4:BCK



Ch1:OUTL, Ch2:3.3V, Ch3:LRCK, Ch4:BCK(zoom-in)



Schematics:







Main board




Audio board
