


**TI.com comparison**




**Datasheet comparison**







The most conditions are different except PVDD= 12V and 15V

Register map >> Same

