6,0,0,-;Booting Linux on physical CPU 0x0000000000 [0x51af8014]
5,1,0,-;Linux version 4.19.152+ (jenkins-slave@CH3UU0007) (clang version 10.0.7 for Android NDK, GNU ld (binutils-2.27-bd24d23f) 2.27.0.20170315) #1 SMP PREEMPT Thu Feb 11 20:52:22 CST 2021
6,2,0,-;Machine model: Qualcomm Technologies, Inc. Honeywell CT45
6,3,0,-;earlycon: msm_geni_serial0 at MMIO 0x0000000004a90000 (options '')
6,4,0,-;bootconsole [msm_geni_serial0] enabled
6,5,0,-;efi: Getting EFI parameters from FDT:
6,6,0,-;efi: UEFI not found.
6,7,0,-;mem-offline: no memory to offline for DDR size:4255121408
3,8,0,-;OF: reserved mem: OVERLAP DETECTED!\x0adisp_rdump_region@5c000000 (0x000000005c000000--0x000000005cf00000) overlaps with cont_splash_region@5c000000 (0x000000005c000000--0x000000005cf00000)
6,9,0,-;Reserved memory: created CMA memory pool at 0x00000000fdc00000, size 32 MiB
6,10,0,-;OF: reserved mem: initialized node linux,cma, compatible id shared-dma-pool
6,11,0,-;Reserved memory: created CMA memory pool at 0x00000000fcc00000, size 16 MiB
6,12,0,-;OF: reserved mem: initialized node qseecom_ta_region, compatible id shared-dma-pool
6,13,0,-;Reserved memory: created CMA memory pool at 0x00000000fbc00000, size 16 MiB
6,14,0,-;OF: reserved mem: initialized node user_contig_region, compatible id shared-dma-pool
6,15,0,-;Reserved memory: created CMA memory pool at 0x00000000fa800000, size 20 MiB
6,16,0,-;OF: reserved mem: initialized node qseecom_region, compatible id shared-dma-pool
6,17,0,-;Reserved memory: created CMA memory pool at 0x00000000fa000000, size 8 MiB
6,18,0,-;OF: reserved mem: initialized node mem_dump_region, compatible id shared-dma-pool
6,19,0,-;Reserved memory: created CMA memory pool at 0x00000000f9800000, size 8 MiB
6,20,0,-;OF: reserved mem: initialized node adsp_region, compatible id shared-dma-pool
6,21,0,-;Reserved memory: created CMA memory pool at 0x00000000f3c00000, size 92 MiB
6,22,0,-;OF: reserved mem: initialized node secure_display_region, compatible id shared-dma-pool
6,23,0,-;Removed memory: created DMA memory pool at 0x0000000045700000, size 6 MiB
6,24,0,-;OF: reserved mem: initialized node hyp_region@45700000, compatible id removed-dma-pool
6,25,0,-;Removed memory: created DMA memory pool at 0x0000000045e00000, size 1 MiB
6,26,0,-;OF: reserved mem: initialized node xbl_aop_region@45e00000, compatible id removed-dma-pool
6,27,0,-;Removed memory: created DMA memory pool at 0x0000000045fff000, size 0 MiB
6,28,0,-;OF: reserved mem: initialized node sec_apps_region@45fff000, compatible id removed-dma-pool
6,29,0,-;Removed memory: created DMA memory pool at 0x0000000046000000, size 2 MiB
6,30,0,-;OF: reserved mem: initialized node smem_region@46000000, compatible id removed-dma-pool
6,31,0,-;Removed memory: created DMA memory pool at 0x0000000046200000, size 30 MiB
6,32,0,-;OF: reserved mem: initialized node cdsp_sec_regions@46200000, compatible id removed-dma-pool
6,33,0,-;Removed memory: created DMA memory pool at 0x000000004ab00000, size 105 MiB
6,34,0,-;OF: reserved mem: initialized node modem_region@4ab00000, compatible id removed-dma-pool
6,35,0,-;Removed memory: created DMA memory pool at 0x0000000051400000, size 5 MiB
6,36,0,-;OF: reserved mem: initialized node pil_video_region@51400000, compatible id removed-dma-pool
6,37,0,-;Removed memory: created DMA memory pool at 0x0000000051900000, size 1 MiB
6,38,0,-;OF: reserved mem: initialized node wlan_msa_region@51900000, compatible id removed-dma-pool
6,39,0,-;Removed memory: created DMA memory pool at 0x0000000051a00000, size 30 MiB
6,40,0,-;OF: reserved mem: initialized node cdsp_regions@51a00000, compatible id removed-dma-pool
6,41,0,-;Removed memory: created DMA memory pool at 0x0000000053800000, size 30 MiB
6,42,0,-;OF: reserved mem: initialized node pil_adsp_region@53800000, compatible id removed-dma-pool
6,43,0,-;Removed memory: created DMA memory pool at 0x0000000055600000, size 0 MiB
6,44,0,-;OF: reserved mem: initialized node ipa_fw_region@55600000, compatible id removed-dma-pool
6,45,0,-;Removed memory: created DMA memory pool at 0x0000000055610000, size 0 MiB
6,46,0,-;OF: reserved mem: initialized node ipa_gsi_region@55610000, compatible id removed-dma-pool
6,47,0,-;Removed memory: created DMA memory pool at 0x0000000055615000, size 0 MiB
6,48,0,-;OF: reserved mem: initialized node gpu_region@55615000, compatible id removed-dma-pool
6,49,0,-;Removed memory: created DMA memory pool at 0x0000000060000000, size 57 MiB
6,50,0,-;OF: reserved mem: initialized node removed_region@60000000, compatible id removed-dma-pool
7,51,0,-;cma: dma_contiguous_reserve(limit 1000000000000)
7,52,0,-;On node 0 totalpages: 970408
7,53,0,-;  Normal zone: 15163 pages used for memmap
7,54,0,-;  Normal zone: 0 pages reserved
7,55,0,-;  Normal zone: 970408 pages, LIFO batch:63
6,56,0,-;psci: probing for conduit method from DT.
6,57,0,-;psci: PSCIv1.0 detected in firmware.
6,58,0,-;psci: Using standard PSCI v0.2 function IDs
6,59,0,-;psci: MIGRATE_INFO_TYPE not supported.
6,60,0,-;psci: SMC Calling Convention v1.1
5,61,0,-;random: fast init done
6,62,0,-;percpu: Embedded 25 pages/cpu s62120 r8192 d32088 u102400
7,63,0,-;pcpu-alloc: s62120 r8192 d32088 u102400 alloc=25*4096
7,64,0,-;pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 [0] 4 [0] 5 [0] 6 [0] 7 
6,65,0,-;Detected VIPT I-cache on CPU0
6,66,0,-;CPU features: enabling workaround for ARM erratum 845719
6,67,0,-;CPU features: kernel page table isolation disabled by kernel configuration
6,68,0,-;Built 1 zonelists, mobility grouping on.  Total pages: 955245
5,69,0,-;Kernel command line: rcupdate.rcu_expedited=1 rcu_nocbs=0-7 kpti=off console=ttyMSM0,115200n8 earlycon=msm_geni_serial,0x4a90000 androidboot.hardware=qcom androidboot.console=ttyMSM0 androidboot.memcg=1 lpm_levels.sleep_disabled=1 video=vfb:640x400,bpp=32,memsize=3072000 msm_rtb.filter=0x237 service_locator.enable=1 swiotlb=2048 loop.max_part=7 buildvariant=userdebug androidboot.verifiedbootstate=orange androidboot.keymaster=1 androidboot.vbmeta.device=PARTUUID=be6503d0-48e6-11eb-b1f0-fb5468a953c3 androidboot.vbmeta.avb_version=1.0 androidboot.vbmeta.device_state=unlocked androidboot.vbmeta.hash_alg=sha256 androidboot.vbmeta.size=7296 androidboot.vbmeta.digest=217bee05af767ef8106ca827637cc5af33757b94f0be6a8e7934d68c80fce89e androidboot.veritymode=disabled androidboot.bootdevice=4804000.ufshc androidboot.fstab_suffix=default androidboot.boot_devices=soc/4804000.ufshc androidboot.serialno=751e5b08 androidboot.baseband=apq msm_drm.dsi_display0=qcom,mdss_dsi_ft8006m_720p_techsta
6,70,0,-;log_buf_len individual max cpu contribution: 131072 bytes
6,71,0,-;log_buf_len total cpu_extra contributions: 917504 bytes
6,72,0,-;log_buf_len min size: 131072 bytes
6,73,0,-;log_buf_len: 1048576 bytes
6,74,0,-;early log buf free: 123780(94%)
6,75,0,-;Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
6,76,0,-;Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
6,77,0,-;mem auto-init: stack:off, heap alloc:off, heap free:off
6,78,0,-;Memory: 3532300K/3881632K available (20476K kernel code, 2928K rwdata, 10168K rodata, 6400K init, 9747K bss, 152724K reserved, 196608K cma-reserved)
5,79,0,-;random: random: get_random_u64 called from __kmem_cache_create+0x8c/0x6c0 with crng_init=1
6,80,0,-;SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=8, Nodes=1
6,81,0,-;ftrace: allocating 48318 entries in 189 pages
6,82,0,-;rcu: Preemptible hierarchical RCU implementation.
6,83,0,-;rcu: \x09RCU dyntick-idle grace-period acceleration is enabled.
6,84,0,-;\x09All grace periods are expedited (rcu_expedited).
6,85,0,-;\x09Tasks RCU enabled.
6,86,0,-;NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
6,87,0,-;GICv3: Distributor has no Range Selector support
6,88,0,-;GICv3: no VLPI support, no direct LPI support
6,89,0,-;rcu: \x09Offload RCU callbacks from CPUs: 0-7.
6,90,0,-;arch_timer: CPU0: Trapping CNTVCT access
6,91,0,-;arch_timer: cp15 and mmio timer(s) running at 19.20MHz (virt/virt).
6,92,0,-;clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x46d987e47, max_idle_ns: 440795202767 ns
6,93,4,-;sched_clock: 56 bits at 19MHz, resolution 52ns, wraps every 4398046511078ns
6,94,8029,-;clocksource: Switched to clocksource arch_sys_counter
6,95,16421,-;kmemleak: Kernel memory leak detector disabled
6,96,21969,-;Calibrating delay loop (skipped), value calculated using timer frequency.. 38.40 BogoMIPS (lpj=192000)
6,97,32394,-;pid_max: default: 32768 minimum: 301
6,98,37610,-;Security Framework initialized
6,99,41770,-;SELinux:  Initializing.
6,100,45941,-;Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
6,101,52769,-;Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
6,102,70006,-;ASID allocator initialised with 65536 entries
6,103,76095,-;rcu: Hierarchical SRCU implementation.
4,104,108802,-;shmbridge is enabled
6,105,112483,-;EFI services will not be available.
6,106,121275,-;smp: Bringing up secondary CPUs ...
6,107,133098,-;Detected VIPT I-cache on CPU1
6,108,133186,-;arch_timer: CPU1: Trapping CNTVCT access
6,109,133196,-;CPU1: Booted secondary processor 0x0000000001 [0x51af8014]
6,110,140911,-;Detected VIPT I-cache on CPU2
6,111,140998,-;arch_timer: CPU2: Trapping CNTVCT access
6,112,141007,-;CPU2: Booted secondary processor 0x0000000002 [0x51af8014]
6,113,148632,-;Detected VIPT I-cache on CPU3
6,114,148722,-;arch_timer: CPU3: Trapping CNTVCT access
6,115,148732,-;CPU3: Booted secondary processor 0x0000000003 [0x51af8014]
6,116,156817,-;CPU features: enabling workaround for ARM erratum 858921
6,117,156884,-;SSBD disabled by kernel configuration
6,118,156895,-;CPU features: enabling workaround for Speculative Store Bypass Disable
6,119,156916,-;Detected VIPT I-cache on CPU4
6,120,157026,-;arch_timer: Enabling local workaround for ARM erratum 858921
6,121,157069,-;arch_timer: CPU4: Trapping CNTVCT access
6,122,157089,-;CPU4: Booted secondary processor 0x0000000100 [0x51af8002]
6,123,165729,-;Detected VIPT I-cache on CPU5
6,124,165827,-;arch_timer: Enabling local workaround for ARM erratum 858921
6,125,165860,-;arch_timer: CPU5: Trapping CNTVCT access
6,126,165880,-;CPU5: Booted secondary processor 0x0000000101 [0x51af8002]
6,127,174452,-;Detected VIPT I-cache on CPU6
6,128,174554,-;arch_timer: Enabling local workaround for ARM erratum 858921
6,129,174587,-;arch_timer: CPU6: Trapping CNTVCT access
6,130,174607,-;CPU6: Booted secondary processor 0x0000000102 [0x51af8002]
6,131,183192,-;Detected VIPT I-cache on CPU7
6,132,183296,-;arch_timer: Enabling local workaround for ARM erratum 858921
6,133,183330,-;arch_timer: CPU7: Trapping CNTVCT access
6,134,183350,-;CPU7: Booted secondary processor 0x0000000103 [0x51af8002]
6,135,184592,-;smp: Brought up 1 node, 8 CPUs
6,136,343722,-;SMP: Total of 8 processors activated.
6,137,348616,-;CPU features: detected: GIC system register CPU interface
6,138,355088,-;CPU features: detected: 32-bit EL0 Support
6,139,360634,-;CPU features: emulated: Privileged Access Never (PAN) using TTBR0_EL1 switching
6,140,369067,-;CPU: All CPU(s) started at EL1
6,141,373360,-;alternatives: patching kernel code
6,142,465479,-;allocated 36700160 bytes of page_ext
6,143,483639,-;Node 0, zone   Normal: page owner found early allocated 9830 pages
5,144,2075087,-;Registered cp15_barrier emulation handler
5,145,2080454,-;Registered setend emulation handler
6,146,2097268,-;clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
6,147,2107682,-;futex hash table entries: 2048 (order: 5, 131072 bytes)
6,148,2504231,-;pinctrl core: initialized pinctrl subsystem
4,149,2523868,-;
4,150,2525433,-;*************************************************************
4,151,2532425,-;**     NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE    **
4,152,2539353,-;**                                                         **
4,153,2546209,-;**  IOMMU DebugFS SUPPORT HAS BEEN ENABLED IN THIS KERNEL  **
4,154,2553165,-;**                                                         **
4,155,2560090,-;** This means that this kernel is built to expose internal **
4,156,2566945,-;** IOMMU data structures, which may compromise security on **
4,157,2573905,-;** your system.                                            **
4,158,2580824,-;**                                                         **
4,159,2587676,-;** If you see this message and you are not debugging the   **
4,160,2594628,-;** kernel, report this immediately to your vendor!         **
4,161,2601541,-;**                                                         **
4,162,2608500,-;**     NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE    **
4,163,2615357,-;*************************************************************
6,164,2625208,-;DMI not present or invalid.
6,165,2636647,-;NET: Registered protocol family 16
6,166,2664995,-;schedtune: configured to support 6 boost groups
6,167,2677309,-;audit: initializing netlink subsys (disabled)
5,168,2684979,-;audit: type=2000 audit(2.669:1): state=initialized audit_enabled=0 res=1
6,169,2700795,-;cpuidle: using governor menu
6,170,2705891,-;cpuidle: using governor qcom
6,171,2715467,-;NET: Registered protocol family 42
6,172,2723418,-;hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
6,173,2764463,-;DMA: preallocated 256 KiB pool for atomic allocations
6,174,2787420,-;DMA: preallocated 256 KiB pool for atomic allocations
6,175,2811600,-;exit: IPA_USB init success!
6,176,2905116,-;platform 61800000.qseecom: assigned reserved memory node qseecom_region
 SUBSYSTEM=platform
 DEVICE=+platform:61800000.qseecom
6,177,2980388,-;platform ab00000.qcom,lpass: assigned reserved memory node pil_adsp_region@53800000
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,178,2994689,-;platform b300000.qcom,turing: assigned reserved memory node cdsp_regions@51a00000
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
6,179,3006692,-;platform soc:mem_dump: assigned reserved memory node mem_dump_region
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
6,180,3081236,-;platform soc:qcom,smem: assigned reserved memory node smem_region@46000000
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,smem
6,181,3101252,-;platform soc:qcom,msm-adsprpc-mem: assigned reserved memory node adsp_region
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-adsprpc-mem
6,182,3181266,-;platform 5ab0000.qcom,venus: assigned reserved memory node pil_video_region@51400000
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
6,183,3199414,-;platform 6080000.qcom,mss: assigned reserved memory node modem_region@4ab00000
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
6,184,3248895,-;platform soc:qcom,ipa_fws: assigned reserved memory node ipa_fw_region@55600000
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ipa_fws
4,185,4077748,-;------------[ cut here ]------------
4,186,4082636,-;WARNING: CPU: 7 PID: 1 at drivers/irqchip/irq-gic-v3.c:1057 gic_irq_domain_translate+0x150/0x158
4,187,4092519,-;Modules linked in:
4,188,4095655,-;CPU: 7 PID: 1 Comm: swapper/0 Not tainted 4.19.152+ #1
4,189,4101889,-;Hardware name: Qualcomm Technologies, Inc. Honeywell CT45 (DT)
4,190,4108819,-;pstate: 60400005 (nZCv daif +PAN -UAO)
4,191,4113666,-;pc : gic_irq_domain_translate+0x150/0x158
4,192,4118770,-;lr : gic_irq_domain_translate+0x14c/0x158
4,193,4123863,-;sp : ffffff800805b630
4,194,4127219,-;x29: ffffff800805b630 x28: ffffff8009fcb0a0 
4,195,4132607,-;x27: 0000000000000000 x26: ffffff8009e816f0 
4,196,4137991,-;x25: 0000000000000001 x24: ffffffc0f5cf1480 
4,197,4143376,-;x23: 00000000006080c0 x22: ffffffc005ff6480 
4,198,4148759,-;x21: ffffff800805b670 x20: ffffff800805b66c 
4,199,4154153,-;x19: ffffff800805b718 x18: 0000000000000034 
4,200,4159535,-;x17: ffffff800a846000 x16: 000000000000003a 
4,201,4164918,-;x15: 0000000000000000 x14: ffffff800a0dc018 
4,202,4170301,-;x13: ffffff800a556c88 x12: ffffff800815faa4 
4,203,4175687,-;x11: 0000000000000015 x10: 000000000682aaab 
4,204,4181080,-;x9 : 7094533e5961e000 x8 : 7094533e5961e000 
4,205,4186462,-;x7 : 7563205b2d2d2d2d x6 : ffffff800a84862c 
4,206,4191848,-;x5 : 0000000000000000 x4 : 0000000000000008 
4,207,4197229,-;x3 : ffffff800805b2a8 x2 : ffffff8008097690 
4,208,4202621,-;x1 : ffffff800815faa4 x0 : 0000000000000000 
4,209,4208006,-;Call trace:
4,210,4210500,-; gic_irq_domain_translate+0x150/0x158
4,211,4215254,-; gic_irq_domain_alloc+0x58/0x260
4,212,4219585,-; irq_domain_alloc_irqs_parent+0x48/0x88
4,213,4224522,-; msm_mpm_gic_chip_alloc+0xe8/0x168
4,214,4229015,-; __irq_domain_alloc_irqs+0x1ac/0x388
4,215,4233683,-; irq_create_fwspec_mapping+0x1f4/0x358
4,216,4238520,-; irq_create_of_mapping+0x64/0x90
4,217,4242843,-; of_irq_to_resource+0xb4/0x1b0
4,218,4246995,-; of_irq_to_resource_table+0x3c/0x78
4,219,4251573,-; of_device_alloc+0x128/0x1e8
4,220,4255546,-; of_platform_device_create_pdata+0x74/0x118
4,221,4260815,-; of_platform_bus_create+0x28c/0x500
4,222,4265389,-; of_platform_bus_create+0x2f0/0x500
4,223,4269961,-; of_platform_populate+0x94/0x120
4,224,4274281,-; of_platform_default_populate_init+0xb0/0xcc
4,225,4279639,-; do_one_initcall+0x120/0x2a0
4,226,4283620,-; kernel_init_freeable+0x304/0x3b8
4,227,4288031,-; kernel_init+0x18/0x298
4,228,4291564,-; ret_from_fork+0x10/0x1c
4,229,4295201,-;---[ end trace e3272503f35f0d74 ]---
3,230,4440397,-;Unable to find DT property: qcom,msm-imem-download_mode
3,231,4449226,-;Unable to find DT property: qcom,msm-imem-emergency_download_mode
6,232,4467411,-;msm_watchdog f017000.qcom,wdt: wdog absent resource not present
 SUBSYSTEM=platform
 DEVICE=+platform:f017000.qcom,wdt
6,233,4477199,-;msm_watchdog f017000.qcom,wdt: MSM Watchdog Initialized
 SUBSYSTEM=platform
 DEVICE=+platform:f017000.qcom,wdt
6,234,4518358,-;MSM Memory Dump base table set up
6,235,4522860,-;MSM Memory Dump apps data table set up
3,236,4528695,-;Minidump: Entry name already exist.
3,237,4533296,-;msm_mem_dump soc:mem_dump: Mini dump entry failed id = 101
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
3,238,4540015,-;Minidump: Entry name already exist.
3,239,4544608,-;msm_mem_dump soc:mem_dump: Mini dump entry failed id = 102
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
3,240,4551358,-;Minidump: Entry name already exist.
3,241,4555955,-;msm_mem_dump soc:mem_dump: Mini dump entry failed id = 103
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
3,242,4562972,-;Minidump: Entry name already exist.
3,243,4567564,-;msm_mem_dump soc:mem_dump: Mini dump entry failed id = 133
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
3,244,4574324,-;Minidump: Entry name already exist.
3,245,4578983,-;msm_mem_dump soc:mem_dump: Mini dump entry failed id = 134
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
3,246,4585624,-;Minidump: Entry name already exist.
3,247,4590317,-;msm_mem_dump soc:mem_dump: Mini dump entry failed id = 135
 SUBSYSTEM=platform
 DEVICE=+platform:soc:mem_dump
3,248,4628486,-;qcom_glink_rpm soc:rpm-glink: failed to register early notif -22
 SUBSYSTEM=platform
 DEVICE=+platform:soc:rpm-glink
6,249,4638759,-;qcom_smd_rpm_probe: RPM-SMD running version 0
6,250,4653742,-;sps:sps is ready.
6,251,4659616,-;spmi spmi-0: PMIC arbiter version v5 (0x50010000)
 SUBSYSTEM=spmi
 DEVICE=+spmi:spmi-0
3,252,4703396,-;LCDB: qpnp_lcdb_regulator_probe: Failed to parse dt rc=-517
6,253,5125563,-;cryptd: max_cpu_qlen set to 1000
3,254,5303200,-;gpu_cx_gdsc: regulator get failed, ret=-517
3,255,5324728,-;gpu_gx_gdsc: regulator get failed, ret=-517
6,256,5391518,-;Minidump: Enabled with max number of regions 200
6,257,5402141,-;KPI: Bootloader start count = 145753
6,258,5406839,-;KPI: Bootloader end count = 520067
6,259,5411501,-;KPI: Bootloader display count = 3087230109
6,260,5416706,-;KPI: Bootloader load kernel count = 2072265091
6,261,5422349,-;KPI: Kernel MPM timestamp = 758560
6,262,5426863,-;KPI: Kernel MPM Clock frequency = 32768
6,263,5432050,-;socinfo_print: v0.15, id=470, ver=1.0, raw_id=372, raw_ver=0, hw_plat=11, hw_plat_ver=65536\x0a accessory_chip=0, hw_plat_subtype=6, pmic_model=65581, pmic_die_revision=65537 foundry_id=2 serial_number=1241726495 num_pmics=2 chip_family=0x6a raw_device_family=0x9 raw_device_number=0x2 nproduct_id=0x41c num_clusters=0x1 ncluster_array_offset=0xb0 num_defective_parts=0xc ndefective_parts_array_offset=0xb4 nmodem_supported=0x0
6,264,5473214,-;mem-offline: System booted with no zone movable memory blocks. Cannot perform memory offlining
3,265,5523819,-;arm-smmu 59a0000.kgsl-smmu: Couldn't get clock: gcc_gpu_memnoc_gfx
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.kgsl-smmu
3,266,5549286,-;AXI: msm_bus_scale_register_client(): msm_bus_scale_register_client: Bus driver not ready.
3,267,5558744,-;arm-smmu c600000.apps-smmu: Bus client registration failed
 SUBSYSTEM=platform
 DEVICE=+platform:c600000.apps-smmu
3,268,5570983,-;Error: Driver 'arm-smmu' is already registered, aborting...
5,269,5595169,-;SCSI subsystem initialized
6,270,5604623,-;usbcore: registered new interface driver usbfs
6,271,5612007,-;usbcore: registered new interface driver hub
6,272,5619775,-;usbcore: registered new device driver usb
4,273,5631488,-;usb_phy_generic soc:usb_nop_phy: soc:usb_nop_phy supply vcc not found, using dummy regulator
 SUBSYSTEM=platform
 DEVICE=+platform:soc:usb_nop_phy
6,274,5643022,-;usb_phy_generic soc:usb_nop_phy: Linked as a consumer to regulator.0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:usb_nop_phy
6,275,5667401,-;qcom,qpnp-power-on 1c40000.qcom,spmi:qcom,pmi632@2:qcom,power-on@800: PMIC@SID2 Power-on reason: Triggered from CBL (External Power Supply) and 'cold' boot
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pmi632@2:qcom,power-on@800
6,276,5682629,-;qcom,qpnp-power-on 1c40000.qcom,spmi:qcom,pmi632@2:qcom,power-on@800: PMIC@SID2: Power-off reason: Triggered from SOFT (Software)
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pmi632@2:qcom,power-on@800
6,277,5702470,-;qcom,qpnp-power-on 1c40000.qcom,spmi:qcom,pm6125@0:qcom,power-on@800: PMIC@SID0 Power-on reason: Triggered from Hard Reset and 'cold' boot
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pm6125@0:qcom,power-on@800
6,278,5716210,-;qcom,qpnp-power-on 1c40000.qcom,spmi:qcom,pm6125@0:qcom,power-on@800: PMIC@SID0: Power-off reason: Triggered from PS_HOLD (PS_HOLD/MSM Controlled Shutdown)
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pm6125@0:qcom,power-on@800
6,279,5736351,-;input: qpnp_pon as /devices/platform/soc/1c40000.qcom,spmi/spmi-0/spmi0-00/1c40000.qcom,spmi:qcom,pm6125@0:qcom,power-on@800/input/input0
6,280,5757900,-;media: Linux media interface: v0.10
6,281,5763565,-;videodev: Linux video capture interface: v2.00
6,282,6101517,-;EDAC MC: Ver: 3.0.0
3,283,6112759,-;qcom-cpufreq-hw f521000.qcom,cpufreq-hw: CPUFreq resource init failed
 SUBSYSTEM=platform
 DEVICE=+platform:f521000.qcom,cpufreq-hw
6,284,6150418,-;platform soc:qcom,ion:qcom,ion-heap@10: assigned reserved memory node secure_display_region
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ion:qcom,ion-heap@10
6,285,6167275,-;platform soc:qcom,ion:qcom,ion-heap@26: assigned reserved memory node user_contig_region
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ion:qcom,ion-heap@26
6,286,6181034,-;platform soc:qcom,ion:qcom,ion-heap@27: assigned reserved memory node qseecom_region
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ion:qcom,ion-heap@27
6,287,6194077,-;platform soc:qcom,ion:qcom,ion-heap@19: assigned reserved memory node qseecom_ta_region
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ion:qcom,ion-heap@19
6,288,6213743,-;ION heap system created
6,289,6219288,-;ION heap secure_heap created
6,290,6223741,-;ION heap secure_display created at 0x00000000f3c00000 with size 5c00000
6,291,6454989,-;platform soc:qcom,ion:qcom,ion-heap@14: ion_secure_carveout: creating heap@0x46200000, size 0x1e00000
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ion:qcom,ion-heap@14
6,292,6465525,-;ION heap secure_carveout created
6,293,6470055,-;ION heap user_contig created at 0x00000000fbc00000 with size 1000000
6,294,6477759,-;ION heap qsecom created at 0x00000000fa800000 with size 1400000
6,295,6484988,-;ION heap qsecom_ta created at 0x00000000fcc00000 with size 1000000
6,296,6515959,-;PMIC@SID2: PMI632 v2.0 options: 0, 0, 0, 0
6,297,6523907,-;PMIC@SID0: PM6125 v1.1 options: 0, 0, 0, 0
6,298,6570626,-;SDAM base=0xb600 size=128 registered successfully
6,299,6579621,-;Advanced Linux Sound Architecture Driver Initialized.
6,300,6604246,-;Bluetooth: Core ver 2.22
6,301,6609191,-;NET: Registered protocol family 31
6,302,6613715,-;Bluetooth: HCI device and connection manager initialized
6,303,6620423,-;Bluetooth: HCI socket layer initialized
6,304,6625531,-;Bluetooth: L2CAP socket layer initialized
6,305,6631887,-;Bluetooth: SCO socket layer initialized
6,306,6637165,-;NetLabel: Initializing
6,307,6640802,-;NetLabel:  domain hash size = 128
6,308,6645238,-;NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
6,309,6654370,-;NetLabel:  unlabeled traffic allowed by default
6,310,6731550,-;qcom-clk-smd-rpm soc:qcom,rpmcc: Registered RPM clocks
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,rpmcc
6,311,6749434,-;pm6125_s3_level: Bringing 1uV into 16-16uV
6,312,6771247,-;pm6125_s3_floor_level: Bringing 1uV into 16-16uV
6,313,6788203,-;gpu_cx_gdsc: supplied by pm6125_s3_level
6,314,6795134,-;gpu_gx_gdsc: supplied by pm6125_s3_level
6,315,6808364,-;pm6125_s3_level_ao: Bringing 1uV into 16-16uV
6,316,6837822,-;pm6125_s5_level: Bringing 1uV into 16-16uV
6,317,6858434,-;pm6125_s5_floor_level: Bringing 1uV into 16-16uV
6,318,6880566,-;pm6125_s5_level_ao: Bringing 1uV into 16-16uV
6,319,6979225,-;pm6125_l2_level: Bringing 1uV into 16-16uV
6,320,7003770,-;pm6125_l3_level: Bringing 1uV into 16-16uV
6,321,7416301,-;LCDB: qpnp_lcdb_regulator_probe: LCDB module successfully registered! lcdb_en=1 ldo_voltage=5500mV ncp_voltage=5500mV bst_voltage=5650mV
6,322,7434060,-;bengal-dispcc 5f00000.qcom,dispcc: Linked as a consumer to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:5f00000.qcom,dispcc
6,323,7447646,-;bengal-dispcc 5f00000.qcom,dispcc: Dropping the link to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:5f00000.qcom,dispcc
6,324,7463326,-;gcc-bengal 1400000.qcom,gcc: Linked as a consumer to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:1400000.qcom,gcc
6,325,7472631,-;gcc-bengal 1400000.qcom,gcc: Linked as a consumer to regulator.15
 SUBSYSTEM=platform
 DEVICE=+platform:1400000.qcom,gcc
6,326,7481989,-;gcc-bengal 1400000.qcom,gcc: Linked as a consumer to regulator.16
 SUBSYSTEM=platform
 DEVICE=+platform:1400000.qcom,gcc
6,327,7578354,-;gcc-bengal 1400000.qcom,gcc: Registered GCC clocks
 SUBSYSTEM=platform
 DEVICE=+platform:1400000.qcom,gcc
6,328,7587921,-;bengal-gpucc 5990000.qcom,gpucc: Linked as a consumer to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:5990000.qcom,gpucc
6,329,7597079,-;bengal-gpucc 5990000.qcom,gpucc: Linked as a consumer to regulator.16
 SUBSYSTEM=platform
 DEVICE=+platform:5990000.qcom,gpucc
6,330,7622677,-;gpu_cc_gx_gfx3d_clk_src: set OPP pair(320000000 Hz: 64 uV) on 5900000.qcom,kgsl-3d0
6,331,7658153,-;gpu_cc_gx_gfx3d_clk_src: set OPP pair(980000000 Hz: 416 uV) on 5900000.qcom,kgsl-3d0
6,332,7667762,-;bengal-gpucc 5990000.qcom,gpucc: Registered GPUCC clocks
 SUBSYSTEM=platform
 DEVICE=+platform:5990000.qcom,gpucc
6,333,7682487,-;arm-smmu 59a0000.kgsl-smmu: Linked as a consumer to regulator.11
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.kgsl-smmu
5,334,7689961,-;arm-smmu 59a0000.kgsl-smmu: \x09non-coherent table walk
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.kgsl-smmu
5,335,7696037,-;arm-smmu 59a0000.kgsl-smmu: \x09(IDR0.CTTW overridden by FW configuration)
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.kgsl-smmu
5,336,7703960,-;arm-smmu 59a0000.kgsl-smmu: \x09stream matching with 4 register groups
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.kgsl-smmu
3,337,7748476,-;AXI: msm_bus_scale_register_client(): msm_bus_scale_register_client: Bus driver not ready.
3,338,7757855,-;arm-smmu c600000.apps-smmu: Bus client registration failed
 SUBSYSTEM=platform
 DEVICE=+platform:c600000.apps-smmu
7,339,8043243,-;energy_model: Created perf domain 0-3
7,340,8054124,-;energy_model: pd4: hertz/watts ratio non-monotonically decreasing: em_cap_state 1 >= em_cap_state0
7,341,8065466,-;energy_model: Created perf domain 4-7
6,342,8067704,-;cpufreq: driver qcom-cpufreq-hw up and running
6,343,8079415,-;bengal-dispcc 5f00000.qcom,dispcc: Linked as a consumer to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:5f00000.qcom,dispcc
6,344,8090238,-;bengal-dispcc 5f00000.qcom,dispcc: Registered Display CC clocks
 SUBSYSTEM=platform
 DEVICE=+platform:5f00000.qcom,dispcc
3,345,8099990,-;AXI: msm_bus_scale_register_client(): msm_bus_scale_register_client: Bus driver not ready.
3,346,8109335,-;arm-smmu c600000.apps-smmu: Bus client registration failed
 SUBSYSTEM=platform
 DEVICE=+platform:c600000.apps-smmu
6,347,8117272,-;clocksource: Switched to clocksource arch_sys_counter
5,348,8528104,-;VFS: Disk quotas dquot_6.6.0
6,349,8532169,-;VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
3,350,8546267,-;msm_bus_fabric_init_driver
3,351,8605977,-;msm_bus_dev_init_qos: Skipping QOS init for 26
6,352,8606287,-;msm_bus_device 1880000.ad-hoc-bus: Bus scaling driver probe successful
 SUBSYSTEM=platform
 DEVICE=+platform:1880000.ad-hoc-bus
6,353,8626943,-;mdss_pll_probe: MDSS pll label = MDSS DSI 0 PLL
6,354,8632613,-;mdss_pll_probe: mdss_pll_probe: label=MDSS DSI 0 PLL PLL SSC enabled
6,355,8641656,-;mdss_pll 5e94400.qcom,mdss_dsi0_pll: Linked as a consumer to regulator.10
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi0_pll
4,356,8650053,-;mdss_pll 5e94400.qcom,mdss_dsi0_pll: Failed to create 5e94400.qcom,mdss_dsi0_pll debugfs directory
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi0_pll
4,357,8660111,-;mdss_pll 5e94400.qcom,mdss_dsi0_pll: Failed to create 5e94400.qcom,mdss_dsi0_pll debugfs directory
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi0_pll
4,358,8670184,-;mdss_pll 5e94400.qcom,mdss_dsi0_pll: Failed to create 5e94400.qcom,mdss_dsi0_pll debugfs directory
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi0_pll
6,359,8682306,-;dsi_pll_clock_register_14nm: Registered DSI PLL ndx=0 clocks successfully
6,360,8691409,-;NET: Registered protocol family 2
6,361,8697472,-;tcp_listen_portaddr_hash hash table entries: 2048 (order: 4, 81920 bytes)
6,362,8705524,-;TCP established hash table entries: 32768 (order: 6, 262144 bytes)
6,363,8713331,-;TCP bind hash table entries: 32768 (order: 8, 1048576 bytes)
6,364,8720422,-;TCP: Hash tables configured (established 32768 bind 32768)
6,365,8727925,-;UDP hash table entries: 2048 (order: 5, 196608 bytes)
6,366,8734309,-;UDP-Lite hash table entries: 2048 (order: 5, 196608 bytes)
6,367,8741957,-;NET: Registered protocol family 1
5,368,8751684,-;arm-smmu c600000.apps-smmu: \x09non-coherent table walk
 SUBSYSTEM=platform
 DEVICE=+platform:c600000.apps-smmu
5,369,8757697,-;arm-smmu c600000.apps-smmu: \x09(IDR0.CTTW overridden by FW configuration)
 SUBSYSTEM=platform
 DEVICE=+platform:c600000.apps-smmu
5,370,8765421,-;arm-smmu c600000.apps-smmu: \x09stream matching with 50 register groups
 SUBSYSTEM=platform
 DEVICE=+platform:c600000.apps-smmu
6,371,8777821,-;qsmmuv500-tbu c789000.mm_rt_tbu: Linked as a consumer to regulator.8
 SUBSYSTEM=platform
 DEVICE=+platform:c789000.mm_rt_tbu
6,372,8787838,-;qsmmuv500-tbu c78d000.mm_nrt_tbu: Linked as a consumer to regulator.9
 SUBSYSTEM=platform
 DEVICE=+platform:c78d000.mm_nrt_tbu
6,373,8797978,-;qsmmuv500-tbu c791000.cdsp_tbu: Linked as a consumer to regulator.7
 SUBSYSTEM=platform
 DEVICE=+platform:c791000.cdsp_tbu
6,374,8807006,-;ipa soc:ipa_smmu_ap: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:ipa_smmu_ap
6,375,8822736,-;iommu: Adding device soc:ipa_smmu_ap to group 0
3,376,8829403,-;ipa: get resource failed for ipa-hw-ver!
6,377,8834786,-;ipa soc:ipa_smmu_wlan: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:ipa_smmu_wlan
6,378,8842942,-;iommu: Adding device soc:ipa_smmu_wlan to group 1
3,379,8849700,-;ipa: get resource failed for ipa-hw-ver!
6,380,8855096,-;ipa soc:ipa_smmu_uc: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:ipa_smmu_uc
6,381,8862952,-;iommu: Adding device soc:ipa_smmu_uc to group 2
3,382,8869534,-;ipa: get resource failed for ipa-hw-ver!
6,383,8874844,-;qupv3_geni_se 4ac0000.qcom,qupv3_0_geni_se: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:4ac0000.qcom,qupv3_0_geni_se
6,384,8896227,-;iommu: Adding device 4ac0000.qcom,qupv3_0_geni_se to group 3
6,385,8905544,-;Trying to unpack rootfs image as initramfs...
6,386,8944595,-;Freeing initrd memory: 1260K
6,387,8951731,-;hw perfevents: enabled with armv8_pmuv3 PMU driver, 7 counters available
6,388,8961826,-;cryptomgr_test (113) used greatest stack depth: 14592 bytes left
6,389,8969197,-;cryptomgr_test (117) used greatest stack depth: 14400 bytes left
5,390,8998105,-;Initialise system trusted keyrings
6,391,9003295,-;workingset: timestamp_bits=45 max_order=20 bucket_order=0
6,392,9074764,-;Registering sdcardfs 0.1
6,393,9080577,-;fuse init (API version 7.27)
6,394,9113565,-;cryptomgr_test (179) used greatest stack depth: 14272 bytes left
5,395,9117505,-;Key type asymmetric registered
5,396,9124748,-;Asymmetric key parser 'x509' registered
6,397,9129706,-;io scheduler noop registered
6,398,9134615,-;io scheduler cfq registered (default)
6,399,9139348,-;io scheduler mq-deadline registered
6,400,9143888,-;io scheduler kyber registered
6,401,9149079,-;io scheduler bfq registered
6,402,9188358,-;gpi_dma 4a00000.qcom,gpi-dma: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:4a00000.qcom,gpi-dma
6,403,9197150,-;iommu: Adding device 4a00000.qcom,gpi-dma to group 4
6,404,9223891,-;gladiator_error_reporting f100000.qcom,msm-gladiator-v2: MSM Gladiator Error Reporting Initialized
 SUBSYSTEM=platform
 DEVICE=+platform:f100000.qcom,msm-gladiator-v2
6,405,9236068,-;subsys-pil-tz ab00000.qcom,lpass: Linked as a consumer to regulator.24
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,406,9243982,-;subsys-pil-tz ab00000.qcom,lpass: Linked as a consumer to regulator.23
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,407,9257226,-;subsys-pil-tz b300000.qcom,turing: Linked as a consumer to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
6,408,9269545,-;subsys-pil-tz 5ab0000.qcom,venus: Linked as a consumer to regulator.5
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
3,409,9277688,-;minidump-id not found for venus
6,410,9282255,-;subsys-pil-tz 5ab0000.qcom,venus: for venus segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
6,411,9290840,-;subsys-pil-tz 5ab0000.qcom,venus: for md_venus segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
6,412,9300532,-;subsys-pil-tz 6080000.qcom,mss: Linked as a consumer to regulator.13
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
3,413,9312762,-;minidump-id not found for ipa_fws
6,414,9317560,-;subsys-pil-tz soc:qcom,ipa_fws: for ipa_fws segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ipa_fws
6,415,9325661,-;subsys-pil-tz soc:qcom,ipa_fws: for md_ipa_fws segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,ipa_fws
3,416,9335365,-;minidump-id not found for a610_zap
6,417,9340217,-;subsys-pil-tz soc:qcom,kgsl-hyp: for a610_zap segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,kgsl-hyp
6,418,9348582,-;subsys-pil-tz soc:qcom,kgsl-hyp: for md_a610_zap segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,kgsl-hyp
6,419,9364471,-;memshare_child soc:qcom,memshare:qcom,client_1: for memshare_GPS segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare:qcom,client_1
6,420,9374754,-;memshare_child soc:qcom,memshare:qcom,client_2: for memshare_FTM segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare:qcom,client_2
6,421,9384947,-;memshare_child soc:qcom,memshare:qcom,client_3: for memshare_DIAG segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare:qcom,client_3
6,422,9420951,-;icnss c800000.qcom,icnss: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,423,9430076,-;iommu: Adding device c800000.qcom,icnss to group 5
6,424,9436893,-;icnss: Recursive recovery allowed for WLAN
6,425,9442447,-;icnss c800000.qcom,icnss: Linked as a consumer to regulator.29
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,426,9449722,-;icnss c800000.qcom,icnss: Linked as a consumer to regulator.37
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,427,9457014,-;icnss c800000.qcom,icnss: Linked as a consumer to regulator.38
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,428,9464438,-;icnss c800000.qcom,icnss: Linked as a consumer to regulator.44
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,429,9471918,-;icnss c800000.qcom,icnss: for wcss_msa0 segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,430,9480748,-;icnss: Platform driver probed successfully
6,431,9495656,-;msm_geni_serial 4a90000.qcom,qup_uart: Serial port0 added.FifoSize 64 is_console1
 SUBSYSTEM=platform
 DEVICE=+platform:4a90000.qcom,qup_uart
6,432,9504880,-;4a90000.qcom,qup_uart: ttyMSM0 at MMIO 0x4a90000 (irq = 142, base_baud = 0) is a MSM
6,433,9528200,-;console [ttyMSM0] enabled
6,434,9535559,-;bootconsole [msm_geni_serial0] disabled
6,435,9549305,-;msm_geni_serial 4a8c000.qcom,qup_uart: Wakeup byte 0xfd
 SUBSYSTEM=platform
 DEVICE=+platform:4a8c000.qcom,qup_uart
6,436,9556758,-;msm_geni_serial 4a8c000.qcom,qup_uart: Serial port0 added.FifoSize 64 is_console0
 SUBSYSTEM=platform
 DEVICE=+platform:4a8c000.qcom,qup_uart
6,437,9571551,-;4a8c000.qcom,qup_uart: ttyHS0 at MMIO 0x4a8c000 (irq = 143, base_baud = 0) is a MSM
6,438,9582908,-;msm_geni_serial_init: Driver initialized
5,439,9596936,-;random: crng init done
6,440,9642047,-;iommu-debug soc:kgsl_iommu_test_device: Linked as a consumer to 59a0000.kgsl-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:kgsl_iommu_test_device
6,441,9651248,-;iommu: Adding device soc:kgsl_iommu_test_device to group 6
6,442,9659719,-;iommu-debug soc:apps_iommu_test_device: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:apps_iommu_test_device
6,443,9668756,-;iommu: Adding device soc:apps_iommu_test_device to group 7
6,444,9676856,-;iommu-debug soc:apps_iommu_coherent_test_device: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:apps_iommu_coherent_test_device
6,445,9686465,-;iommu: Adding device soc:apps_iommu_coherent_test_device to group 8
6,446,9757601,-;brd: module loaded
6,447,9870118,-;loop: module loaded
6,448,9875683,-;zram: Added device: zram0
6,449,9880877,-;QSEECOM: qseecom_init_control: qseecom.qsee_version = 0x1402000
4,450,9887979,-;QSEECOM: qseecom_retrieve_ce_data: Device does not support PFE
6,451,9908295,-;qce 1b20000.qcedev: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:1b20000.qcedev
6,452,9916525,-;iommu: Adding device 1b20000.qcedev to group 9
6,453,9929905,-;qce 1b20000.qcedev: QTI Crypto 5.5.1 device found @0x1b20000
 SUBSYSTEM=platform
 DEVICE=+platform:1b20000.qcedev
6,454,9938679,-;sps:BAM 0x0000000001b04000 is registered.
6,455,9939310,-;sps:BAM 0x0000000001b04000 (va:0xffffff8013ec0000) enabled: ver:0x27, number of pipes:16
6,456,9954430,-;QCE50: qce_sps_init:  QTI MSM CE-BAM at 0x0000000001b04000 irq 14
6,457,9966866,-;qce 1b20000.qcedev:qcom_cedev_ns_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:1b20000.qcedev:qcom_cedev_ns_cb
6,458,9976538,-;iommu: Adding device 1b20000.qcedev:qcom_cedev_ns_cb to group 10
6,459,9986415,-;qce 1b20000.qcedev:qcom_cedev_s_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:1b20000.qcedev:qcom_cedev_s_cb
6,460,9996713,-;iommu: Adding device 1b20000.qcedev:qcom_cedev_s_cb to group 11
3,461,10009259,-;Error: Driver 'qcrypto' is already registered, aborting...
6,462,10020769,-;ufshcd-qcom 4804000.ufshc: ufshcd_populate_vreg: Unable to find vccq-supply regulator, assuming enabled
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
4,463,10031338,-;ufshcd-qcom 4804000.ufshc: no vccq2-voltage-level property.
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,464,10038921,-;ufshcd-qcom 4804000.ufshc: Linked as a consumer to regulator.2
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,465,10046979,-;ufshcd-qcom 4804000.ufshc: Linked as a consumer to regulator.45
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,466,10054351,-;ufshcd-qcom 4804000.ufshc: Linked as a consumer to regulator.32
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,467,10066206,-;ufshcd-qcom 4804000.ufshc: Linked as a consumer to regulator.39
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,468,10073848,-;ufs_qcom_phy_qmp_v3_660 4807000.ufsphy_mem: Linked as a consumer to regulator.33
 SUBSYSTEM=platform
 DEVICE=+platform:4807000.ufsphy_mem
6,469,10082670,-;ufs_qcom_phy_qmp_v3_660 4807000.ufsphy_mem: Linked as a consumer to regulator.25
 SUBSYSTEM=platform
 DEVICE=+platform:4807000.ufsphy_mem
6,470,10091755,-;ufshcd-qcom 4804000.ufshc: ufs_qcom_parse_reg_info: Unable to find qcom,vccq-parent-supply regulator, assuming enabled
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,471,10108917,-;scsi host0: ufshcd
 SUBSYSTEM=scsi
 DEVICE=+scsi:host0
6,472,10145937,-;SCSI Media Changer driver v0.25 
6,473,10153144,-;Ethernet Channel Bonding Driver: v3.7.1 (April 27, 2011)
3,474,10156168,-;ufshcd-qcom 4804000.ufshc: ufshcd_print_pwr_info:[RX, TX]: gear=[1, 1], lane[1, 1], pwr[SLOWAUTO_MODE, SLOWAUTO_MODE], rate = 0
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,475,10172698,-;libphy: Fixed MDIO Bus: probed
6,476,10176818,-;tun: Universal TUN/TAP device driver, 1.6
6,477,10182348,-;PPP generic driver version 2.4.2
6,478,10186974,-;PPP BSD Compression module registered
6,479,10191765,-;PPP Deflate Compression module registered
6,480,10196898,-;PPP MPPE Compression module registered
6,481,10201734,-;NET: Registered protocol family 24
6,482,10206336,-;PPTP driver version 0.8.5
6,483,10213387,-;CLD80211: Initializing
6,484,10217786,-;usbcore: registered new interface driver r8152
6,485,10246717,-;msm_sharedmem: msm_sharedmem_probe: Device created for client 'rmtfs'
4,486,10260501,-;msm-qusb-phy 1613000.qusb: 1613000.qusb supply USB3_GDSC not found, using dummy regulator
 SUBSYSTEM=platform
 DEVICE=+platform:1613000.qusb
6,487,10270222,-;msm-qusb-phy 1613000.qusb: Linked as a consumer to regulator.0
 SUBSYSTEM=platform
 DEVICE=+platform:1613000.qusb
3,488,10273467,-;ufshcd-qcom 4804000.ufshc: ufshcd_print_pwr_info:[RX, TX]: gear=[3, 3], lane[1, 1], pwr[FAST MODE, FAST MODE], rate = 2
 SUBSYSTEM=platform
 DEVICE=+platform:4804000.ufshc
6,489,10277532,-;msm-qusb-phy 1613000.qusb: Linked as a consumer to regulator.25
 SUBSYSTEM=platform
 DEVICE=+platform:1613000.qusb
5,490,10292305,-;scsi 0:0:0:49488: Well-known LUN    SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:49488
6,491,10296298,-;msm-qusb-phy 1613000.qusb: Linked as a consumer to regulator.36
 SUBSYSTEM=platform
 DEVICE=+platform:1613000.qusb
6,492,10311840,-;msm-qusb-phy 1613000.qusb: Linked as a consumer to regulator.33
 SUBSYSTEM=platform
 DEVICE=+platform:1613000.qusb
5,493,10323969,-;scsi 0:0:0:49476: Well-known LUN    SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:49476
6,494,10325120,-;msm-usb-ssphy-qmp 1615000.ssphy: Linked as a consumer to regulator.25
 SUBSYSTEM=platform
 DEVICE=+platform:1615000.ssphy
6,495,10340416,-;msm-usb-ssphy-qmp 1615000.ssphy: Linked as a consumer to regulator.33
 SUBSYSTEM=platform
 DEVICE=+platform:1615000.ssphy
5,496,10350405,-;scsi 0:0:0:49456: Well-known LUN    SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:49456
6,497,10353428,-;msm-dwc3 4e00000.ssusb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
6,498,10367528,-;iommu: Adding device 4e00000.ssusb to group 12
5,499,10370936,-;scsi 0:0:0:0: Direct-Access     SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:0
6,500,10374705,-;msm-dwc3 4e00000.ssusb: Linked as a consumer to regulator.3
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
5,501,10383454,-;scsi 0:0:0:1: Direct-Access     SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:1
3,502,10392719,-;dwc3 4e00000.dwc3: Failed to get clk 'ref': -2
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.dwc3
5,503,10398168,-;scsi 0:0:0:2: Direct-Access     SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:2
6,504,10402237,-;dwc3 4e00000.dwc3: changing max_speed on rev 00000000
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.dwc3
5,505,10411644,-;scsi 0:0:0:3: Direct-Access     SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:3
5,506,10426114,-;scsi 0:0:0:4: Direct-Access     SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:4
5,507,10441274,-;scsi 0:0:0:5: Direct-Access     SAMSUNG  KM5C7001DM-B622  0200 PQ: 0 ANSI: 6
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:5
3,508,10441506,-;Invalid index Defaulting curr to 0
4,509,10453657,-;sd 0:0:0:0: Power-on or device reset occurred
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:0
6,510,10454561,-;msm-dwc3 4e00000.ssusb: Dropping the link to regulator.3
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
5,511,10461008,-;sd 0:0:0:0: [sda] Write Protect is off
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:0
4,512,10465036,-;sd 0:0:0:1: Power-on or device reset occurred
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:1
6,513,10468979,-;usbcore: registered new interface driver usb-storage
6,514,10469154,-;usbcore: registered new interface driver usb_ehset_test
6,515,10469258,-;usbcore: registered new interface driver lvs
7,516,10470244,-;sd 0:0:0:0: [sda] Mode Sense: 00 32 00 10
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:0
6,517,10473019,-;usbcore: registered new interface driver xpad
4,518,10475337,-;sd 0:0:0:2: Power-on or device reset occurred
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:2
6,519,10476361,-;input: hall_switch as /devices/platform/soc/soc:hall_switch/input/input1
4,520,10478343,-;genirq: irq_chip msmgpio did not update eff. affinity mask of irq 213
6,521,10479670,-;hall_switch soc:hall_switch: Linked as a consumer to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:soc:hall_switch
6,522,10485191,-;rtc-pm8xxx 1c40000.qcom,spmi:qcom,pm6125@0:qcom,pm6125_rtc: rtc core: registered pm8xxx_rtc as rtc0
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pm6125@0:qcom,pm6125_rtc
4,523,10487188,-;sd 0:0:0:4: Power-on or device reset occurred
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:4
6,524,10492978,-;rtc-pm8xxx 1c40000.qcom,spmi:qcom,pm6125@0:qcom,pm6125_rtc: setting system clock to 1970-01-01 01:24:44 UTC (5084)
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pm6125@0:qcom,pm6125_rtc
4,525,10498392,-;sd 0:0:0:5: Power-on or device reset occurred
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:5
6,526,10504689,-;i2c /dev entries driver
4,527,10509809,-;sd 0:0:0:3: Power-on or device reset occurred
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:3
6,528,10519612,-;i2c_geni 4a84000.i2c: Bus frequency is set to 400000Hz
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
6,529,10525693,-;sd 0:0:0:0: [sda] Optimal transfer size 8192 bytes
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:0
5,530,10527076,-;sd 0:0:0:1: [sdb] Write Protect is off
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:1
7,531,10527111,-;sd 0:0:0:1: [sdb] Mode Sense: 00 32 00 10
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:1
5,532,10528241,-;sd 0:0:0:2: [sdc] Write Protect is off
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:2
7,533,10528261,-;sd 0:0:0:2: [sdc] Mode Sense: 00 32 00 10
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:2
6,534,10528676,-;sd 0:0:0:1: [sdb] Optimal transfer size 8192 bytes
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:1
5,535,10529081,-;sd 0:0:0:3: [sdd] Write Protect is off
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:3
7,536,10529111,-;sd 0:0:0:3: [sdd] Mode Sense: 00 32 00 10
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:3
6,537,10529139,-;sd 0:0:0:2: [sdc] Optimal transfer size 8192 bytes
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:2
5,538,10529291,-;sd 0:0:0:4: [sde] Write Protect is off
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:4
7,539,10529318,-;sd 0:0:0:4: [sde] Mode Sense: 00 32 00 10
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:4
6,540,10529993,-;sd 0:0:0:3: [sdd] Optimal transfer size 8192 bytes
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:3
6,541,10532226,-;sd 0:0:0:4: [sde] Optimal transfer size 8192 bytes
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:4
5,542,10533420,-;sd 0:0:0:5: [sdf] Write Protect is off
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:5
7,543,10533451,-;sd 0:0:0:5: [sdf] Mode Sense: 00 32 00 10
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:5
6,544,10534432,-;sd 0:0:0:5: [sdf] Optimal transfer size 8192 bytes
 SUBSYSTEM=scsi
 DEVICE=+scsi:0:0:0:5
6,545,10536342,-; sdc: sdc1 sdc2
6,546,10547021,-; sdd: sdd1 sdd2 sdd3
6,547,10547195,-; sdb: sdb1 sdb2
6,548,10549699,-;PMIC@SID0: PM8008 v1.0 options: 0, 0, 0, 0
6,549,10553216,-; sda: sda1 sda2 sda3 sda4 sda5 sda6 sda7 sda8 sda9 sda10 sda11 sda12 sda13 sda14 sda15 sda16 sda17 sda18 sda19 sda20 sda21 sda22 sda23 sda24 sda25 sda26 sda27 sda28 sda29 sda30 sda31
6,550,10555599,-; sdf: sdf1 sdf2 sdf3 sdf4 sdf5
6,551,10556278,-; sde: sde1 sde2 sde3 sde4 sde5 sde6 sde7 sde8 sde9 sde10 sde11 sde12 sde13 sde14 sde15 sde16 sde17 sde18 sde19 sde20 sde21 sde22 sde23 sde24 sde25 sde26 sde27 sde28 sde29 sde30 sde31 sde32 sde33 sde34 sde35 sde36 sde37 sde38 sde39 sde40 sde41 sde42 sde43 sde44 sde45 sde46 sde47 sde48 sde49 sde50 sde51 sde52 sde53 sde54 sde55 sde56 sde57 sde58
6,552,10716910,-;I2C PMIC: i2c_pmic_probe: I2C PMIC probe successful
6,553,10729987,-;qcom,pm8008-regulator 4a84000.i2c:qcom,pm8008@9:qcom,pm8008-regulator: Linked as a consumer to regulator.19
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c:qcom,pm8008@9:qcom,pm8008-regulator
6,554,10741239,-;qcom,pm8008-regulator 4a84000.i2c:qcom,pm8008@9:qcom,pm8008-regulator: Linked as a consumer to regulator.49
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c:qcom,pm8008@9:qcom,pm8008-regulator
6,555,10768356,-;pm8008_l5: Bringing 1800000uV into 2800000-2800000uV
6,556,10783650,-;pm8008_l7: Bringing 2800000uV into 1800000-1800000uV
6,557,10793834,-;I2C PMIC: i2c_pmic_probe: I2C PMIC probe successful
4,558,10803049,-;pca953x 0-0020: 0-0020 supply vcc not found, using dummy regulator
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0020
4,559,10806278,-;nq-nci 0-0028: ese GPIO <OPTIONAL> error getting from OF node
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
6,560,10810725,-;pca953x 0-0020: Linked as a consumer to regulator.0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0020
3,561,10817205,-;nq-nci 0-0028: error reading NFC VDDIO min and max value
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
3,562,10829844,-;nq-nci 0-0028: error reading NFC current value
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
4,563,10831453,-;pca953x 0-0020: interrupt support not compiled in
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0020
3,564,10835559,-;nq-nci 0-0028: nqx_probe: ese gpio not provided
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
6,565,10843807,-;at24 0-0050: 8192 byte 24c64 EEPROM, writable, 32 bytes/write
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0050
3,566,10847547,-;nq-nci 0-0028: nfc_ldo_config: regulator entry not present
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
6,567,10855285,-;i2c_geni 4a88000.i2c: Bus frequency is set to 400000Hz
 SUBSYSTEM=platform
 DEVICE=+platform:4a88000.i2c
6,568,10871498,-;[FTS][Info]display x(0 720) y(0 1280)
6,569,10876233,-;[FTS][Info]VK(1): (256, 0, 0), [540, 0, 0][1580]
6,570,10882111,-;[FTS][Info]max touch number:3, irq gpio:1247, reset gpio:1238
6,571,10890120,-;[FTS][Info]set key capabilities
6,572,10894955,-;input: focaltech as /devices/platform/soc/4a88000.i2c/i2c-1/1-0038/input/input2
3,573,10904910,-;[FTS][Error]Pin state[release] not found
6,574,10912484,-;[FTS][Info]get ic information, chip id = 0x8006
6,575,10918123,-;[FTS][Info]Create proc entry success!
6,576,10922960,-;[FTS][Info][EX]: sysfs_create_group() succeeded!!
3,577,10926354,-;nq-nci 0-0028: nqx_probe: probing NFCC NQxxx exited successfully
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
6,578,10928787,-;[FTS][Info]irq in ts_data:220 irq in client:220
6,579,10941439,-;[FTS][Info]irq flag:1
6,580,10945615,-;[FTS][Info]fw upgrade init function
6,581,10950267,-;[FTS][Info]fw upgrade work function
6,582,10954846,-;[FTS][Info]get upgrade fw file
3,583,10956751,-;max1720x 0-0036: ====================>> max1720x_probe, addr=0x36
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,584,10959004,-;[FTS][Info]upgrade fw file len:0
3,585,10966163,-;max1720x 0-0036: ====================>> VER.1.01.001-20181122
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,586,10970471,-;[FTS][Error]fw file len(0) fail
3,587,10970860,-;[FTS][Error]get file fail, can't upgrade
3,588,10981215,-;max1720x 0-0036: -------- jcount=6 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,589,10991863,-;max1720x 0-0036: -------- j=0 target=FFF0 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,590,11002034,-;max1720x 0-0036: -------- j=1 target=FFF9 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,591,11013012,-;max1720x 0-0036: -------- j=2 target=0400 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,592,11019236,-;max1720x 0-0036: -------- j=3 target=FFF0 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,593,11029425,-;max1720x 0-0036: -------- j=4 target=0001 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,594,11035626,-;max1720x 0-0036: -------- j=5 target=0000 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,595,11041499,-;max1720x 0-0036: -------- DesginCap=3840 mAh--------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,596,11049338,-;max1720x 0-0036: -------- SN=0x5588 --------
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,597,11055391,-;max1720x 0-0036: === check profile = 0x00000000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,598,11061001,-;max1720x 0-0036: === flag_LOCK_NV_PAGES=0x0000h, flag_UPD_BY_FW_VER=0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,599,11072947,-;max1720x 0-0036: case 5 === SN=TWMX2049505588
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,600,11079201,-;max1720x 0-0036: ====== max1720x(fg-fw ver=0002) probe Success
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,601,11088536,-;Couldn't parse device tree rc=-517
6,602,11092547,-;max1720x 0-0036: case 5 === SN=TWMX2049505588
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,603,11099992,-;ads1015 0-0048: mode is 0, channel is 4
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
4,604,11105028,-;ads1015 0-0048: hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,605,11106483,-;max1720x 0-0036: SOC routine soc(51) pre_soc(0)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,606,11117634,-;ads1015 0-0048: config ads1015 in continous, compare mode
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,607,11122762,-;max1720x 0-0036: Booting first time or resume
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,608,11129849,-;ads1015 0-0048: config mode is 0x4288, read mode is 0x4288
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,609,11134665,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,610,11141833,-;ads1015 0-0048: threshold register config value is 0x3519, read value is 0x3519
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
6,611,11156308,-;ads1015 0-0048: threshold register config value is 0x2eda, read value is 0x2eda
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
6,612,11167093,-; hon-accessory: no dock detect pin supported
6,613,11173220,-; hon-accessory: Adding honacc_trigger- type:0 gpio:1251 irq:221 flags:3
6,614,11181405,-; hon-accessory: Adding honacc_trigger- type:0 gpio:1233 irq:222 flags:3
6,615,11189421,-; not_connected: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,616,11197738,-; not_connected: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,617,11206055,-; not_connected: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,618,11214291,-; hon-accessory: Adding honacc_state - index:0 label:not_connected min:100 max:340 input_current_limit:0 charge_current_limit=0
6,619,11227060,-; EBase: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:1
6,620,11234741,-; EBase: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:1
6,621,11242397,-; EBase: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,622,11249962,-; EBase: Adding honacc_action - type:1 gpio:0 notify_num:8 enable:1
6,623,11257209,-; hon-accessory: Adding honacc_state - index:1 label:EBase min:341 max:460 input_current_limit:0 charge_current_limit=0
6,624,11269427,-; 4-bay_net_base: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:1
6,625,11277830,-; 4-bay_net_base: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:1
6,626,11286244,-; 4-bay_net_base: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,627,11294589,-; 4-bay_net_base: Adding honacc_action - type:1 gpio:0 notify_num:2 enable:1
6,628,11302652,-; 4-bay_net_base: Adding honacc_action - type:1 gpio:0 notify_num:8 enable:1
6,629,11310715,-; hon-accessory: Adding honacc_state - index:2 label:4-bay_net_base min:461 max:580 input_current_limit:0 charge_current_limit=0
6,630,11323560,-; 30_bay_charge_rack: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,631,11332336,-; 30_bay_charge_rack: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,632,11341081,-; 30_bay_charge_rack: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,633,11349757,-; hon-accessory: Adding honacc_state - index:3 label:30_bay_charge_rack min:581 max:700 input_current_limit:0 charge_current_limit=0
6,634,11362884,-; V-Dock: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:1
6,635,11370605,-; V-Dock: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:1
6,636,11378286,-; V-Dock: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,637,11385885,-; V-Dock: Adding honacc_action - type:1 gpio:0 notify_num:8 enable:1
6,638,11393258,-; hon-accessory: Adding honacc_state - index:4 label:V-Dock min:701 max:820 input_current_limit:0 charge_current_limit=0
6,639,11405566,-; Display_Dock: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:1
6,640,11413846,-; Display_Dock: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:1
6,641,11422108,-; Display_Dock: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,642,11430284,-; Display_Dock: Adding honacc_action - type:1 gpio:0 notify_num:8 enable:1
6,643,11438155,-; hon-accessory: Adding honacc_state - index:5 label:Display_Dock min:821 max:940 input_current_limit:0 charge_current_limit=0
6,644,11450929,-; USB-CUP: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,645,11458747,-; USB-CUP: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,646,11466536,-; USB-CUP: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,647,11474255,-; hon-accessory: Adding honacc_state - index:6 label:USB-CUP min:941 max:1060 input_current_limit:0 charge_current_limit=0
6,648,11486592,-; TBD7: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,649,11494157,-; TBD7: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,650,11501700,-; TBD7: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,651,11509157,-; hon-accessory: Adding honacc_state - index:7 label:TBD7 min:1061 max:1180 input_current_limit:0 charge_current_limit=0
6,652,11521242,-; EPop_Lop: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:1
6,653,11529143,-; EPop_Lop: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:1
6,654,11536990,-; EPop_Lop: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,655,11544782,-; EPop_Lop: Adding honacc_action - type:1 gpio:0 notify_num:8 enable:1
6,656,11552324,-; hon-accessory: Adding honacc_state - index:8 label:EPop_Lop min:1181 max:1300 input_current_limit:0 charge_current_limit=0
6,657,11564840,-; TBD9: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,658,11572379,-; TBD9: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,659,11579884,-; TBD9: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,660,11587301,-; hon-accessory: Adding honacc_state - index:9 label:TBD9 min:1301 max:1420 input_current_limit:0 charge_current_limit=0
6,661,11599523,-; HB: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,662,11606903,-; HB: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,663,11614316,-; HB: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,664,11621581,-; hon-accessory: Adding honacc_state - index:10 label:HB min:1421 max:1540 input_current_limit:0 charge_current_limit=0
6,665,11633699,-; HBase: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,666,11641341,-; HBase: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,667,11648998,-; HBase: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,668,11656502,-; hon-accessory: Adding honacc_state - index:11 label:HBase min:1541 max:1660 input_current_limit:0 charge_current_limit=1000000
6,669,11669315,-; otgcup: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:1
6,670,11677010,-; otgcup: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:1
6,671,11684714,-; otgcup: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:1
6,672,11692346,-; hon-accessory: Adding honacc_state - index:12 label:otgcup min:0 max:30 input_current_limit:0 charge_current_limit=0
6,673,11704370,-; usbcup: Adding honacc_action - type:0 gpio:1274 notify_num:0 enable:0
6,674,11712083,-; usbcup: Adding honacc_action - type:0 gpio:1226 notify_num:0 enable:0
6,675,11719769,-; usbcup: Adding honacc_action - type:0 gpio:1275 notify_num:0 enable:0
6,676,11727364,-; hon-accessory: Adding honacc_state - index:13 label:usbcup min:31 max:99 input_current_limit:0 charge_current_limit=0
6,677,11739168,-; hon-accessory: vadc_channel is 4, debounce_time is 2000, detect_delay is 80, \x09\x09deter_pop_time is 100, debounce_interval is 0
6,678,11752134,-; hon-accessory: honacc_choose_state_by_label, label is not_connected
6,679,11759569,-; hon-accessory: honacc_force_trigger, force trigger
6,680,11802130,-;reg-cooling-device soc:qcom,rpm-smd:rpm-regulator-smpa3:cx-cdev-lvl: Linked as a consumer to regulator.14
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,rpm-smd:rpm-regulator-smpa3:cx-cdev-lvl
6,681,11814588,-;reg-cooling-device soc:qcom,rpm-smd:rpm-regulator-smpa5:mx-cdev-lvl: Linked as a consumer to regulator.16
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,rpm-smd:rpm-regulator-smpa5:mx-cdev-lvl
6,682,11843628,-;device-mapper: uevent: version 1.0.3
6,683,11849965,-;device-mapper: ioctl: 4.39.0-ioctl (2018-04-03) initialised: dm-devel@redhat.com
6,684,11861001,-;bt_power_populate_dt_pinfo: bt-reset-gpio not provided in devicetree
6,685,11868551,-;bt_power_populate_dt_pinfo: wl-reset-gpio not provided in devicetree
6,686,11876204,-;bt_dt_parse_vreg_info: qca,bt-vdd-ldo: is not provided in device tree
6,687,11883729,-;bt_dt_parse_vreg_info: qca,bt-chip-pwd: is not provided in device tree
6,688,11891369,-;bt_dt_parse_vreg_info: qca,bt-vdd-aon: is not provided in device tree
6,689,11898893,-;bt_dt_parse_vreg_info: qca,bt-vdd-dig: is not provided in device tree
6,690,11906402,-;bt_dt_parse_vreg_info: qca,bt-vdd-rfa1: is not provided in device tree
6,691,11914036,-;bt_dt_parse_vreg_info: qca,bt-vdd-rfa2: is not provided in device tree
6,692,11921644,-;bt_dt_parse_vreg_info: qca,bt-vdd-asd: is not provided in device tree
6,693,11929222,-;bt_dt_parse_clk_info: clocks is not provided in device tree
6,694,11943649,-;sdhci: Secure Digital Host Controller Interface driver
6,695,11949950,-;sdhci: Copyright(c) Pierre Ossman
6,696,11954331,-;sdhci-pltfm: SDHCI platform and OF driver helper
3,697,11972843,-;sdhci_msm 4784000.sdhci: core_reset unavailable,err = -2
 SUBSYSTEM=platform
 DEVICE=+platform:4784000.sdhci
6,698,11976435,-;qpnp_vibrator_ldo_probe: Vibrator LDO successfully registered: uV = 3000000, overdrive = disabled
3,699,11979309,-;sdhci_msm 4784000.sdhci: Reset data parsing error
 SUBSYSTEM=platform
 DEVICE=+platform:4784000.sdhci
6,700,11993180,-;usbcore: registered new interface driver usbhid
6,701,12000762,-;usbhid: USB HID core driver
6,702,12001689,-;sdhci_msm 4784000.sdhci: Linked as a consumer to regulator.43
 SUBSYSTEM=platform
 DEVICE=+platform:4784000.sdhci
6,703,12011576,-;ashmem: initialized
6,704,12011981,-;sdhci_msm 4784000.sdhci: Linked as a consumer to regulator.26
 SUBSYSTEM=platform
 DEVICE=+platform:4784000.sdhci
6,705,12014750,-;ipa_ut ipa_ut_module_init:1036 Loading IPA test module...
6,706,12021975,-;sdhci_msm 4784000.sdhci: Linked as a consumer to regulator.28
 SUBSYSTEM=platform
 DEVICE=+platform:4784000.sdhci
3,707,12028023,-;ipa_get_ipc_logbuf:3437 IPA HW is not supported
3,708,12040423,-;ipa_get_ipc_logbuf_low:3450 IPA HW is not supported
3,709,12046380,-;ipa_get_ipc_logbuf:3437 IPA HW is not supported
6,710,12048787,-;mmc0: SDHCI controller on 4784000.sdhci [4784000.sdhci] using 64-bit ADMA in legacy mode
3,711,12051995,-;ipa_get_ipc_logbuf_low:3450 IPA HW is not supported
3,712,12067081,-;ipa_register_ipa_ready_cb:3294 IPA HW is not supported
3,713,12073299,-;ipa_ut ipa_ut_module_init:1075 IPA CB reg failed - -1
3,714,12079429,-;ipa_get_ipc_logbuf:3437 IPA HW is not supported
3,715,12085029,-;ipa_get_ipc_logbuf_low:3450 IPA HW is not supported
6,716,12094646,-;bimc-bwmon 1b8e300.qcom,cpu-cpu-ddr-bwmon: BW HWmon governor registered.
 SUBSYSTEM=platform
 DEVICE=+platform:1b8e300.qcom,cpu-cpu-ddr-bwmon
6,717,12107335,-;arm-memlat-mon soc:qcom,cpu0-cpugrp:qcom,cpu0-cpu-ddr-latmon: Memory Latency governor registered.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cpu0-cpugrp:qcom,cpu0-cpu-ddr-latmon
6,718,12118721,-;arm-memlat-mon soc:qcom,cpu0-cpugrp:qcom,cpu0-computemon: Compute governor registered.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cpu0-cpugrp:qcom,cpu0-computemon
6,719,12129141,-;arm-memlat-mon soc:qcom,cpu4-cpugrp:qcom,cpu4-cpu-ddr-latmon: Memory Latency governor registered.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cpu4-cpugrp:qcom,cpu4-cpu-ddr-latmon
6,720,12140273,-;arm-memlat-mon soc:qcom,cpu4-cpugrp:qcom,cpu4-computemon: Compute governor registered.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cpu4-cpugrp:qcom,cpu4-computemon
6,721,12196314,-;[l2 counters error]: Registered L2 cache PMU cluster 0
6,722,12203232,-;[l2 counters error]: Registered L2 cache PMU cluster 1
6,723,12209496,-;l2cache-pmu soc:l2cache_pmu: CPU0 associated with cluster 0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,724,12216262,-;l2cache-pmu soc:l2cache_pmu: CPU1 associated with cluster 0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,725,12222997,-;l2cache-pmu soc:l2cache_pmu: CPU2 associated with cluster 0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,726,12229761,-;l2cache-pmu soc:l2cache_pmu: CPU3 associated with cluster 0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,727,12236440,-;l2cache-pmu soc:l2cache_pmu: CPU4 associated with cluster 1
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,728,12243139,-;l2cache-pmu soc:l2cache_pmu: CPU5 associated with cluster 1
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,729,12249865,-;l2cache-pmu soc:l2cache_pmu: CPU6 associated with cluster 1
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,730,12256543,-;l2cache-pmu soc:l2cache_pmu: CPU7 associated with cluster 1
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
6,731,12263675,-;l2cache-pmu soc:l2cache_pmu: Registered L2 cache PMU using 2 HW PMUs
 SUBSYSTEM=platform
 DEVICE=+platform:soc:l2cache_pmu
3,732,12274247,-;coresight-tmc 8047000.tmc: No csr data
 SUBSYSTEM=amba
 DEVICE=+amba:8047000.tmc
3,733,12279093,-;coresight-tmc 8047000.tmc: invalid cti data
 SUBSYSTEM=amba
 DEVICE=+amba:8047000.tmc
6,734,12285564,-;coresight-tmc 8048000.tmc: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=amba
 DEVICE=+amba:8048000.tmc
6,735,12294052,-;iommu: Adding device 8048000.tmc to group 13
6,736,12318352,-;coresight-etm4x 9040000.etm: CPU0: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9040000.etm
6,737,12324649,-;coresight-etm4x 9040000.etm: CPU0: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9040000.etm
6,738,12333278,-;coresight-etm4x 9140000.etm: CPU1: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9140000.etm
6,739,12339593,-;coresight-etm4x 9140000.etm: CPU1: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9140000.etm
6,740,12348306,-;coresight-etm4x 9240000.etm: CPU2: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9240000.etm
6,741,12354601,-;coresight-etm4x 9240000.etm: CPU2: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9240000.etm
6,742,12363287,-;coresight-etm4x 9340000.etm: CPU3: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9340000.etm
6,743,12369621,-;coresight-etm4x 9340000.etm: CPU3: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9340000.etm
6,744,12378255,-;coresight-etm4x 9440000.etm: CPU4: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9440000.etm
6,745,12384549,-;coresight-etm4x 9440000.etm: CPU4: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9440000.etm
6,746,12393278,-;coresight-etm4x 9540000.etm: CPU5: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9540000.etm
6,747,12399591,-;coresight-etm4x 9540000.etm: CPU5: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9540000.etm
6,748,12408273,-;coresight-etm4x 9640000.etm: CPU6: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9640000.etm
6,749,12414568,-;coresight-etm4x 9640000.etm: CPU6: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9640000.etm
6,750,12423256,-;coresight-etm4x 9740000.etm: CPU7: ETM v0.4 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9740000.etm
6,751,12429589,-;coresight-etm4x 9740000.etm: CPU7: (null) initialized
 SUBSYSTEM=amba
 DEVICE=+amba:9740000.etm
6,752,12438856,-;coresight-stm 8002000.stm: stm_register_device failed, probing deffered
 SUBSYSTEM=amba
 DEVICE=+amba:8002000.stm
3,753,12447154,-;OF: graph: no port node found in /soc/cti@8B30000
3,754,12453946,-;OF: graph: no port node found in /soc/cti@98E0000
3,755,12460558,-;OF: graph: no port node found in /soc/cti@98F0000
3,756,12467097,-;OF: graph: no port node found in /soc/cti@8867000
3,757,12473781,-;OF: graph: no port node found in /soc/cti@8833000
3,758,12480536,-;OF: graph: no port node found in /soc/cti@8A02000
3,759,12487250,-;OF: graph: no port node found in /soc/cti@8B59000
3,760,12494035,-;OF: graph: no port node found in /soc/cti@8B5A000
3,761,12500678,-;OF: graph: no port node found in /soc/cti@8B5B000
3,762,12507303,-;OF: graph: no port node found in /soc/cti@8B5C000
3,763,12514106,-;OF: graph: no port node found in /soc/cti@8010000
3,764,12520787,-;OF: graph: no port node found in /soc/cti@8011000
3,765,12527495,-;OF: graph: no port node found in /soc/cti@801a000
3,766,12534187,-;OF: graph: no port node found in /soc/cti@801b000
3,767,12540766,-;OF: graph: no port node found in /soc/cti@801c000
3,768,12547551,-;OF: graph: no port node found in /soc/cti@801d000
3,769,12554293,-;OF: graph: no port node found in /soc/cti@801e000
3,770,12561024,-;OF: graph: no port node found in /soc/cti@801f000
3,771,12567684,-;OF: graph: no port node found in /soc/cti@8012000
3,772,12574347,-;OF: graph: no port node found in /soc/cti@8013000
3,773,12581161,-;OF: graph: no port node found in /soc/cti@8014000
3,774,12587855,-;OF: graph: no port node found in /soc/cti@8015000
3,775,12594535,-;OF: graph: no port node found in /soc/cti@8016000
3,776,12601317,-;OF: graph: no port node found in /soc/cti@8017000
3,777,12607946,-;OF: graph: no port node found in /soc/cti@8018000
3,778,12614684,-;OF: graph: no port node found in /soc/cti@8019000
3,779,12663565,-;OF: graph: no port node found in /soc/csr@8001000
6,780,12669870,-;coresight-csr 8001000.csr: CSR initialized: coresight-csr
 SUBSYSTEM=platform
 DEVICE=+platform:8001000.csr
3,781,12676571,-;OF: graph: no port node found in /soc/csr@8a03000
6,782,12682932,-;coresight-csr 8a03000.csr: CSR initialized: coresight-swao-csr
 SUBSYSTEM=platform
 DEVICE=+platform:8a03000.csr
3,783,12691575,-;OF: graph: no port node found in /soc/hwevent
6,784,12697379,-;coresight-hwevent soc:hwevent: Hardware Event driver initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:hwevent
6,785,12707434,-;coresight-dummy soc:modem_rfxe: Dummy device initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:modem_rfxe
6,786,12715353,-;coresight-dummy soc:snoc: Dummy device initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:snoc
6,787,12722590,-;coresight-dummy soc:tpdm@8a26000: Dummy device initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:tpdm@8a26000
6,788,12730611,-;coresight-dummy soc:tpdm@899c000: Dummy device initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:tpdm@899c000
6,789,12740321,-;coresight-remote-etm soc:audio_etm0: Remote ETM initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:audio_etm0
6,790,12748696,-;coresight-remote-etm soc:turing_etm0: Remote ETM initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:turing_etm0
6,791,12757031,-;coresight-remote-etm soc:modem_etm0: Remote ETM initialized
 SUBSYSTEM=platform
 DEVICE=+platform:soc:modem_etm0
3,792,12764932,-;OF: graph: no port node found in /soc/tgu@9900000
4,793,12777959,-;ENGINE/I hon_engine_init: E
4,794,12783053,-;ENGINE/I hon_engine_get_dt_data: dts illum gpio: 1235
4,795,12789276,-;ENGINE/I hon_engine_get_dt_data: dts aimer gpio: 1242
4,796,12795702,-;ENGINE/I ##Scan Engine probe successfully!!##
4,797,12801686,-;ENGINE/I hon_engine_init: X
6,798,12806313,-;usbcore: registered new interface driver snd-usb-audio
6,799,12813225,-;uaudio-qmi soc:usb_audio_qmi_dev: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:usb_audio_qmi_dev
6,800,12821584,-;iommu: Adding device soc:usb_audio_qmi_dev to group 14
6,801,12843421,-;msm_cam_smmu soc:qcom,cam_smmu:msm_cam_smmu_tfe: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cam_smmu:msm_cam_smmu_tfe
6,802,12853893,-;iommu: Adding device soc:qcom,cam_smmu:msm_cam_smmu_tfe to group 15
6,803,12863549,-;msm_cam_smmu soc:qcom,cam_smmu:msm_cam_smmu_ope: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cam_smmu:msm_cam_smmu_ope
6,804,12873932,-;iommu: Adding device soc:qcom,cam_smmu:msm_cam_smmu_ope to group 16
6,805,12883633,-;msm_cam_smmu soc:qcom,cam_smmu:msm_cam_smmu_cpas_cdm: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,cam_smmu:msm_cam_smmu_cpas_cdm
6,806,12894496,-;iommu: Adding device soc:qcom,cam_smmu:msm_cam_smmu_cpas_cdm to group 17
6,807,12907846,-;cam-cpas 5c11000.qcom,cam-cpas: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c11000.qcom,cam-cpas
6,808,12915797,-;CAM_INFO: CAM-CPAS: cam_cpas_get_hw_features: 436 feature 0x2 addr 0x1b401d0, bit 5 enable type:0 hw_id=2
6,809,12926478,-;CAM_INFO: CAM-CPAS: cam_cpas_get_hw_features: 487 num entries:0 feature 0x2 enable=1 hw id=2
6,810,12936021,-;CAM_INFO: CAM-CPAS: cam_cpas_get_hw_features: 436 feature 0x3 addr 0x1b401d0, bit 6 enable type:0 hw_id=2
6,811,12946695,-;CAM_INFO: CAM-CPAS: cam_cpas_get_hw_features: 487 num entries:1 feature 0x3 enable=1 hw id=2
6,812,12970251,-;msm_cam_cdm 5c23000.qcom,cpas-cdm0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c23000.qcom,cpas-cdm0
6,813,12986425,-;msm_cam_cdm 5c42000.qcom,ope-cdm0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c42000.qcom,ope-cdm0
6,814,13000401,-;tpg_v1 5c66000.qcom,tpg0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c66000.qcom,tpg0
6,815,13010880,-;tpg_v1 5c68000.qcom,tpg0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c68000.qcom,tpg0
6,816,13021860,-;csid_530 5c6e000.qcom,tfe_csid0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c6e000.qcom,tfe_csid0
6,817,13030680,-;csid_530 5c75000.qcom,tfe_csid1: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c75000.qcom,tfe_csid1
6,818,13039481,-;csid_530 5c7c000.qcom,tfe_csid2: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c7c000.qcom,tfe_csid2
6,819,13049528,-;CAM_INFO: CAM-UTIL: cam_soc_util_get_option_clk_by_name: 559 No clk data for tfe_dsp_clk
6,820,13058699,-;CAM_WARN: CAM-ISP: cam_tfe_init_soc_resources: 50 Option clk get failed with rc -22
6,821,13067755,-;cam_tfe 5c6e000.qcom,tfe0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c6e000.qcom,tfe0
6,822,13078253,-;CAM_INFO: CAM-UTIL: cam_soc_util_get_option_clk_by_name: 559 No clk data for tfe_dsp_clk
6,823,13087403,-;CAM_WARN: CAM-ISP: cam_tfe_init_soc_resources: 50 Option clk get failed with rc -22
6,824,13096450,-;cam_tfe 5c75000.qcom,tfe1: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c75000.qcom,tfe1
6,825,13106902,-;CAM_INFO: CAM-UTIL: cam_soc_util_get_option_clk_by_name: 559 No clk data for tfe_dsp_clk
6,826,13116101,-;CAM_WARN: CAM-ISP: cam_tfe_init_soc_resources: 50 Option clk get failed with rc -22
6,827,13125142,-;cam_tfe 5c7c000.qcom,tfe2: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c7c000.qcom,tfe2
6,828,13138325,-;CAM_ERR: CAM-ISP: cam_isp_context_debug_register: 4944 failed to create dentry
6,829,13146634,-;CAM_ERR: CAM-ISP: cam_isp_context_debug_register: 4944 failed to create dentry
6,830,13154983,-;CAM_ERR: CAM-ISP: cam_isp_context_debug_register: 4944 failed to create dentry
6,831,13163287,-;CAM_INFO: CAM-ISP: cam_isp_dev_probe: 207 Camera ISP probe complete
6,832,13172755,-;CAM_INFO: CAM: cam_res_mgr_probe: 682 Disable shared gpio support.
6,833,13183860,-;cam-cci-driver 5c1b000.qcom,cci0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0
6,834,13201006,-;CAM_INFO: CAM-CCI: cam_cci_platform_probe: 519 Device Type :0
6,835,13210262,-;cam-csiphy-driver 5c52000.qcom,csiphy0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c52000.qcom,csiphy0
6,836,13219392,-;cam-csiphy-driver 5c53000.qcom,csiphy1: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c53000.qcom,csiphy1
6,837,13228379,-;cam-csiphy-driver 5c54000.qcom,csiphy2: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c54000.qcom,csiphy2
6,838,13239389,-;CAM_INFO: CAM-ACTUATOR: cam_actuator_parse_dt: 60 No GPIO found
6,839,13249859,-;CAM_INFO: CAM-SENSOR: cam_sensor_driver_get_dt_data: 211 is_scanner: 0
6,840,13259145,-;CAM_INFO: CAM-SENSOR: cam_sensor_driver_get_dt_data: 211 is_scanner: 0
6,841,13268868,-;CAM_INFO: CAM-SENSOR: cam_sensor_driver_get_dt_data: 211 is_scanner: 1
6,842,13278829,-;CAM_INFO: CAM-SENSOR: cam_sensor_driver_get_dt_data: 211 is_scanner: 1
6,843,13297387,-;ope 5c42000.qcom,ope: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c42000.qcom,ope
6,844,13308688,-;CAM_INFO: CAM-SMMU: cam_smmu_create_add_handle_in_table: 858 ope already got handle 0x156a5
4,845,13321452,-;dsi_phy 5e94400.qcom,mdss_dsi_phy0: 5e94400.qcom,mdss_dsi_phy0 supply gdsc not found, using dummy regulator
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi_phy0
6,846,13332614,-;dsi_phy 5e94400.qcom,mdss_dsi_phy0: Linked as a consumer to regulator.0
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi_phy0
6,847,13340653,-;dsi_phy 5e94400.qcom,mdss_dsi_phy0: Linked as a consumer to regulator.16
 SUBSYSTEM=platform
 DEVICE=+platform:5e94400.qcom,mdss_dsi_phy0
6,848,13348485,-;[drm:dsi_phy_driver_probe] [msm-dsi-info]: DSI_0: Probe successful
4,849,13358296,-;drm_dsi_ctrl 5e94000.qcom,mdss_dsi0_ctrl: 5e94000.qcom,mdss_dsi0_ctrl supply refgen not found, using dummy regulator
 SUBSYSTEM=platform
 DEVICE=+platform:5e94000.qcom,mdss_dsi0_ctrl
6,850,13370251,-;drm_dsi_ctrl 5e94000.qcom,mdss_dsi0_ctrl: Linked as a consumer to regulator.0
 SUBSYSTEM=platform
 DEVICE=+platform:5e94000.qcom,mdss_dsi0_ctrl
6,851,13378863,-;drm_dsi_ctrl 5e94000.qcom,mdss_dsi0_ctrl: Linked as a consumer to regulator.39
 SUBSYSTEM=platform
 DEVICE=+platform:5e94000.qcom,mdss_dsi0_ctrl
3,852,13387167,-;AXI: get_pdata(): Error: Client name not found
3,853,13392716,-;AXI: msm_bus_cl_get_pdata(): client has to provide missing entry for successful registration
6,854,13402314,-;[drm:dsi_ctrl_dev_probe] [msm-dsi-info]: dsi-ctrl-0: Probe successful
4,855,13414102,-;msm-dsi-display soc:qcom,dsi-display-primary: Falling back to syfs fallback for: dsi_prop
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,dsi-display-primary
6,856,13431443,-;msm_vidc:   err : ffffffff: .....: no device Registered
6,857,13444898,-;msm_vidc_v4l2 5a00000.qcom,vidc:non_secure_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:5a00000.qcom,vidc:non_secure_cb
6,858,13455003,-;iommu: Adding device 5a00000.qcom,vidc:non_secure_cb to group 18
6,859,13464339,-;msm_vidc_v4l2 5a00000.qcom,vidc:secure_bitstream_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:5a00000.qcom,vidc:secure_bitstream_cb
6,860,13475528,-;iommu: Adding device 5a00000.qcom,vidc:secure_bitstream_cb to group 19
6,861,13485515,-;msm_vidc_v4l2 5a00000.qcom,vidc:secure_pixel_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:5a00000.qcom,vidc:secure_pixel_cb
6,862,13496335,-;iommu: Adding device 5a00000.qcom,vidc:secure_pixel_cb to group 20
6,863,13505966,-;msm_vidc_v4l2 5a00000.qcom,vidc:secure_non_pixel_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:5a00000.qcom,vidc:secure_non_pixel_cb
6,864,13517181,-;iommu: Adding device 5a00000.qcom,vidc:secure_non_pixel_cb to group 21
6,865,13527393,-;GACT probability NOT on
6,866,13530984,-;Mirror/redirect action on
6,867,13534761,-;netem: version 1.3
6,868,13537833,-;u32 classifier
6,869,13540575,-;    Actions configured
6,870,13548754,-;xt_time: kernel timezone is -0000
6,871,13553214,-;gre: GRE over IPv4 demultiplexor driver
6,872,13558150,-;IPv4 over IPsec tunneling driver
6,873,13565903,-;Initializing XFRM netlink socket
6,874,13570303,-;IPsec XFRM device driver
6,875,13577762,-;NET: Registered protocol family 10
6,876,13587547,-;Segment Routing with IPv6
6,877,13591895,-;mip6: Mobile IPv6
6,878,13598311,-;sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
6,879,13607959,-;NET: Registered protocol family 17
6,880,13612493,-;NET: Registered protocol family 15
6,881,13617719,-;l2tp_core: L2TP core driver, V2.0
6,882,13622139,-;l2tp_ppp: PPPoL2TP kernel driver, V2.0
6,883,13626946,-;l2tp_ip: L2TP IP encapsulation support (L2TPv3)
6,884,13633101,-;l2tp_netlink: L2TP netlink interface
6,885,13637926,-;l2tp_eth: L2TP ethernet pseudowire support (L2TPv3)
6,886,13643983,-;l2tp_debugfs: L2TP debugfs support
6,887,13648492,-;l2tp_ip6: L2TP IP encapsulation support for IPv6 (L2TPv3)
6,888,13656541,-;sctp: Hash tables configured (bind 128/128)
5,889,13663266,-;Key type dns_resolver registered
6,890,13671033,-;kgsl-3d 5900000.qcom,kgsl-3d0: Linked as a consumer to regulator.11
 SUBSYSTEM=platform
 DEVICE=+platform:5900000.qcom,kgsl-3d0
6,891,13678783,-;kgsl-3d 5900000.qcom,kgsl-3d0: Linked as a consumer to regulator.12
 SUBSYSTEM=platform
 DEVICE=+platform:5900000.qcom,kgsl-3d0
6,892,13690442,-;platform 59a0000.qcom,kgsl-iommu:gfx3d_user: Linked as a consumer to 59a0000.kgsl-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.qcom,kgsl-iommu:gfx3d_user
6,893,13699791,-;iommu: Adding device 59a0000.qcom,kgsl-iommu:gfx3d_user to group 22
6,894,13709015,-;platform 59a0000.qcom,kgsl-iommu:gfx3d_secure: Linked as a consumer to 59a0000.kgsl-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:59a0000.qcom,kgsl-iommu:gfx3d_secure
6,895,13718475,-;iommu: Adding device 59a0000.qcom,kgsl-iommu:gfx3d_secure to group 23
6,896,13783555,-;msm-dwc3 4e00000.ssusb: Linked as a consumer to regulator.3
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
3,897,13793758,-;dwc3 4e00000.dwc3: Failed to get clk 'ref': -2
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.dwc3
6,898,13800002,-;dwc3 4e00000.dwc3: changing max_speed on rev 00000000
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.dwc3
6,899,13825527,-;usb_bam_init: setting SPS_BAM_SMMU_EN flag with (4f04000.qcom,usbbam)
6,900,13834610,-;sps:BAM 0x0000000004f04000 is registered.
3,901,13834679,-;ipa_get_transport_type:2925 IPA HW is not supported
3,902,13854644,-;Invalid index Defaulting curr to 0
6,903,13858089,-;ads1015 0-0048: read from continous mode from usbid channel
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,904,13863889,-;ipa_rm ipa_rm_delete_resource:139 IPA RM was not initialized
6,905,13869653,-;ads1015 0-0048: read voltage is 186
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,906,13875930,-;ipa_get_ipc_logbuf:3437 IPA HW is not supported
6,907,13880500,-;ads1015 0-0048: read from continous mode from usbid channel
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,908,13886084,-;ipa_get_ipc_logbuf_low:3450 IPA HW is not supported
6,909,13893081,-;ads1015 0-0048: read voltage is 186
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
3,910,13898680,-;usb_bam_ipa_delete_resources: Failed to delete USB_PROD resource
6,911,13903224,-; hon-accessory: detect voltage is 186
3,912,13910338,-;ipa_rm ipa_rm_delete_resource:139 IPA RM was not initialized
6,913,13915040,-; hon-accessory: No state change necessary-not_connected
3,914,13921766,-;ipa_get_ipc_logbuf:3437 IPA HW is not supported
6,915,13928079,-; hon-accessory: send uevent EXTRA_DOCK_STATE_UNDOCKED
3,916,13933673,-;ipa_get_ipc_logbuf_low:3450 IPA HW is not supported
3,917,13945724,-;usb_bam_ipa_delete_resources: Failed to delete USB_CONS resource
6,918,13955404,-;msm-dwc3 4e00000.ssusb: Dropping the link to regulator.3
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
6,919,14028623,-;qcom,qpnp-smb5 1c40000.qcom,spmi:qcom,pmi632@2:qcom,qpnp-smb5: Linked as a consumer to regulator.48
 SUBSYSTEM=platform
 DEVICE=+platform:1c40000.qcom,spmi:qcom,pmi632@2:qcom,qpnp-smb5
6,920,14046552,-; hon-accessory: charger event from usbin
3,921,14051835,-;pmi632_charger: smblib_eval_chg_termination: Couldn't read SOC value, rc=-22
3,922,14070973,-;bcl_soc:bcl_read_soc battery percentage read error:-61
6,923,14101544,-;SMB5 status - usb:present=1 type=0 batt:present = 1 health = 1 charge = 1
6,924,14109831,-;QPNP SMB5 probed successfully
3,925,14121091,-;bcl_soc:bcl_read_soc battery percentage read error:-61
6,926,14168722,-;of_batterydata_get_best_profile: tws_max1720x_maxell_4020mah_10k found
6,927,14185614,-;QG-K: qg_batterydata_init: QG Battery-profile loaded
6,928,14197601,-;QG-K: qg_determine_pon_soc: using SHUTDOWN_SOC @ PON ocv_uv=3868400uV soc=51
6,929,14212895,-;QG-K: qpnp_qg_probe: QG initialized! battery_profile=tws_max1720x_maxell_4020mah_10k SOC=51 QG_subtype=3 QG_version=QG_PMIC5 QG_mode=QG_V_I
6,930,14228284,-;of_batterydata_get_best_profile: tws_max1720x_maxell_4020mah_10k found
3,931,14236587,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,932,14242290,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,933,14249656,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,934,14255339,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,935,14266357,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,936,14272087,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,937,14279425,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,938,14285774,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,939,14292069,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,940,14299579,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,941,14307257,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,942,14312985,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,943,14320632,-;tmc_etr_bam_init: setting SPS_BAM_SMMU_EN flag with (8048000.tmc)
6,944,14329083,-;sps:BAM 0x0000000008064000 is registered.
6,945,14332725,-;coresight-stm 8002000.stm: STM32 initialized
 SUBSYSTEM=amba
 DEVICE=+amba:8002000.stm
6,946,14344434,-;msm-dwc3 4e00000.ssusb: Linked as a consumer to regulator.3
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
3,947,14355945,-;dwc3 4e00000.dwc3: Failed to get clk 'ref': -2
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.dwc3
6,948,14361981,-;dwc3 4e00000.dwc3: changing max_speed on rev 00000000
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.dwc3
3,949,14385606,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,950,14387344,-;usb_bam_init: setting SPS_BAM_SMMU_EN flag with (4f04000.qcom,usbbam)
3,951,14391358,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,952,14400196,-;sps:BAM 0x0000000004f04000 is registered.
3,953,14400265,-;ipa_get_transport_type:2925 IPA HW is not supported
3,954,14406166,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,955,14414909,-;msm-dwc3 4e00000.ssusb: Linked as a consumer to regulator.48
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
3,956,14416099,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,957,14434840,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,958,14440018,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,959,14440229,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,960,14445712,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,961,14450693,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,962,14461944,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,963,14467288,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,964,14472484,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,965,14472697,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,966,14478210,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,967,14483124,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,968,14494194,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,969,14494412,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,970,14499918,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,971,14504837,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,972,14515697,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
6,973,14522973,-;EDAC DEVICE0: Giving out device to module soc:arm64_cpu_erp controller cache: DEV soc:arm64_cpu_erp (INTERRUPT)
3,974,14536639,-;ARM64 CPU ERP: Could not find <cci-irq> IRQ property. Proceeding anyway.
3,975,14544419,-;ARM64 CPU ERP: SBE detection is disabled.
6,976,14551660,-;core_ctl: Creating CPU group 0
6,977,14555775,-;core_ctl: Init CPU0 state
6,978,14559481,-;core_ctl: Init CPU1 state
6,979,14563162,-;core_ctl: Init CPU2 state
6,980,14566842,-;core_ctl: Init CPU3 state
6,981,14571361,-;core_ctl: Creating CPU group 4
6,982,14575476,-;core_ctl: Init CPU4 state
6,983,14579175,-;core_ctl: Init CPU5 state
6,984,14582856,-;core_ctl: Init CPU6 state
6,985,14586537,-;core_ctl: Init CPU7 state
6,986,14593052,-;registered taskstats version 1
5,987,14597166,-;Loading compiled-in X.509 certificates
6,988,14603494,-;cryptomgr_probe (398) used greatest stack depth: 14032 bytes left
5,989,14604930,-;Loaded X.509 cert 'Build time autogenerated kernel key: b1fd81475348f7e2bde6c9c5d4ddb78577f4dd51'
5,990,14624993,-;Key type ._fscrypt registered
5,991,14629043,-;Key type .fscrypt registered
5,992,14632989,-;Key type fscrypt-provisioning registered
6,993,14793216,-;fastrpc soc:qcom,msm-adsprpc-mem: for adsp_rh segments only will be dumped.
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-adsprpc-mem
6,994,14801901,-;adsprpc: init_secure_vmid_list: secure VMID = 22
6,995,14807585,-;adsprpc: init_secure_vmid_list: secure VMID = 37
6,996,14813423,-;adsprpc: fastrpc_probe: service location enabled for avs/audio (audio_pdr_adsprpc)
6,997,14822130,-;adsprpc: fastrpc_probe: service location enabled for tms/servreg (sensors_pdr_adsprpc)
6,998,14832527,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb1: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb1
6,999,14843788,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb1 to group 24
6,1000,14854905,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb2: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb2
6,1001,14866209,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb2 to group 25
4,1002,14875918,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1003,14885066,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb3: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb3
6,1004,14896312,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb3 to group 26
4,1005,14905962,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1006,14915229,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb4: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb4
6,1007,14926397,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb4 to group 27
4,1008,14936140,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1009,14945268,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb5: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb5
6,1010,14956482,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb5 to group 28
4,1011,14966175,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1012,14975475,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb6: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb6
6,1013,14986624,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb6 to group 29
4,1014,14996318,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1015,15005389,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb9: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb9
6,1016,15016685,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb9 to group 30
4,1017,15026349,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1018,15035445,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb10: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb10
6,1019,15046988,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb10 to group 31
4,1020,15056806,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1021,15065957,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb11: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb11
6,1022,15077377,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb11 to group 32
4,1023,15087130,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1024,15096217,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb12: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb12
6,1025,15107594,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb12 to group 33
4,1026,15117391,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1027,15126564,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb13: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb13
6,1028,15137944,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb13 to group 34
4,1029,15147732,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1030,15156887,-;fastrpc soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb14: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb14
6,1031,15168322,-;iommu: Adding device soc:qcom,msm_fastrpc:qcom,msm_fastrpc_compute_cb14 to group 35
4,1032,15178107,-;Error: swapper/0: fastrpc_cb_probe: failed to create debugfs global file
6,1033,15188259,-;adsprpc: fastrpc_device_init: SSR notifier registered for adsp
6,1034,15195153,-;adsprpc: fastrpc_device_init: SSR notifier registered for modem
6,1035,15202157,-;adsprpc: fastrpc_device_init: SSR notifier registered for slpi
6,1036,15209091,-;adsprpc: fastrpc_device_init: SSR notifier registered for cdsp
6,1037,15230181,-;input: gpio-keys as /devices/platform/soc/soc:gpio_keys/input/input3
4,1038,15240793,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1039,15247714,-;atmel_maxtouch_ts 1-004a: enter mxt_parse_dt
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
6,1040,15253143,-;atmel_maxtouch_ts 1-004a: mxt_parse_dt: atmel,cfg_name is ct45_mxt640u.raw
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
6,1041,15261101,-;atmel_maxtouch_ts 1-004a: mxt_parse_dt: atmel,fw_name is maxtouch_v1.1.AA.fw
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
6,1042,15269253,-;atmel_maxtouch_ts 1-004a: mxt_parse_dt: atmel,hon-version is ct45
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
6,1043,15276483,-;atmel_maxtouch_ts 1-004a: mxt_parse_dt: atmel,reset-gpio is 1238
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
6,1044,15283641,-;atmel_maxtouch_ts 1-004a: mxt_parse_dt: atmel,irq-gpio is 1247
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
3,1045,15291684,-;bengal-pinctrl 400000.pinctrl: pin GPIO_80 already requested by 1-0038; cannot claim for 1-004a
 SUBSYSTEM=platform
 DEVICE=+platform:400000.pinctrl
3,1046,15301460,-;bengal-pinctrl 400000.pinctrl: pin-80 (1-004a) status -22
 SUBSYSTEM=platform
 DEVICE=+platform:400000.pinctrl
3,1047,15307920,-;bengal-pinctrl 400000.pinctrl: could not request pin 80 (GPIO_80) from group gpio80  on device 400000.pinctrl
 SUBSYSTEM=platform
 DEVICE=+platform:400000.pinctrl
3,1048,15316235,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1049,15318908,-;atmel_maxtouch_ts 1-004a: Error applying setting, reverse things back
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
3,1050,15318915,-;atmel_maxtouch_ts 1-004a: can not set pmx_ts_active pins
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
3,1051,15318922,-;atmel_maxtouch_ts 1-004a: Failed to configure gpios
 SUBSYSTEM=i2c
 DEVICE=+i2c:1-004a
4,1052,15319093,-;atmel_maxtouch_ts: probe of 1-004a failed with error -22
3,1053,15324603,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1054,15335015,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
3,1055,15339753,-;msm-usb-ssphy-qmp 1615000.ssphy: USB QMP PHY: Update TYPEC CTRL(2)
 SUBSYSTEM=platform
 DEVICE=+platform:1615000.ssphy
3,1056,15345548,-;[NVT-ts] nvt_driver_init 1958: start
6,1057,15352070,-;msm-dwc3 4e00000.ssusb: DWC3 exited from low power mode
 SUBSYSTEM=platform
 DEVICE=+platform:4e00000.ssusb
3,1058,15357081,-;[NVT-ts] nvt_driver_init 1966: finished
4,1059,15400428,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1060,15417277,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
3,1061,15425405,-;ipa-wan ipa3_wwan_init:4763 ipa3_ctx was not initialized
3,1062,15431843,-;ipa_get_ipc_logbuf:3437 IPA HW is not supported
3,1063,15437429,-;ipa_get_ipc_logbuf_low:3450 IPA HW is not supported
6,1064,15444116,-;RNDIS_IPA module is loaded.
6,1065,15453979,-;CAM_ERR: CAM-CCI: cam_cci_assign_fops: 599 Invalid dev node:0000000000000000 offset: 0
6,1066,15464182,-;msm notifier probed successfully
4,1067,15470337,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1068,15479171,-;sde_rotator 5e00000.qcom,mdss_rotator: ignoring dependency for device, assuming no driver
 SUBSYSTEM=platform
 DEVICE=+platform:5e00000.qcom,mdss_rotator
5,1069,15489554,-;cfg80211: Loading compiled-in X.509 certificates for regulatory database
6,1070,15498891,-;cryptomgr_probe (425) used greatest stack depth: 13536 bytes left
5,1071,15499554,-;cfg80211: Loaded X.509 cert 'sforshee: 00b28ddf47aef9cea7'
6,1072,15520381,-;regulator_proxy_consumer_remove_all: removing regulator proxy consumer requests
6,1073,15529287,-;ALSA device list:
6,1074,15532277,-;  No soundcards found.
6,1075,15567124,-;Freeing unused kernel memory: 6400K
6,1076,15571757,-;Run /init as init process
14,1077,15609392,-;init: init first stage started!
14,1078,15614110,-;init: Unable to open /lib/modules, skipping module loading.
14,1079,15623140,-;init: [libfs_mgr]dt_fstab: Skip disabled entry for partition vendor
14,1080,15630558,-;init: [libfs_mgr]ReadFstabFromDt(): failed to read fstab from dt
14,1081,15638568,-;init: [libfs_mgr]dt_fstab: Skip disabled entry for partition vendor
14,1082,15648955,-;init: Using Android DT directory /proc/device-tree/firmware/android/
14,1083,15908249,-;init: [libfs_mgr]superblock s_max_mnt_count:65535,/dev/block/by-name/metadata
14,1084,15923320,-;init: [libfs_mgr]check_fs(): mount(/dev/block/by-name/metadata,/metadata,ext4)=-1: No such file or directory
14,1085,15934639,-;init: [libfs_mgr]Running /system/bin/e2fsck on /dev/block/sda11
11,1086,15945172,-;logwrapper: Cannot log to file /dev/fscklogs/log
14,1087,15953891,-;e2fsck: e2fsck 1.45.4 (23-Sep-2019)
14,1088,15968830,-;e2fsck: Pass 1: Checking inodes, blocks, and sizes
14,1089,15978749,-;e2fsck: Pass 2: Checking directory structure
14,1090,15984125,-;e2fsck: Pass 3: Checking directory connectivity
14,1091,15989773,-;e2fsck: Pass 4: Checking reference counts
6,1092,15992990,-;e2fsck (427) used greatest stack depth: 12352 bytes left
14,1093,15994880,-;e2fsck: Pass 5: Checking group summary information
14,1094,16007118,-;e2fsck: /dev/block/by-name/metadata: 37/4096 files (0.0% non-contiguous), 1200/4096 blocks
6,1095,16008139,-;of_batterydata_get_best_profile: tws_max1720x_maxell_4020mah_10k found
3,1096,16024071,-;QCOM-STEPCHG: read_range_data_from_node: Count qcom,step-chg-ranges failed, rc=-22
6,1097,16036006,-;EXT4-fs (sda11): mounted filesystem with ordered data mode. Opts: discard
6,1098,16105199,-;EXT4-fs (dm-0): mounted filesystem without journal. Opts: barrier=1,discard
6,1099,16147761,-;EXT4-fs (dm-1): mounted filesystem without journal. Opts: barrier=1,discard
6,1100,16178081,-;ads1015 0-0048: read from continous mode from usbid channel
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
6,1101,16182937,-;EXT4-fs (dm-3): mounted filesystem without journal. Opts: barrier=1,discard
6,1102,16185170,-;ads1015 0-0048: read voltage is 186
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
6,1103,16197318,-;ads1015 0-0048: read from continous mode from usbid channel
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
6,1104,16204350,-;ads1015 0-0048: read voltage is 186
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0048
6,1105,16208920,-; hon-accessory: detect voltage is 186
6,1106,16213646,-; hon-accessory: No state change necessary-not_connected
6,1107,16215214,-;EXT4-fs (dm-2): mounted filesystem without journal. Opts: barrier=1,discard
6,1108,16219965,-; hon-accessory: send uevent EXTRA_DOCK_STATE_UNDOCKED
6,1109,17007996,-;max1720x 0-0036: case 5 === SN=TWMX2049505588
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1110,17021313,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1111,17026997,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1112,17317778,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1113,17323493,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1114,17330471,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1115,17336154,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1116,17391765,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1117,17397449,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,1118,17762684,-;fsck.f2fs: executing /system/bin/fsck.f2fs failed: No such file or directory
6,1119,17764945,-;init (439) used greatest stack depth: 11696 bytes left
14,1120,17770911,-;fsck.f2fs: fsck.f2fs terminated by exit(255)\x0a
6,1121,17988543,-;F2FS-fs (dm-4): recover fsync data on readonly fs
5,1122,17996133,-;F2FS-fs (dm-4): Mounted with checkpoint version = 5f71a0e8
14,1123,18046519,-;fsck.f2fs: executing /system/bin/fsck.f2fs failed: No such file or directory
5,1124,18261806,-;F2FS-fs (dm-4): Mounted with checkpoint version = 5f71a0e8
4,1125,18336492,-;init: 1 output lines suppressed due to ratelimiting
4,1126,18342527,-;init: 44 output lines suppressed due to ratelimiting
14,1127,18566752,-;init: [libfs_mgr]dt_fstab: Skip disabled entry for partition vendor
14,1128,18591700,-;init: Loading SELinux policy
6,1129,19410434,-;SELinux:  policy capability network_peer_controls=1
6,1130,19416385,-;SELinux:  policy capability open_perms=1
6,1131,19421402,-;SELinux:  policy capability extended_socket_class=1
6,1132,19427345,-;SELinux:  policy capability always_check_network=0
6,1133,19433240,-;SELinux:  policy capability cgroup_seclabel=0
6,1134,19438683,-;SELinux:  policy capability nnp_nosuid_transition=1
5,1135,19936058,-;audit: type=1403 audit(5093.929:2): auid=4294967295 ses=4294967295 lsm=selinux res=1
14,1136,19936948,-;selinux: SELinux: Loaded policy from /vendor/etc/selinux/precompiled_sepolicy
14,1137,19953174,-;selinux: 
5,1138,19956593,-;audit: type=1404 audit(5093.959:3): enforcing=1 old_enforcing=0 auid=4294967295 ses=4294967295 enabled=1 old-enabled=1 lsm=selinux res=1
14,1139,19986430,-;selinux: SELinux: Loaded file_contexts
14,1140,19991304,-;selinux: 
14,1141,20049248,-;init: init second stage started!
14,1142,20176128,-;init: Using Android DT directory /proc/device-tree/firmware/android/
11,1143,20209208,-;init: Do not have permissions to set 'persist.backup.ntpServer' to '0.pool.ntp.org' in property file '/vendor/build.prop': SELinux permission check failed
12,1144,20224414,-;init: Overriding previous 'ro.' property 'dalvik.vm.heapsize':'36m' with new value '256m'
11,1145,20234078,-;init: Do not have permissions to set 'ro.qc.sdk.audio.ssr' to 'false' in property file '/vendor/build.prop': SELinux permission check failed
11,1146,20247819,-;init: Do not have permissions to set 'ro.qc.sdk.audio.fluencetype' to 'none' in property file '/vendor/build.prop': SELinux permission check failed
11,1147,20262368,-;init: Do not have permissions to set 'persist.audio.fluence.voicecall' to 'true' in property file '/vendor/build.prop': SELinux permission check failed
11,1148,20277052,-;init: Do not have permissions to set 'persist.audio.fluence.voicerec' to 'false' in property file '/vendor/build.prop': SELinux permission check failed
11,1149,20291742,-;init: Do not have permissions to set 'persist.audio.fluence.speaker' to 'true' in property file '/vendor/build.prop': SELinux permission check failed
11,1150,20306616,-;init: Do not have permissions to set 'persist.vendor.bt.a2dp_offload_cap' to 'sbc-aptx-aptxtws-aptxhd-aac-ldac' in property file '/vendor/build.prop': SELinux permission check failed
5,1151,20499224,-;audit: type=1107 audit(5094.499:4): pid=1 uid=0 auid=4294967295 ses=4294967295 subj=u:r:init:s0 msg='avc:  denied  { read } for property=persist.debug.trace pid=0 uid=0 gid=0 scontext=u:r:vendor_init:s0 tcontext=u:object_r:persist_debug_prop:s0 tclass=file permissive=0'
6,1152,20868153,-;linkerconfig (447) used greatest stack depth: 11312 bytes left
14,1153,20971280,-;ueventd: ueventd started!
14,1154,20981035,-;selinux: SELinux: Loaded file_contexts
14,1155,20985870,-;selinux: 
14,1156,20988792,-;ueventd: Parsing file /system/etc/ueventd.rc...
14,1157,20996960,-;ueventd: Parsing file /vendor/ueventd.rc...
11,1158,21007419,-;ueventd: /vendor/ueventd.rc: 175: /sys/ lines must have 5 entries
11,1159,21015517,-;ueventd: /vendor/ueventd.rc: 412: Invalid section keyword found
14,1160,21022962,-;ueventd: Parsing file /odm/ueventd.rc...
14,1161,21028128,-;ueventd: Unable to read config file '/odm/ueventd.rc': open() failed: No such file or directory
14,1162,21037966,-;ueventd: Parsing file /ueventd.qcom.rc...
14,1163,21068753,-;apexd: This device does not support updatable APEX. Exiting
6,1164,21079861,-;apexd (449) used greatest stack depth: 11152 bytes left
6,1165,21265751,-;boringssl_self_ (451) used greatest stack depth: 10880 bytes left
5,1166,21409302,-;audit: type=1400 audit(5095.409:5): avc:  denied  { mounton } for  pid=1 comm="init" path="/sys/kernel/tracing" dev="tracefs" ino=1 scontext=u:r:init:s0 tcontext=u:object_r:debugfs_tracing_debug:s0 tclass=dir permissive=0
6,1167,21537928,-;max1720x 0-0036: case 5 === SN=TWMX2049505588
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1168,21551167,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1169,21556856,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1170,21634281,-;q6_pdr_dlkm: loading out-of-tree module taints kernel.
4,1171,21669740,-;apr_dlkm: no symbol version for snd_event_notify
5,1172,21679020,-;audit: type=1400 audit(5095.679:6): avc:  denied  { search } for  pid=454 comm="modprobe" name="ipc_logging" dev="debugfs" ino=2077 scontext=u:r:vendor_modprobe:s0 tcontext=u:object_r:vendor_debugfs_ipc:s0 tclass=dir permissive=0
4,1173,21706011,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1174,21719794,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
3,1175,21800707,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1176,21802482,-;
3,1177,21806382,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1178,21807877,-;**********************************************************
3,1179,21814806,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1180,21820567,-;**   NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE   **
3,1181,21826218,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1182,21832770,-;**                                                      **
4,1183,21845419,-;** trace_printk() being used. Allocating extra memory.  **
4,1184,21851978,-;**                                                      **
4,1185,21858546,-;** This means that this is a DEBUG kernel and it is     **
4,1186,21865089,-;** unsafe for production use.                           **
4,1187,21871648,-;**                                                      **
4,1188,21878206,-;** If you see this message and you are not debugging    **
4,1189,21884742,-;** the kernel, report this immediately to your vendor!  **
4,1190,21891295,-;**                                                      **
3,1191,21892356,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1192,21897828,-;**   NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE NOTICE   **
3,1193,21903510,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1194,21910063,-;**********************************************************
3,1195,21954624,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1196,21960361,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1197,21968294,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1198,21973983,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1199,21980847,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1200,21986534,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1201,21994148,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1202,21999878,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1203,22006873,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1204,22012594,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1205,22076983,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1206,22090792,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1207,22101984,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1208,22110919,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1209,22129878,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1210,22147891,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1211,22170045,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1212,22178728,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1213,22187474,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1214,22196193,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1215,22204741,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1216,22213356,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1217,22222002,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1218,22230623,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1219,22239506,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1220,22248269,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1221,22256903,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1222,22265451,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1223,22274128,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1224,22285185,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1225,22388304,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1226,22412118,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1227,22437692,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1228,22481316,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
5,1229,23081900,-;audit: type=1400 audit(5097.079:7): avc:  denied  { read } for  pid=475 comm="cat" name="sku_version" dev="sysfs" ino=53298 scontext=u:r:vendor_qti_media:s0 tcontext=u:object_r:sysfs:s0 tclass=file permissive=0
3,1230,24020316,-;Trying to create more than 6 SchedTune boosting groups
5,1231,24114029,-;Registered swp emulation handler
38,1232,24211723,-;logd.auditd: start
46,1233,24215489,-;logd.klogd: 24207439313
14,1234,25211506,-;init: Service 'exec 6 (/vendor/bin/sh /vendor/bin/init.qti.usb.debug.sh)' (pid 516) exited with status 0 waiting took 0.591000 seconds
14,1235,25224720,-;init: Sending signal 9 to service 'exec 6 (/vendor/bin/sh /vendor/bin/init.qti.usb.debug.sh)' (pid 516) process group...
14,1236,25237084,-;libprocessgroup: Successfully killed process cgroup uid 0 pid 516 in 0ms
14,1237,25245464,-;init: processing action (init) from (/vendor/etc/init/hw/init.target.rc:34)
14,1238,25264377,-;init: wait for '/dev/block/platform/soc/4804000.ufshc' took 0ms
14,1239,25273501,-;init: starting service 'vendor.qseecomd'...
14,1240,25293617,-;init: Command 'start keymaster-4-0' action=init (/vendor/etc/init/hw/init.target.rc:46) took 0ms and failed: service keymaster-4-0 not found
14,1241,25307434,-;init: processing action (init) from (/system/etc/init/hw/init.hssi.plat.rc:5)
14,1242,25315783,-;init: processing action (init) from (/system/etc/init/audioserver.rc:56)
14,1243,25325113,-;init: processing action (init) from (/vendor/etc/init/android.hardware.keymaster@4.1-service-qti.rc:1)
14,1244,25337869,-;init: starting service 'vendor.keymaster-4-1'...
14,1245,25378006,-;init: wait for '/dev/qseecom' took 0ms
6,1246,25481013,-;EXT4-fs (sda2): mounted filesystem with ordered data mode. Opts: barrier=1
6,1247,25519096,-;EXT4-fs (sde9): mounted filesystem with ordered data mode. Opts: barrier=1
36,1248,25539432,-;type=1107 audit(5099.539:8): uid=0 auid=4294967295 ses=4294967295 subj=u:r:init:s0 msg='avc: denied { set } for property=ro.hon.touch.ver.fw pid=520 uid=0 gid=0 scontext=u:r:hsm_property:s0 tcontext=u:object_r:default_prop:s0 tclass=property_service permissive=0'
36,1249,25564244,-;type=1107 audit(5099.539:9): uid=0 auid=4294967295 ses=4294967295 subj=u:r:init:s0 msg='avc: denied { set } for property=persist.touch.module.name pid=520 uid=0 gid=0 scontext=u:r:hsm_property:s0 tcontext=u:object_r:default_prop:s0 tclass=property_service permissive=0'
4,1250,25571652,-;EXT4-fs (sda30): Ignoring removed nomblk_io_submit option
36,1251,25589402,-;type=1107 audit(5099.539:10): uid=0 auid=4294967295 ses=4294967295 subj=u:r:init:s0 msg='avc: denied { set } for property=ro.hon.panel.name pid=520 uid=0 gid=0 scontext=u:r:hsm_property:s0 tcontext=u:object_r:default_prop:s0 tclass=property_service permissive=0'
6,1252,25607187,-;EXT4-fs (sda30): mounted filesystem with ordered data mode. Opts: errors=remount-ro,nomblk_io_submit
14,1253,25712104,-;e2fsck: e2fsck 1.45.4 (23-Sep-2019)
14,1254,25727964,-;e2fsck: /dev/block/bootdevice/by-name/IPSM: clean, 46/131072 files, 24656/524288 blocks
36,1255,25733051,-;type=1400 audit(5099.729:11): avc: denied { kill } for comm="e2fsck" capability=5 scontext=u:r:fsck:s0 tcontext=u:r:fsck:s0 tclass=capability permissive=0
6,1256,25767916,-;EXT4-fs (sda30): mounted filesystem with ordered data mode. Opts: discard
4,1257,25795667,-;EXT4-fs (sda20): Ignoring removed nomblk_io_submit option
6,1258,25806881,-;EXT4-fs (sda20): mounted filesystem with ordered data mode. Opts: errors=remount-ro,nomblk_io_submit
14,1259,25874608,-;e2fsck: e2fsck 1.45.4 (23-Sep-2019)
14,1260,25888757,-;e2fsck: /dev/block/bootdevice/by-name/secure: clean, 11/16384 files, 1546/16384 blocks
36,1261,25902062,-;type=1400 audit(5099.899:12): avc: denied { kill } for comm="e2fsck" capability=5 scontext=u:r:fsck:s0 tcontext=u:r:fsck:s0 tclass=capability permissive=0
6,1262,25918562,-;EXT4-fs (sda20): mounted filesystem with ordered data mode. Opts: discard
3,1263,26064345,-;tas2563 0-004c: Driver ID: 1.0.0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1264,26068689,-;tas2563 0-004c: tas2563_i2c_probe enter
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1265,26074188,-;tas2563 0-004c: ti,channels=1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1266,26074200,-;tas2563 0-004c: ti,left-channel=0x4c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1267,26074298,-;tas2563 0-004c: ti,reset-gpio=1162
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1268,26074387,-;tas2563 0-004c: ti,irq-gpio=1250
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1269,26074396,-;tas2563 0-004c: tas2563_parse_dt: mono config, don't parse stereo params!
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1270,26082798,-;tas2563 0-004c: Linked as a consumer to regulator.30
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1271,26128739,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:1, VAL: 0x01
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1272,26128953,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:5, VAL: 0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1273,26148131,-;tas2563 0-004c: tas2563_dev_read: chn: 1 chn_num: 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1274,26148472,-;tas2563 0-004c: tas2563_dev_read: chn:4c:BOOK:PAGE:REG 0:0:125,0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1275,26148481,-;tas2563 0-004c: tas2563_dev_read: chn: 2 chn_num: 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1276,26148805,-;tas2563 0-004c: tas2563_dev_read: chn:4c:BOOK:PAGE:REG 0:0:125,0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1277,26148813,-;tas2563 0-004c: LPGID: 16 RPGID:16
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1278,26153281,-;tas2563 0-004c: tas2563_dev_read: chn: 1 chn_num: 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1279,26153614,-;tas2563 0-004c: tas2563_dev_read: chn:4c:BOOK:PAGE:REG 0:0:3,0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1280,26153623,-;tas2563 0-004c: tas2563_dev_read: chn: 2 chn_num: 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1281,26153943,-;tas2563 0-004c: tas2563_dev_read: chn:4c:BOOK:PAGE:REG 0:0:3,0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1282,26154481,-;tas2563 0-004c: irq = 286
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,1283,26154729,-;tas2563 0-004c: tas2563_register_codec, enter
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1284,26160762,-;tas2563 0-004c: tas2563_register_misc, leave
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1285,26166103,-;tas2563 0-004c: tiload_driver_init
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1286,26170879,-;tas2563 0-004c: allocated Major Number: 503
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1287,26176686,-;tas2563 0-004c: Registered TiLoad driver, Major number: 503
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1288,26183637,-;tas2563 0-004c: Dropping the link to regulator.30
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
4,1289,26183662,-;tas2563 0-004c: Falling back to syfs fallback for: tas2563_uCDSP.bin
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
4,1290,26193191,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1291,26230786,-;EXT4-fs (sda22): mounted filesystem with ordered data mode. Opts: barrier=1
15,1292,26303775,-;vdc: Waited 0ms for vold
14,1293,26595383,-;ueventd: firmware: loading 'tas2563_uCDSP.bin' for '/devices/platform/soc/4a84000.i2c/i2c-0/0-004c/firmware/tas2563_uCDSP.bin'
14,1294,26615521,-;ueventd: loading /devices/platform/soc/4a84000.i2c/i2c-0/0-004c/firmware/tas2563_uCDSP.bin took 20ms
3,1295,26626112,-;tas2563 0-004c: tas2563_fw_ready: start
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1296,26631220,-;tas2563 0-004c: firmware size: 20681
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1297,26635871,-;tas2563 0-004c: FW timestamp: 1611133424
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1298,26640944,-;tas2563 0-004c: FW Size       = 20681
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1299,26642686,-;bad ioctl: -1072934383
6,1300,26645677,-;tas2563 0-004c: Checksum      = 0xF2CFE31A
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1301,26652860,-;wait_for_keymaster: Waiting for Keymaster device
6,1302,26654297,-;tas2563 0-004c: PPC Version   = 0x34100
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1303,26664915,-;tas2563 0-004c: FW  Version    = 0x1010000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1304,26666321,-;wait_for_keymaster: List of Keymaster HALs found:
6,1305,26670125,-;tas2563 0-004c: Driver Version= 0x0202
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1306,26670133,-;tas2563 0-004c: Timestamp     = 1611133424
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1307,26676427,-;wait_for_keymaster: Keymaster HAL #1: Keymaster HAL: 4 from QTI SecurityLevel: TRUSTED_ENVIRONMENT HAL: android.hardware.keymaster@4.1::IKeymasterDevice/default
6,1308,26680748,-;tas2563 0-004c: DDC Name      = CT45-V0.0-SS1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1309,26687743,-;wait_for_keymaster: Computing HMAC with params { (seed: 207b8f9e714263c4e1cc5cfbff15bcf2401d559d46855f17de29755104a5e, nonce: ba463a5a40ed9dc0797c70d6c4b44591bdd87ae6822eee2091859f391291391) }
6,1310,26695279,-;bad ioctl: -1072934383
6,1311,26701344,-;tas2563 0-004c: Description   = TI SmartAmp
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1312,26706796,-;wait_for_keymaster: Computing HMAC for Keymaster HAL: 4 from QTI SecurityLevel: TRUSTED_ENVIRONMENT HAL: android.hardware.keymaster@4.1::IKeymasterDevice/default
6,1313,26710200,-;tas2563 0-004c: header size: 112, line: 1192
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1314,26720810,-;tas2563 0-004c: FW i2sMode: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1315,26722727,-;wait_for_keymaster: Using Keymaster HAL: 4 from QTI for encryption.  Security level: TRUSTED_ENVIRONMENT, HAL: android.hardware.keymaster@4.1::IKeymasterDevice/default
6,1316,26724842,-;tas2563 0-004c: fw_parse_data, 1006
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1317,26739038,-;bad ioctl: -1072934383
14,1318,26740929,-;wait_for_keymaster: Keymaster device ready
6,1319,26745461,-;tas2563 0-004c: fw_parse_block_data, 965
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1320,26759072,-;tas2563 0-004c: fw_parse_block_data, 969
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1321,26764092,-;tas2563 0-004c: fw_parse_block_data, 994
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1322,26769129,-;tas2563 0-004c: program data number: 16564
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1323,26774297,-;tas2563 0-004c: program size: 16655, line: 1209
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1324,26779968,-;tas2563 0-004c: configuration, mnProgram: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1325,26783186,-;bad ioctl: -1072934383
6,1326,26785214,-;tas2563 0-004c: configuration samplerate: 48000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1327,26794262,-;tas2563 0-004c: Fs rate: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1328,26798083,-;tas2563 0-004c: fw_parse_data, 1006
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1329,26802670,-;tas2563 0-004c: fw_parse_block_data, 965
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1330,26806100,-;vdc: Waited 0ms for vold
6,1331,26807662,-;tas2563 0-004c: fw_parse_block_data, 969
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1332,26812696,-;tas2563 0-004c: fw_parse_block_data, 994
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1333,26817685,-;tas2563 0-004c: fw_parse_block_data, 965
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1334,26822735,-;tas2563 0-004c: fw_parse_block_data, 969
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
36,1335,26823459,-;type=1400 audit(5100.819:13): avc: denied { kill } for comm="vdc" capability=5 scontext=u:r:vdc:s0 tcontext=u:r:vdc:s0 tclass=capability permissive=0
6,1336,26827727,-;tas2563 0-004c: fw_parse_block_data, 994
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1337,26832517,-;bad ioctl: -1072934383
6,1338,26850703,-;tas2563 0-004c: configuration, mnProgram: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1339,26855958,-;tas2563 0-004c: configuration samplerate: 48000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1340,26861625,-;tas2563 0-004c: Fs rate: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1341,26865399,-;tas2563 0-004c: fw_parse_data, 1006
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1342,26870033,-;tas2563 0-004c: fw_parse_block_data, 965
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1343,26875027,-;tas2563 0-004c: fw_parse_block_data, 969
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1344,26876468,-;bad ioctl: -1072934383
6,1345,26880062,-;tas2563 0-004c: fw_parse_block_data, 994
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1346,26888492,-;tas2563 0-004c: fw_parse_block_data, 965
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1347,26893481,-;tas2563 0-004c: fw_parse_block_data, 969
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1348,26897437,-;vdc: Waited 0ms for vold
6,1349,26898528,-;tas2563 0-004c: fw_parse_block_data, 994
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1350,26903516,-;tas2563 0-004c: config size: 3914, line: 1217
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1351,26908969,-;tas2563 0-004c: calib size: 0, line: 1227
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1352,26914116,-;tas2563 0-004c: tas2563_fw_ready:  set program : 0 
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,1353,26920105,-;tas2563 0-004c: tas2563_set_program() :  program : 0, config : -1, chl = 3 
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1354,26928149,-;tas2563 0-004c: find default configuration 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1355,26928377,-;bad ioctl: -1072934383
3,1356,26933816,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,1357,26978342,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:1, VAL: 0x01
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1358,26985296,-;bad ioctl: -1072934383
6,1359,26998150,-;tas2563 0-004c: load program 0 (Tuning Mode)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1360,27003494,-;tas2563 0-004c: TAS2563 load data: TuningMode Program, Blocks = 1, Block Type = 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1361,27012099,-;tas2563 0-004c: TAS2563 load block: Type = 1, commands = 4108
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1362,27017140,-;fsck.f2fs: Info: Fix the reported corruption.
7,1363,27019171,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:126, VAL: 0x00
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1364,27024850,-;fsck.f2fs: \x09Info: No support kernel version!
7,1365,27024956,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:1:2, VAL: 0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1366,27030422,-;fsck.f2fs: Info: Segments per section = 1
6,1367,27032119,-;bad ioctl: -1072934383
7,1368,27032213,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:1:8, len: 0x2c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1369,27034240,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:1:56, len: 0x48
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1370,27035592,-;fsck.f2fs: Info: Sections per zone = 1
7,1371,27037487,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:2:16, len: 0x70
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
36,1372,27041312,-;type=1400 audit(5101.039:14): avc: denied { kill } for comm="fsck.f2fs" capability=5 scontext=u:r:fsck:s0 tcontext=u:r:fsck:s0 tclass=capability permissive=0
14,1373,27043831,-;fsck.f2fs: Info: sector size = 4096
7,1374,27059055,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:3:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1375,27063552,-;fsck.f2fs: Info: total sectors = 12752307 (49813 MB)
7,1376,27066981,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:4:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1377,27069685,-;fsck.f2fs: Info: MKFS version
7,1378,27073047,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:5:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1379,27073745,-;fsck.f2fs:   "4.4.0-62-generic #83-Ubuntu SMP Wed Jan 18 14:10:15 UTC 2017"
7,1380,27077165,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:6:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1381,27081827,-;fsck.f2fs: Info: FSCK version
6,1382,27082770,-;bad ioctl: -1072934383
7,1383,27085420,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:7:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1384,27085878,-;fsck.f2fs:   from "4.19.152+ #1 SMP PREEMPT Thu Feb 11 20:52:22 CST 2021"
7,1385,27088856,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:8:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1386,27092293,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:9:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1387,27100634,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:10:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1388,27104061,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:11:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1389,27107481,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:12:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1390,27110908,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:13:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1391,27114350,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:14:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1392,27115712,-;F2FS-fs (dm-5): Reduce reserved blocks for root = 3972
7,1393,27117783,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:15:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1394,27129842,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:16:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1395,27132964,-;bad ioctl: -1072934383
7,1396,27133287,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:17:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1397,27151414,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:18:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1398,27154884,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:19:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1399,27158388,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:20:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1400,27161870,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:21:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1401,27165342,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:22:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1402,27168820,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:23:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1403,27172313,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:24:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1404,27175774,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:25:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1405,27179278,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:26:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1406,27180642,-;bad ioctl: -1072934383
7,1407,27182773,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:27:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1408,27187577,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:28:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1409,27191141,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:29:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1410,27194597,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:30:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1411,27198140,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:31:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1412,27201604,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:32:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1413,27205075,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:33:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1414,27208530,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:34:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1415,27211995,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:35:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1416,27215456,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:36:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1417,27218924,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:37:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1418,27222398,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:38:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1419,27225871,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:39:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1420,27228504,-;bad ioctl: -1072934383
7,1421,27229351,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:40:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1422,27235409,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:41:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1423,27239027,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:42:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1424,27242514,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:43:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1425,27244770,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 140:44:8, len: 0x48
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1426,27246428,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:1:28, len: 0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1427,27247459,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:1:60, len: 0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1428,27248602,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:1:92, len: 0x24
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1429,27249138,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:2:8, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1430,27249961,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:2:12, len: 0x18
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1431,27252495,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:2:36, len: 0x5c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1432,27255240,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:3:8, len: 0x5c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1433,27256055,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:3:104, len: 0x18
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1434,27259496,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:4:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1435,27260428,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:5:8, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1436,27261203,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:5:80, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1437,27262027,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:6:20, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1438,27262750,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:6:84, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1439,27264992,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:15:56, len: 0x48
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1440,27268438,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:16:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1441,27271889,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:17:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1442,27275345,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:18:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1443,27275890,-;bad ioctl: -1072934383
5,1444,27278947,-;F2FS-fs (dm-5): Mounted with checkpoint version = 59359e5b
7,1445,27286212,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:19:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1446,27289650,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:20:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1447,27293101,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:21:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
36,1448,27296080,-;type=1400 audit(5101.289:15): avc: denied { kill } for comm="vdc" capability=5 scontext=u:r:vdc:s0 tcontext=u:r:vdc:s0 tclass=capability permissive=0
7,1449,27310660,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:22:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1450,27314097,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:23:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1451,27317529,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:24:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1452,27320971,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:25:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1453,27323521,-;bad ioctl: -1072934383
7,1454,27324400,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:26:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1455,27330428,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:27:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1456,27333870,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:28:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1457,27337301,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:29:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1458,27340735,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:30:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1459,27344151,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:31:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1460,27347568,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:32:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1461,27351063,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:33:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1462,27354508,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:34:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1463,27357966,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:35:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1464,27361521,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:36:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1465,27364988,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:37:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1466,27368466,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:38:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1467,27371968,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:39:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1468,27372941,-;bad ioctl: -1072934383
7,1469,27376414,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:40:8, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1470,27381430,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:41:48, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1471,27382388,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:42:56, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1472,27383126,-;vdc: Waited 0ms for vold
7,1473,27383241,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:43:28, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1474,27385809,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:50:44, len: 0x54
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1475,27389289,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:51:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1476,27392769,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:52:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1477,27396193,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:53:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1478,27399624,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:54:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1479,27403049,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:55:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1480,27406490,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:56:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1481,27409946,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:57:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1482,27413406,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:58:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1483,27414237,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:59:8, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1484,27417085,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:59:24, len: 0x68
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1485,27420547,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:60:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1486,27421128,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 100:61:8, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1487,27423043,-;bad ioctl: -1072934383
7,1488,27426516,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:12, len: 0x74
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1489,27430068,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1490,27433535,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1491,27435022,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:8, len: 0x28
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1492,27436779,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:64, len: 0x3c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1493,27437122,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:124, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1494,27440574,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:6:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1495,27440941,-;vdc: Waited 0ms for vold
7,1496,27441087,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:8, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1497,27441505,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:12, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1498,27441921,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:120, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1499,27445355,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1500,27446065,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:9:8, len: 0x0c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1501,27446671,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:9:28, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1502,27447077,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:9:52, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1503,27449503,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:10:48, len: 0x50
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1504,27452934,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:11:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1505,27456383,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:12:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1506,27459843,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:13:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1507,27462993,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:14:8, len: 0x6c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1508,27463410,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:14:116, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1509,27463715,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:14:124, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1510,27467165,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:15:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1511,27470620,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:16:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1512,27473343,-;bad ioctl: -1072934383
7,1513,27476820,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:17:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1514,27478369,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:8, len: 0x2c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1515,27480511,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:52, len: 0x4c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1516,27483945,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1517,27487366,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:20:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1518,27490808,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:21:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1519,27498217,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:22:8, len: 0x70
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1520,27498532,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:22:120, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1521,27498844,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:22:124, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1522,27502269,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:23:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1523,27505710,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:24:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1524,27509160,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:25:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1525,27512601,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:26:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1526,27516051,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:27:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1527,27519501,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:28:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1528,27522319,-;bad ioctl: -1072934383
7,1529,27525802,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:29:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1530,27529278,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:30:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1531,27532719,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:31:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1532,27536155,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:32:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1533,27536593,-;fscrypt: AES-256-CTS-CBC using implementation "cts(cbc-aes-ce)"
7,1534,27539586,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:33:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1535,27547013,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:34:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1536,27550547,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:35:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1537,27553973,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:36:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1538,27557426,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:37:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1539,27560866,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:38:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1540,27564657,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:39:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1541,27568226,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:40:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1542,27570347,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:41:8, len: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1543,27570382,-;bad ioctl: -1072934383
7,1544,27570828,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:253:13, VAL: 0x0d
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1545,27588123,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:253:50, VAL: 0x49
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1546,27588478,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:253:63, VAL: 0x21
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1547,27588707,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:253:25, VAL: 0x80
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1548,27588928,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:253:13, VAL: 0x0d
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1549,27589146,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:253:95, VAL: 0xc1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1550,27589576,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:10, VAL: 0x03
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1551,27589793,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1552,27590012,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xa6
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1553,27590229,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1554,27590447,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:29, VAL: 0xff
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1555,27590661,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:48, VAL: 0x19
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1556,27590874,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:50, VAL: 0x81
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1557,27591088,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:56, VAL: 0x00
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1558,27591311,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:48, VAL: 0x19
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1559,27591523,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:51, VAL: 0x34
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1560,27591734,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:52, VAL: 0x4b
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1561,27591954,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:53, VAL: 0x84
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1562,27592171,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:60, VAL: 0x38
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1563,27592709,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:96, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1564,27594155,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:20, len: 0x30
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1565,27594683,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:92, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1566,27594998,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:96, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1567,27595319,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:100, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1568,27595634,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:104, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1569,27595948,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:108, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1570,27596277,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:112, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1571,27596604,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:116, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1572,27596929,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:120, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1573,27597253,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:124, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1574,27597787,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:8, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1575,27598181,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:12, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1576,27598510,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:16, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1577,27598851,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:84, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1578,27599174,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:108, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1579,27599598,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:4, VAL: 0xc6
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1580,27599816,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:10, VAL: 0x03
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1581,27600037,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:18, VAL: 0x12
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1582,27600254,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:19, VAL: 0x76
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1583,27600470,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:20, VAL: 0x01
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1584,27600683,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:21, VAL: 0x2e
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1585,27600899,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:23, VAL: 0x0e
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1586,27601113,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:25, VAL: 0x00
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1587,27601325,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:51, VAL: 0x34
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1588,27601538,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:52, VAL: 0x4b
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1589,27601753,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:59, VAL: 0x38
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1590,27601970,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:62, VAL: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1591,27602185,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:64, VAL: 0xb6
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1592,27602399,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:65, VAL: 0x41
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1593,27602822,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:1:8, VAL: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1594,27603432,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:12, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1595,27603750,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:16, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1596,27604268,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:104, len: 0x0c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1597,27604586,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:20, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1598,27604900,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:24, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1599,27605214,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:28, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1600,27605531,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:32, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1601,27606391,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:36, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1602,27606828,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:40, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1603,27607151,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:44, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1604,27607477,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:92, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1605,27607795,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:2:100, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1606,27608943,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:100, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1607,27609811,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:64, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1608,27610205,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:4:76, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1609,27610741,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:36, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1610,27611065,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:24, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1611,27611392,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:28, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1612,27611718,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:32, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1613,27612044,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:3:40, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1614,27612478,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:4, VAL: 0xc6
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1615,27612716,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:10, VAL: 0x03
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1616,27613392,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:49, VAL: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1617,27614209,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:9:52, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1618,27614539,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:9:56, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1619,27614548,-;tas2563 0-004c: tas2563_dev_read: chn: 1 chn_num: 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1620,27615106,-;tas2563 0-004c: tas2563_dev_read: chn:4c:BOOK:PAGE:REG 0:0:126,0xbf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,1621,27615115,-;tas2563 0-004c: Block PChkSum Left Channel: FW = 0xbf, Reg = 0xbf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1622,27618697,-;apexd: This device does not support updatable APEX. Exiting
6,1623,27619134,-;bad ioctl: -1072934383
6,1624,27622375,-;tas2563 0-004c: Block[0x1] Left  PChkSum match
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,1625,27629015,-;apexd: Marking APEXd as activated
6,1626,27632349,-;tas2563 0-004c: TAS2563 load data: TuningMode Program, Blocks = 1, Block Type = 8
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1627,27650869,-;tas2563 0-004c: load configuration configuration_Tuning Mode_48 KHz_s1_0 conefficient pre block
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1628,27660689,-;tas2563 0-004c: TAS2563 load data: V0.0, Blocks = 2, Block Type = 4
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1629,27662888,-;bad ioctl: -1072934383
6,1630,27668024,-;tas2563 0-004c: TAS2563 load block: Type = 4, commands = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1631,27678008,-;tas2563 0-004c: TAS2563 load data: V0.0, Blocks = 2, Block Type = 11
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1632,27685466,-;tas2563 0-004c: load new configuration: configuration_Tuning Mode_48 KHz_s1_0, coeff block data
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1633,27695269,-;tas2563 0-004c: TAS2563 load data: V0.0, Blocks = 2, Block Type = 3
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1634,27702642,-;tas2563 0-004c: TAS2563 load block: Type = 3, commands = 432
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1635,27709624,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:126, VAL: 0x00
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1636,27710131,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:84, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1637,27710836,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:8, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1638,27711546,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:28, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1639,27711858,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:5:88, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1640,27712779,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:6:60, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1641,27713492,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:6:80, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1642,27714104,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:120, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1643,27714845,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:8, len: 0x0c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1644,27715555,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:20, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1645,27715654,-;bad ioctl: -1072934383
7,1646,27716266,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:40, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1647,27719822,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:60, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1648,27720579,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:80, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1649,27721103,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:12, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1650,27722218,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:8:100, len: 0x1c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1651,27722939,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:9:8, len: 0x0c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1652,27725366,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:10:48, len: 0x50
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1653,27728801,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:11:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1654,27731618,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:12:8, len: 0x60
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1655,27732029,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:12:120, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1656,27732641,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:13:12, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1657,27733045,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:13:24, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1658,27735550,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:13:36, len: 0x5c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1659,27738961,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:14:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1660,27742378,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:15:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1661,27745789,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:16:8, len: 0x78
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1662,27748410,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:17:8, len: 0x58
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1663,27748986,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:92, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1664,27749305,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:96, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1665,27749622,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:104, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1666,27750243,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:112, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1667,27751680,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:20:8, len: 0x28
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1668,27752299,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:20:112, len: 0x10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1669,27753732,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:21:8, len: 0x28
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1670,27754257,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:108, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1671,27754780,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:20:108, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1672,27755693,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:52, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1673,27756658,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:19:52, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1674,27757231,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:16, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1675,27758497,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:17:96, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1676,27759029,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:17:116, len: 0x0c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1677,27759684,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:8, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1678,27760000,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:16, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1679,27760436,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:20, len: 0x08
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1680,27761190,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:28, len: 0x14
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1681,27761523,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:18:48, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1682,27762067,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:12, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1683,27762516,-;tas2563 0-004c: tas2563_dev_bulk_write: chn4c:BOOK:PAGE:REG 0:7:16, len: 0x04
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1684,27762526,-;tas2563 0-004c: tas2563_dev_read: chn: 1 chn_num: 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1685,27763103,-;tas2563 0-004c: tas2563_dev_read: chn:4c:BOOK:PAGE:REG 0:0:126,0x4c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,1686,27763111,-;tas2563 0-004c: Block PChkSum Left Channel: FW = 0x4c, Reg = 0x4c
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1687,27764198,-;bad ioctl: -1072934383
6,1688,27770352,-;tas2563 0-004c: Block[0x3] Left  PChkSum match
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1689,27779272,-;tas2563 0-004c: TAS2563 load data: V0.0, Blocks = 2, Block Type = 10
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1690,27786707,-;tas2563 0-004c: tas2563_load_default, 1714, ret = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1691,27792688,-;tas2563 0-004c: tas2563_set_slot, slot_width:0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1692,27798214,-;tas2563 0-004c: tas2563_load_default, 1719, ret = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1693,27804384,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:10, VAL: 0xf3
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1694,27804608,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:10, VAL: 0x13
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1695,27804617,-;tas2563 0-004c: INV format: NBNF
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1696,27809314,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:7, mask: 0x1, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1697,27809649,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:7, mask: 0x3e, val: 0x2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1698,27809657,-;tas2563 0-004c: tas2563_load_default, 1739, ret = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1699,27815601,-;tas2563 0-004c: tas2563_set_bitwidth 1565
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1700,27817923,-;bad ioctl: -1072934383
6,1701,27820721,-;tas2563 0-004c: Not supported params format
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1702,27829418,-;tas2563 0-004c: tas2563_set_slot, slot_width:0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1703,27834932,-;tas2563 0-004c: mnCh_size: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1704,27838923,-;tas2563 0-004c: tas2563_load_default, 1744, ret = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1705,27844868,-;tas2563 0-004c: tas2563_set_samplerate, unsupported sample rate, 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1706,27852701,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:26, mask: 0x4, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1707,27853513,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:1:49, mask: 0x2, val: 0x2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1708,27854281,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:48, mask: 0x40, val: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1709,27854827,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:11, mask: 0xff, val: 0x42
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1710,27855350,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1711,27855358,-;tas2563 0-004c: tas2563_load_default, 1775, ret = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1712,27861909,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:2, mask: 0xc, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,1713,27861920,-;tas2563 0-004c: tas2563_set_program() : finish 
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1714,27867725,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:2, VAL: 0x0e
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,1715,27868500,-;bad ioctl: -1072934383
7,1716,27868739,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:48, mask: 0x4, val: 0x4
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,1717,27871928,-;tas2563 0-004c: tas2563_fw_ready: finish
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,1718,27877137,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:5, VAL: 0x20
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
15,1719,27913953,-;vdc: Waited 0ms for vold
6,1720,27915531,-;bad ioctl: -1072934383
6,1721,27962847,-;bad ioctl: -1072934383
6,1722,28010165,-;bad ioctl: -1072934383
6,1723,28057447,-;bad ioctl: -1072934383
6,1724,28104795,-;bad ioctl: -1072934383
6,1725,28152124,-;bad ioctl: -1072934383
14,1726,28159809,-;apexd: This device does not support updatable APEX. Exiting
14,1727,28166482,-;apexd: Marking APEXd as ready
6,1728,28200012,-;bad ioctl: -1072934383
6,1729,28247646,-;bad ioctl: -1072934383
6,1730,28295498,-;bad ioctl: -1072934383
6,1731,28343693,-;bad ioctl: -1072934383
6,1732,28392144,-;bad ioctl: -1072934383
6,1733,28440912,-;bad ioctl: -1072934383
6,1734,28489199,-;bad ioctl: -1072934383
6,1735,28537922,-;bad ioctl: -1072934383
6,1736,28585808,-;bad ioctl: -1072934383
6,1737,28633627,-;bad ioctl: -1072934383
6,1738,28681722,-;bad ioctl: -1072934383
14,1739,28685736,-;update_verifier: Started with arg 1: nonencrypted
14,1740,28699904,-;update_verifier: Booting slot 0: isSlotMarkedSuccessful=1
14,1741,28706404,-;update_verifier: Leaving update_verifier.
6,1742,28729215,-;bad ioctl: -1072934383
6,1743,28780573,-;bad ioctl: -1072934383
4,1744,28799638,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.mdt
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1745,28809344,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.mdt
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
14,1746,28832472,-;ueventd: firmware: loading 'adsp.mdt' for '/devices/platform/soc/ab00000.qcom,lpass/firmware/adsp.mdt'
6,1747,28837247,-;bad ioctl: -1072934383
6,1748,28850390,-;subsys-pil-tz ab00000.qcom,lpass: adsp: loading from 0x0000000053800000 to 0x0000000055400000
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
14,1749,28851093,-;ueventd: loading /devices/platform/soc/ab00000.qcom,lpass/firmware/adsp.mdt took 19ms
14,1750,28852113,-;ueventd: firmware: loading 'cdsp.mdt' for '/devices/platform/soc/b300000.qcom,turing/firmware/cdsp.mdt'
6,1751,28862739,-;subsys-pil-tz b300000.qcom,turing: cdsp: loading from 0x0000000051a00000 to 0x0000000053800000
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
14,1752,28863044,-;ueventd: loading /devices/platform/soc/b300000.qcom,turing/firmware/cdsp.mdt took 13ms
6,1753,28893926,-;bad ioctl: -1072934383
11,1754,28898701,-;ueventd: firmware: could not find firmware for dsi_prop
11,1755,28908577,-;ueventd: firmware: attempted /etc/firmware/dsi_prop, open failed: No such file or directory
11,1756,28918168,-;ueventd: firmware: attempted /odm/firmware/dsi_prop, open failed: No such file or directory
11,1757,28931913,-;ueventd: firmware: attempted /vendor/firmware/dsi_prop, open failed: No such file or directory
6,1758,28942165,-;[drm:dsi_display_firmware_display] [msm-dsi-info]: no firmware available, fallback to device node
4,1759,28945492,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b02
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1760,28949008,-;bad ioctl: -1072934383
3,1761,28952445,-;OF: graph: no port node found in /soc/qcom,dsi-display-primary
4,1762,28953882,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b03
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1763,28954529,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b04
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1764,28958734,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b05
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1765,28958973,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b06
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1766,28961701,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b07
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1767,28961868,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b08
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1768,28964341,-;[drm] [msm-dsi-warn]: [FT8006M 720P video mode dsi panel] fallback to default te-pin-select
4,1769,28969914,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b09
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1770,28970926,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b10
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1771,28972118,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b12
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1772,28973403,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b13
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1773,28974510,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b14
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1774,28975226,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b15
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1775,28976420,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b16
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1776,28979046,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b17
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1777,28980434,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b18
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1778,28981940,-;msm_drm 5e00000.qcom,mdss_mdp: Linked as a consumer to regulator.10
 SUBSYSTEM=platform
 DEVICE=+platform:5e00000.qcom,mdss_mdp
6,1779,28984889,-;[drm:sde_dbg_init:4738] evtlog_status: enable:11, panic:1, dump:2
6,1780,28986646,-;msm-dsi-display soc:qcom,dsi-display-primary: Linked as a consumer to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,dsi-display-primary
6,1781,28987119,-;msm-dsi-display soc:qcom,dsi-display-primary: Linked as a consumer to regulator.46
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,dsi-display-primary
6,1782,28987574,-;msm-dsi-display soc:qcom,dsi-display-primary: Linked as a consumer to regulator.47
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,dsi-display-primary
4,1783,28996585,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b19
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1784,29006076,-;bad ioctl: -1072934383
4,1785,29006550,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b20
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1786,29012997,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b21
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1787,29015146,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b22
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1788,29016709,-;[drm:dsi_display_bind] [msm-dsi-info]: Successfully bind display panel 'qcom,mdss_dsi_ft8006m_720p_techstar_video'
4,1789,29017338,-;irq 131, desc: ffffffc0f63ca880, depth: 0, count: 0, unhandled: 0
6,1790,29017347,-;msm_drm 5e00000.qcom,mdss_mdp: bound soc:qcom,dsi-display-primary (ops dsi_display_comp_ops)
 SUBSYSTEM=platform
 DEVICE=+platform:5e00000.qcom,mdss_mdp
4,1791,29017356,-;->handle_irq():  ffffff80085d8c58, msm_gpio_irq_handler+0x0/0x1a0
4,1792,29017363,-;->irq_data.chip(): ffffff800a5d2190, msm_mpm_gic_chip+0x0/0x110
4,1793,29017365,-;->action(): ffffff800a57e880
4,1794,29017371,-;->action->handler(): ffffff80081675e0, bad_chained_irq+0x0/0x50
4,1795,29017373,-;     IRQ_LEVEL set
4,1796,29017375,-;   IRQ_NOPROBE set
4,1797,29017377,-; IRQ_NOREQUEST set
4,1798,29017379,-;  IRQ_NOTHREAD set
6,1799,29017437,-;[drm] mapped mdp address space @ffffff8018600000
4,1800,29018811,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b23
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1801,29019723,-;[drm:_sde_kms_hw_init_blocks:3588] sde hardware revision:0x60030000
4,1802,29021155,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b24
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1803,29023517,-;msmdrm_smmu 5e00000.qcom,mdss_mdp:qcom,smmu_sde_unsec_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:5e00000.qcom,mdss_mdp:qcom,smmu_sde_unsec_cb
6,1804,29026662,-;iommu: Adding device 5e00000.qcom,mdss_mdp:qcom,smmu_sde_unsec_cb to group 36
4,1805,29026838,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b25
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1806,29027685,-;[drm] probing device qcom,smmu_sde_unsec
6,1807,29027709,-;[drm] Created domain mdp_ns, secure=0
4,1808,29032188,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b26
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1809,29032865,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b27
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1810,29039208,-;msmdrm_smmu 5e00000.qcom,mdss_mdp:qcom,smmu_sde_sec_cb: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:5e00000.qcom,mdss_mdp:qcom,smmu_sde_sec_cb
4,1811,29039475,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b29
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1812,29040045,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b28
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1813,29058962,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b30
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1814,29061370,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b31
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1815,29066025,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b32
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1816,29067443,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1817,29069757,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b33
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1818,29072809,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b34
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
4,1819,29086460,-;subsys-pil-tz ab00000.qcom,lpass: Falling back to syfs fallback for: adsp.b35
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1820,29089000,-;bad ioctl: -1072934383
6,1821,29089031,-;iommu: Adding device 5e00000.qcom,mdss_mdp:qcom,smmu_sde_sec_cb to group 37
6,1822,29090095,-;[drm] probing device qcom,smmu_sde_sec
6,1823,29090126,-;[drm] Created domain mdp_s, secure=1
6,1824,29092949,-;[drm:dsi_panel_get_mode] [msm-dsi-info]: default topology: lm: 1 comp_enc:0 intf: 1
4,1825,29099089,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b02
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
4,1826,29099848,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1827,29102593,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b03
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
4,1828,29103491,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b04
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
4,1829,29106890,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b05
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
4,1830,29113210,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b06
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
4,1831,29124975,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b08
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
4,1832,29125245,-;subsys-pil-tz b300000.qcom,turing: Falling back to syfs fallback for: cdsp.b10
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
6,1833,29127976,-;[drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
6,1834,29176056,-;bad ioctl: -1072934383
6,1835,29181538,-;[drm] No driver support for vblank timestamp query.
6,1836,29196189,-;[drm] Initialized msm_drm 1.3.0 20130625 for 5e00000.qcom,mdss_mdp on minor 0
6,1837,29266698,-;bad ioctl: -1072934383
6,1838,29268438,-;[drm] cont_splash feature not enabled
6,1839,29570590,-;subsys-pil-tz ab00000.qcom,lpass: adsp: Brought out of reset
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1840,29594350,-;bad ioctl: -1072934383
6,1841,29608868,-;subsys-pil-tz b300000.qcom,turing: cdsp: Brought out of reset
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
6,1842,29623611,-;subsys-pil-tz b300000.qcom,turing: Subsystem error monitoring/handling services are up
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
6,1843,29632745,-;subsys-pil-tz b300000.qcom,turing: cdsp: Power/Clock ready interrupt received
 SUBSYSTEM=platform
 DEVICE=+platform:b300000.qcom,turing
6,1844,29644917,-;bad ioctl: -1072934383
6,1845,29650824,-;adsprpc: fastrpc_restart_notifier_cb: cdsp subsystem is up
6,1846,29654272,-;adsprpc: fastrpc_rpmsg_probe: opened rpmsg channel for cdsp
4,1847,29660361,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
3,1848,29670070,-;166200771:Entered
3,1849,29674984,-;166200771:SMD QRTR driver probed
4,1850,29682624,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1851,29695684,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1852,29708223,-;subsys-pil-tz ab00000.qcom,lpass: Subsystem error monitoring/handling services are up
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1853,29713836,-;bad ioctl: -1072934383
6,1854,29717175,-;subsys-pil-tz ab00000.qcom,lpass: adsp: Power/Clock ready interrupt received
 SUBSYSTEM=platform
 DEVICE=+platform:ab00000.qcom,lpass
6,1855,29730876,-;adsprpc: fastrpc_restart_notifier_cb: adsp subsystem is up
6,1856,29732222,-;adsprpc: fastrpc_rpmsg_probe: opened rpmsg channel for adsp
4,1857,29751913,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1858,29751987,-;apr_tal_rpmsg qcom,glink:adsp.apr_audio_svc.-1.-1: apr_tal_rpmsg_probe: Channel[apr_audio_svc] state[Up]
 SUBSYSTEM=rpmsg
 DEVICE=+rpmsg:qcom,glink:adsp.apr_audio_svc.-1.-1
3,1859,29773446,-;166200771:Entered
4,1860,29785031,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
3,1861,29792533,-;166200771:SMD QRTR driver probed
4,1862,29806776,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
3,1863,29832106,-;msm_get_platform_subtype: Invalid hardware platform sub type for qrd found
3,1864,30116224,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1865,30123454,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1866,30133057,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1867,30139076,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1868,30145493,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1869,30151320,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1870,30157815,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1871,30163652,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1872,30170490,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1873,30176177,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,1874,30654557,-;init: Service 'exec 18 (/vendor/bin/init.qcom.early_boot.sh)' (pid 706) exited with status 0 waiting took 0.965000 seconds
14,1875,30667098,-;init: Sending signal 9 to service 'exec 18 (/vendor/bin/init.qcom.early_boot.sh)' (pid 706) process group...
14,1876,30679194,-;libprocessgroup: Successfully killed process cgroup uid 0 pid 706 in 0ms
14,1877,30689903,-;init: Command 'exec u:r:vendor_qti_init_shell:s0 -- /vendor/bin/init.qti.can.sh' action=early-boot (/vendor/etc/init/hw/init.qcom.rc:92) took 0ms and failed: Could not start exec service: Cannot find '/vendor/bin/init.qti.can.sh': No such file or directory
14,1878,30734014,-;init: processing action (early-boot) from (/vendor/etc/init/hw/init.target.rc:73)
14,1879,30743267,-;init: processing action (early-boot) from (/system/etc/init/installd.rc:5)
14,1880,30832197,-;init: processing action (early-boot) from (/vendor/etc/init/init.vendor.sensors.rc:32)
14,1881,30849465,-;init: processing action (early-boot) from (/vendor/etc/init/ipa_fws.rc:6)
36,1882,30859023,-;type=1400 audit(1614200565.346:16): avc: denied { create } for comm="init" name="ipa" scontext=u:r:vendor_init:s0 tcontext=u:object_r:vendor_ipa_dev:s0 tclass=file permissive=0
14,1883,30859407,-;init: Command 'write /dev/ipa 1' action=early-boot (/vendor/etc/init/ipa_fws.rc:7) took 1ms and failed: Unable to write to file '/dev/ipa': open() failed: Permission denied
14,1884,30893091,-;init: processing action (boot) from (/system/etc/init/hw/init.rc:866)
36,1885,30917472,-;type=1400 audit(1614200565.396:17): avc: denied { read } for comm="init" name="device" dev="sysfs" ino=48978 scontext=u:r:init:s0 tcontext=u:object_r:vendor_sysfs_graphics:s0 tclass=lnk_file permissive=0
36,1886,30937578,-;type=1400 audit(1614200565.396:18): avc: denied { read } for comm="init" name="device" dev="sysfs" ino=48978 scontext=u:r:init:s0 tcontext=u:object_r:vendor_sysfs_graphics:s0 tclass=lnk_file permissive=0
36,1887,30956945,-;type=1400 audit(1614200565.396:19): avc: denied { read } for comm="init" name="device" dev="sysfs" ino=48978 scontext=u:r:init:s0 tcontext=u:object_r:vendor_sysfs_graphics:s0 tclass=lnk_file permissive=0
12,1888,31266487,-;healthd: Unknown power supply type 'BMS'
12,1889,31272355,-;healthd: Unknown power supply type 'Main'
12,1890,31280189,-;healthd: batteryCapacityLevelPath not found
36,1891,31281036,-;type=1400 audit(1614200565.766:20): avc: denied { read } for comm="android.hardwar" name="type" dev="sysfs" ino=48097 scontext=u:r:hal_health_default:s0 tcontext=u:object_r:sysfs:s0 tclass=file permissive=0
3,1892,31300326,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
36,1893,31305668,-;type=1400 audit(1614200565.766:21): avc: denied { read } for comm="android.hardwar" name="type" dev="sysfs" ino=47804 scontext=u:r:hal_health_default:s0 tcontext=u:object_r:sysfs:s0 tclass=file permissive=0
3,1894,31310618,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1895,31323133,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1896,31342037,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,1897,31352187,-;healthd: battery l=51 v=3711 t=30.7 h=2 st=2 c=-924072 fc=3812000 cc=0 chg=a
3,1898,31362034,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1899,31367730,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1900,31382339,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1901,31388842,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1902,31430167,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1903,31436340,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1904,31447927,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1905,31454596,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1906,31466826,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,1907,31473042,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,1908,31910984,-;QSEECOM: qseecom_load_app: App (soter64) does'nt exist, loading apps for first time
4,1909,31952337,-;QSEECOM: qseecom_load_app: App with id 3 (soter64) now loaded
6,1910,32064791,-;coresight-remote-etm soc:audio_etm0: Connection established between QMI handle and 5 service
 SUBSYSTEM=platform
 DEVICE=+platform:soc:audio_etm0
6,1911,32068827,-;coresight-remote-etm soc:turing_etm0: Connection established between QMI handle and 13 service
 SUBSYSTEM=platform
 DEVICE=+platform:soc:turing_etm0
6,1912,32071524,-;sysmon-qmi: ssctl_new_server: Connection established between QMI handle and cdsp's SSCTL service
6,1913,32071614,-;sysmon-qmi: ssctl_new_server: Connection established between QMI handle and adsp's SSCTL service
3,1914,32075178,-;diag: In diag_send_feature_mask_update, control channel is not open, p: 5, ffffff800b0849b8
3,1915,32115822,-;diag: In diag_send_peripheral_buffering_mode, buffering flag not set for 5
3,1916,32124280,-;diag: In diag_send_peripheral_buffering_mode, buffering flag not set for 1
6,1917,32225463,-;servloc: service_locator_new_server: Connection established with the Service locator
6,1918,32225504,-;servloc: init_service_locator: Service locator initialized
36,1919,32229088,-;type=1400 audit(1614200566.706:22): avc: denied { read } for comm="pm-service" name="name" dev="sysfs" ino=36988 scontext=u:r:vendor_per_mgr:s0 tcontext=u:object_r:sysfs:s0 tclass=file permissive=0
6,1920,32238518,-;adsprpc: fastrpc_get_service_location_notify: PDR notifier for adsp registered for msm/adsp/audio_pd (audio_pdr_adsprpc)
6,1921,32238543,-;service-notifier: service_notifier_new_server: Connection established between QMI handle and 74 service
6,1922,32240721,-;adsprpc: fastrpc_pdr_notifier_cb: msm/adsp/audio_pd (audio_pdr_adsprpc) is up on adsp
6,1923,32259790,-;sps:BAM 0x000000000a584000 (va:0xffffff8016180000) enabled: ver:0x19, number of pipes:13
6,1924,32276155,-;adsprpc: fastrpc_get_service_location_notify: PDR notifier for adsp registered for msm/adsp/sensor_pd (sensors_pdr_adsprpc)
6,1925,32283139,-;sps:BAM 0x000000000a584000 is registered.
31,1926,32303688,-;logd: logdr: UID=1000 GID=1000 PID=833 n tail=50 logMask=8 pid=809 start=0ns timeout=0ns
6,1927,32303721,-;service-notifier: service_notifier_new_server: Connection established between QMI handle and 74 service
6,1928,32304881,-;adsprpc: fastrpc_pdr_notifier_cb: msm/adsp/sensor_pd (sensors_pdr_adsprpc) is up on adsp
4,1929,32307326,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1930,32312595,-;audio_notifer_reg_service: service PDR_ADSP is in use
6,1931,32312607,-;apr_adsp_up: Q6 is Up
31,1932,32322536,-;logd: logdr: UID=1000 GID=1000 PID=833 n tail=50 logMask=1 pid=809 start=0ns timeout=0ns
6,1933,32328237,-;adsprpc: fastrpc_get_service_location_notify: audio_pdr_adsprpc (msm/adsp/audio_pd) PDR service for adsp is uninitialized
4,1934,32340677,-;kgsl kgsl-3d0: Falling back to syfs fallback for: a630_sqe.fw
 SUBSYSTEM=kgsl
 DEVICE=c239:0
31,1935,32342868,-;logd: logdr: UID=1000 GID=1000 PID=833 n tail=0 logMask=8 pid=809 start=0ns timeout=0ns
6,1936,32344299,-;adsprpc: fastrpc_get_service_location_notify: sensors_pdr_adsprpc (msm/adsp/sensor_pd) PDR service for adsp is uninitialized
6,1937,32386886,-;msm-audio-ion soc:qcom,msm-audio-apr:qcom,msm-audio-ion: Linked as a consumer to c600000.apps-smmu
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,msm-audio-ion
14,1938,32394880,-;ueventd: firmware: loading 'a630_sqe.fw' for '/devices/platform/soc/5900000.qcom,kgsl-3d0/kgsl/kgsl-3d0/a630_sqe.fw'
14,1939,32405278,-;rmt_storage:INFO:check_support_using_libmdm: Modem subsystem found on target!
6,1940,32412784,-;iommu: Adding device soc:qcom,msm-audio-apr:qcom,msm-audio-ion to group 38
14,1941,32425914,-;rmt_storage:INFO:main: Done with init now waiting for messages!
14,1942,32426101,-;ueventd: loading /devices/platform/soc/5900000.qcom,kgsl-3d0/kgsl/kgsl-3d0/a630_sqe.fw took 31ms
4,1943,32445776,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1944,32524950,-;subsys-pil-tz soc:qcom,kgsl-hyp: Falling back to syfs fallback for: a610_zap.mdt
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,kgsl-hyp
3,1945,32558204,-;qcom-lpi-pinctrl soc:qcom,msm-audio-apr:qcom,q6core-audio:lpi_pinctrl@ac40000: snd_event_notify: No snd dev entry found
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:lpi_pinctrl@ac40000
14,1946,32560490,-;ueventd: firmware: loading 'a610_zap.mdt' for '/devices/platform/soc/soc:qcom,kgsl-hyp/firmware/a610_zap.mdt'
14,1947,32596427,-;ueventd: loading /devices/platform/soc/soc:qcom,kgsl-hyp/firmware/a610_zap.mdt took 36ms
4,1948,32609522,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: Max WSA devices is 0 for this target?
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
4,1949,32620323,-;bolero-clk-rsc-mngr bolero-clk-rsc-mngr: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:bolero-clk-rsc-mngr
4,1950,32629303,-;va_macro va-macro: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:va-macro
6,1951,32630455,-;va_macro va-macro: bolero_register_macro: register macro successful:3
 SUBSYSTEM=platform
 DEVICE=+platform:va-macro
4,1952,32632565,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1953,32636975,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: Max WSA devices is 0 for this target?
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,1954,32639674,-;Mass Storage Function, version: 2009/09/11
6,1955,32639704,-;LUN: removable file: (no medium)
4,1956,32640602,-;rx_macro rx-macro: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:rx-macro
6,1957,32641763,-;rx_macro rx-macro: bolero_register_macro: register macro successful:1
 SUBSYSTEM=platform
 DEVICE=+platform:rx-macro
4,1958,32642886,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1959,32647628,-;tx_macro tx-macro: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:tx-macro
3,1960,32647756,-;msm_cdc_pinctrl_get_gpiodata: device node is null
4,1961,32655573,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: Max WSA devices is 0 for this target?
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
4,1962,32657437,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1963,32657611,-;tx_macro tx-macro: bolero_register_macro: register macro successful:0
 SUBSYSTEM=platform
 DEVICE=+platform:tx-macro
4,1964,32660684,-;wcd937x_codec wcd937x-codec: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
6,1965,32666790,-;file system registered
4,1966,32670011,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: Max WSA devices is 0 for this target?
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
4,1967,32671995,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
4,1968,32673216,-;swr-wcd rx_swr_ctrl: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:rx_swr_ctrl
4,1969,32674994,-;swr-wcd va_swr_ctrl: DMA mask not set
 SUBSYSTEM=platform
 DEVICE=+platform:va_swr_ctrl
6,1970,32682961,-;f_cdev_alloc: port_name:at_usb0 (ffffffc0a15a6680) portno:(0)
6,1971,32683242,-;subsys-pil-tz soc:qcom,kgsl-hyp: a610_zap: loading from 0x00000000fe100000 to 0x00000000fe101000
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,kgsl-hyp
6,1972,32687170,-;f_cdev_alloc: port_name:at_usb1 (ffffffc09e2a9e80) portno:(1)
6,1973,32691071,-;f_cdev_alloc: port_name:at_usb2 (ffffffc0a1e63080) portno:(2)
4,1974,32742335,-;subsys-pil-tz soc:qcom,kgsl-hyp: Falling back to syfs fallback for: a610_zap.b02
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,kgsl-hyp
4,1975,32753814,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: Max WSA devices is 0 for this target?
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
4,1976,32756029,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,1977,32757191,-;wcd937x_codec wcd937x-codec: msm_cdc_dt_parse_vreg_info: cdc-vdd-rxtx: vol=[1800000 1800000]uV, curr=[10000]uA, ond 0 lpm 0
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
6,1978,32757215,-;wcd937x_codec wcd937x-codec: msm_cdc_dt_parse_vreg_info: cdc-vddpx: vol=[1800000 1800000]uV, curr=[20000]uA, ond 0 lpm 0
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
6,1979,32757237,-;wcd937x_codec wcd937x-codec: msm_cdc_dt_parse_vreg_info: cdc-vdd-buck: vol=[1800000 1800000]uV, curr=[650000]uA, ond 1 lpm 0
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
6,1980,32757798,-;wcd937x_codec wcd937x-codec: Linked as a consumer to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
6,1981,32758799,-;wcd937x_codec wcd937x-codec: Linked as a consumer to regulator.35
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
14,1982,32766442,-;ueventd: firmware: loading 'a610_zap.b02' for '/devices/platform/soc/soc:qcom,kgsl-hyp/firmware/a610_zap.b02'
6,1983,32773289,-;wcd937x_codec wcd937x-codec: bound wcd937x-slave.a01170224 (ops wcd937x_slave_comp_ops [wcd937x_slave_dlkm])
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
6,1984,32773380,-;wcd937x_codec wcd937x-codec: bound wcd937x-slave.a01170223 (ops wcd937x_slave_comp_ops [wcd937x_slave_dlkm])
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
14,1985,32779663,-;ueventd: loading /devices/platform/soc/soc:qcom,kgsl-hyp/firmware/a610_zap.b02 took 13ms
6,1986,32783305,-;subsys-pil-tz soc:qcom,kgsl-hyp: a610_zap: Brought out of reset
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,kgsl-hyp
4,1987,32792371,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: Max WSA devices is 0 for this target?
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,1988,32792408,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_init_aux_dev: found 1 AUX codecs registered with ALSA core
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,1989,32888675,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no source widget found for AUDIO_REF_EC_UL30 MUX
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1990,32898589,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route AUDIO_REF_EC_UL30 MUX -> direct -> MM_UL30
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1991,32911025,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no source widget found for PRI_TDM_TX_3
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1992,32920160,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route PRI_TDM_TX_3 -> PRI_TDM_TX_3_Voip -> Voip_Tx Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1993,32937235,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no source widget found for AUX_PCM_TX
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1994,32946181,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route AUX_PCM_TX -> AUX_PCM_UL_TX -> VoLTE Stub Tx Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1995,32964110,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no source widget found for AUX_PCM_RX
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1996,32973166,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route AUX_PCM_RX -> direct -> BE_OUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1997,32995694,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no sink widget found for SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1998,33005605,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route VOIP_DL -> Voip -> SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,1999,33017028,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no sink widget found for SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,2000,33026937,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route QCHAT_DL -> QCHAT -> SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,2001,33039021,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no sink widget found for SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,2002,33049030,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route VOICEMMODE1_DL -> VoiceMMode1 -> SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,2003,33061606,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no sink widget found for SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,2004,33071561,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route VOICEMMODE2_DL -> VoiceMMode2 -> SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
3,2005,33084019,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: no source widget found for SEN_MI2S_RX_Voice Mixer
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
6,2006,33087467,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor2: Linked as a consumer to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor2
3,2007,33094150,-;msm-pcm-routing soc:qcom,msm-pcm-routing: ASoC: Failed to add route SEN_MI2S_RX_Voice Mixer -> direct -> SEN_MI2S_RX
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-pcm-routing
6,2008,33120330,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor2: Linked as a consumer to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor2
6,2009,33189333,-;CAM_INFO: CAM-SENSOR: cam_sensor_match_id: 630 THIS IS A SCANNER!!
6,2010,33189351,-;ENGINE/I hon_engine_sensor_probe: get pwren gpio 1136, reset gpio 1146
6,2011,33189933,-;CAM_ERR: CAM-CCI: cam_cci_irq: 265 Base:ffffff80131ed000, M1_Q1 NACK ERROR: 0x40000000
3,2012,33818820,-;tas2563 0-004c: tas2563_codec_probe
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,2013,33835584,-;tas2563 0-004c: ASoC: no source widget found for DAC
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,2014,33841668,-;tas2563 0-004c: ASoC: Failed to add route DAC -> direct -> OUT
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2015,33851700,-;wcd937x_codec wcd937x-codec: wcd937x_soc_codec_probe()
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
3,2016,33912825,-;wcd937x_codec wcd937x-codec: ASoC: unknown pin LO
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
3,2017,33928599,-;wcd937x_codec wcd937x-codec: ASoC: unknown pin AMIC4
 SUBSYSTEM=platform
 DEVICE=+platform:wcd937x-codec
3,2018,33958319,-;msm-dai-fe soc:qcom,msm-dai-fe: ASoC: no sink widget found for AUXPCM_DL_HL
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-dai-fe
3,2019,33966357,-;msm-dai-fe soc:qcom,msm-dai-fe: ASoC: Failed to add route AUXPCM_HOSTLESS Playback -> direct -> AUXPCM_DL_HL
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-dai-fe
3,2020,33977493,-;msm-dai-fe soc:qcom,msm-dai-fe: ASoC: no source widget found for AUXPCM_UL_HL
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-dai-fe
3,2021,33985739,-;msm-dai-fe soc:qcom,msm-dai-fe: ASoC: Failed to add route AUXPCM_UL_HL -> direct -> AUXPCM_HOSTLESS Capture
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-dai-fe
6,2022,34642663,-;[drm:dsi_display_set_mode] [msm-dsi-info]: mdp_transfer_time_us=0 us
6,2023,34642676,-;[drm:dsi_display_set_mode] [msm-dsi-info]: hactive= 720,vactive= 1280,fps=60
6,2024,34643080,-;[drm:dsi_ctrl_isr_configure] [msm-dsi-info]: dsi-ctrl-0: IRQ 303 registered
3,2025,34722231,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no sink widget found for AMIC4
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2026,34728287,-;CAM_ERR: CAM-CCI: cam_cci_read: 1305 wait_for_completion_timeout rc = -110 FIFO buf_lvl: 0x0
3,2027,34732576,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route MIC BIAS3 -> direct -> AMIC4
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2028,34732668,-;CAM_ERR: CAM-CCI: cam_cci_read_bytes_v_1_2: 1575 failed to read rc:-110
6,2029,34744750,-;CAM_ERR: CAM-SENSOR: cam_cci_i2c_read: 35 rc = -110
6,2030,34744760,-;ENGINE/E hon_engine_sensor_probe: failed to read sensor id
3,2031,34745896,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no sink widget found for SpkrMono WSA_IN
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2032,34752883,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor2: Dropping the link to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor2
3,2033,34757002,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route AUX -> direct -> SpkrMono WSA_IN
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2034,34757505,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for ADC3_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2035,34764955,-;[FTS][Info]invalid point_num(15)
6,2036,34773382,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor2: Dropping the link to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor2
3,2037,34780124,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route ADC3_OUTPUT -> direct -> TX SWR_MIC5
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2038,34780349,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC1_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2039,34786922,-;pll_vco_round_rate_14nm: rate=4347715680 NOT supportted
3,2040,34786938,-;pll_vco_round_rate_14nm: rate=4347715680 NOT supportted
3,2041,34786953,-;pll_vco_round_rate_14nm: rate=4347715680 NOT supportted
3,2042,34787036,-;pll_vco_round_rate_14nm: rate=4347715680 NOT supportted
3,2043,34787050,-;pll_vco_round_rate_14nm: rate=4347715680 NOT supportted
3,2044,34787063,-;pll_vco_round_rate_14nm: rate=4347715680 NOT supportted
6,2045,34826352,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Linked as a consumer to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2046,34828810,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC1_OUTPUT -> direct -> TX SWR_MIC8
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2047,34829036,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC2_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2048,34844425,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Linked as a consumer to regulator.50
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2049,34854081,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC2_OUTPUT -> direct -> TX SWR_MIC9
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2050,34854317,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC3_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2051,34871551,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Linked as a consumer to regulator.53
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2052,34877852,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC3_OUTPUT -> direct -> TX SWR_MIC8
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2053,34878193,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC4_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2054,34896168,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2055,34901431,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC4_OUTPUT -> direct -> TX SWR_MIC9
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2056,34901661,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC5_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2057,34930326,-;CAM_INFO: CAM-SENSOR: cam_sensor_match_id: 643 read id: 0x253 expected id 0x253:
3,2058,34936119,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC5_OUTPUT -> direct -> TX SWR_MIC10
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2059,34936364,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC6_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2060,34949202,-;CAM_INFO: CAM-SENSOR: cam_sensor_driver_cmd: 739 Probe success,slot:0,slave_addr:0x6c,sensor_id:0x253
3,2061,34959920,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC6_OUTPUT -> direct -> TX SWR_MIC11
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2062,34962039,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for ADC3_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2063,34962912,-;wlan: Loading driver v5.2.05.23C +TIMER_MANAGER +MEMORY_DEBUG +PANIC_ON_BUG; 2021-02-11T13:13:06Z; cld:; cmn:;
6,2064,34962933,-;qdf_print_ctrl_register: Allocated print control object 0
6,2065,34972896,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Dropping the link to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2066,34983548,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route ADC3_OUTPUT -> direct -> VA SWR_MIC5
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2067,34983779,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC1_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2068,35001016,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Dropping the link to regulator.53
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2069,35007310,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC1_OUTPUT -> direct -> VA SWR_MIC8
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2070,35010141,-;ipa_uc_reg_rdyCB:2154 IPA HW is not supported
6,2071,35019672,-;wlan_hdd_state wlan major(500) initialized
6,2072,35025154,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Dropping the link to regulator.50
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2073,35031164,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC2_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2074,35043212,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor0: Dropping the link to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor0
3,2075,35047416,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC2_OUTPUT -> direct -> VA SWR_MIC9
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2076,35060297,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC3_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2077,35071443,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC3_OUTPUT -> direct -> VA SWR_MIC8
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2078,35084274,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC4_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2079,35095347,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC4_OUTPUT -> direct -> VA SWR_MIC9
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2080,35108311,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC5_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2081,35119440,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC5_OUTPUT -> direct -> VA SWR_MIC10
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2082,35132423,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no source widget found for DMIC6_OUTPUT
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
3,2083,35143467,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: Failed to add route DMIC6_OUTPUT -> direct -> VA SWR_MIC11
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
4,2084,35156200,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: ASoC: no DMI vendor name!
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
6,2085,35165976,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor3: Linked as a consumer to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor3
6,2086,35174306,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor3: Linked as a consumer to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor3
6,2087,35257790,-;input: bengal-qrd-snd-card Headset Jack as /devices/platform/soc/soc:qcom,msm-audio-apr/soc:qcom,msm-audio-apr:qcom,q6core-audio/soc:qcom,msm-audio-apr:qcom,q6core-audio:sound/sound/card0/input4
6,2088,35259642,-;input: bengal-qrd-snd-card Button Jack as /devices/platform/soc/soc:qcom,msm-audio-apr/soc:qcom,msm-audio-apr:qcom,q6core-audio/soc:qcom,msm-audio-apr:qcom,q6core-audio:sound/sound/card0/input5
6,2089,35261768,-;bengal-asoc-snd soc:qcom,msm-audio-apr:qcom,q6core-audio:sound: msm_asoc_machine_probe: Sound card bengal-qrd-snd-card registered
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,msm-audio-apr:qcom,q6core-audio:sound
4,2090,35268881,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,2091,35394429,-;CAM_INFO: CAM-SENSOR: cam_sensor_match_id: 630 THIS IS A SCANNER!!
6,2092,35394440,-;ENGINE/I hon_engine_sensor_probe: get pwren gpio 1136, reset gpio 1146
6,2093,35394453,-;ENGINE/E hon_engine_power_on_init: failed to request illum gpio 1235
6,2094,35394460,-;ENGINE/E hon_engine_sensor_probe: failed to do power on initialize
6,2095,35401478,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor3: Dropping the link to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor3
6,2096,35405010,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor3: Dropping the link to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor3
6,2097,35432525,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Linked as a consumer to regulator.55
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2098,35440851,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Linked as a consumer to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2099,35448291,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Linked as a consumer to regulator.51
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2100,35488379,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Linked as a consumer to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2101,35506423,-;CAM_INFO: CAM-SENSOR: cam_sensor_match_id: 643 read id: 0x487b expected id 0x487b:
6,2102,35506435,-;CAM_INFO: CAM-SENSOR: cam_sensor_driver_cmd: 739 Probe success,slot:1,slave_addr:0x5a,sensor_id:0x487b
6,2103,35506597,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Dropping the link to regulator.1
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2104,35521725,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Dropping the link to regulator.51
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2105,35524927,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Dropping the link to regulator.56
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
6,2106,35529275,-;qcom,camera 5c1b000.qcom,cci0:qcom,cam-sensor1: Dropping the link to regulator.55
 SUBSYSTEM=platform
 DEVICE=+platform:5c1b000.qcom,cci0:qcom,cam-sensor1
14,2107,35678477,-;init: processing action (persist.heapprofd.enable= && traced.lazy.heapprofd=) from (/system/etc/init/heapprofd.rc:34)
14,2108,35688782,-;init: processing action (debug.atrace.user_initiated= && persist.traced.enable=1) from (/system/etc/init/perfetto.rc:47)
14,2109,35690466,-;init: starting service 'traced_probes'...
14,2110,35690671,-;init: Opened file '/dev/kmsg', flags 1
6,2111,35691054,-;read descriptors
6,2112,35691210,-;read strings
14,2113,35734526,-;init: processing action (persist.traced.enable=1) from (/system/etc/init/perfetto.rc:50)
14,2114,35737197,-;init: starting service 'traced'...
14,2115,35740430,-;init: Created socket '/dev/socket/traced_consumer', mode 666, user 0, group 0
6,2116,35740591,-;subsys-restart: __subsystem_get(): Changing subsys fw_name to modem
14,2117,35742783,-;init: Created socket '/dev/socket/traced_producer', mode 666, user 0, group 0
6,2118,35744674,-;memshare soc:qcom,memshare: memshare: SUBSYS_BEFORE_POWERUP: enable_ramdump: 0, ramdump_event: 0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
6,2119,35744685,-;memshare soc:qcom,memshare: memshare: notifier_cb processed for code: 2
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
4,2120,35744856,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.mdt
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
14,2121,35769901,-;ueventd: firmware: loading 'modem.mdt' for '/devices/platform/soc/6080000.qcom,mss/firmware/modem.mdt'
14,2122,35778658,-;ueventd: loading /devices/platform/soc/6080000.qcom,mss/firmware/modem.mdt took 9ms
6,2123,35778785,-;subsys-pil-tz 6080000.qcom,mss: modem: loading from 0x000000004ab00000 to 0x0000000051400000
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
6,2124,35779466,-;memshare soc:qcom,memshare: memshare: notifier_cb processed for code: 7
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
4,2125,35793225,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b02
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
14,2126,35832749,-;ueventd: firmware: loading 'modem.b02' for '/devices/platform/soc/6080000.qcom,mss/firmware/modem.b02'
14,2127,35847543,-;ueventd: loading /devices/platform/soc/6080000.qcom,mss/firmware/modem.b02 took 21ms
4,2128,35849774,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b03
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
36,2129,35870500,-;type=1400 audit(1614200570.356:50): avc: denied { read } for comm="Binder:557_2" name="wakeup3" dev="sysfs" ino=36646 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
14,2130,35874028,-;init: Command 'start traced' action=persist.traced.enable=1 (/system/etc/init/perfetto.rc:59) took 138ms and succeeded
14,2131,35874188,-;init: Service 'exec 27 (/system/bin/bootstat --set_system_boot_reason)' (pid 1041) exited with status 0 oneshot service took 0.198000 seconds in background
36,2132,35877344,-;type=1400 audit(1614200570.356:51): avc: denied { read } for comm="Binder:557_2" name="wakeup65" dev="sysfs" ino=64046 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2133,35877485,-;type=1400 audit(1614200570.356:52): avc: denied { read } for comm="Binder:557_2" name="wakeup27" dev="sysfs" ino=47829 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2134,35877578,-;type=1400 audit(1614200570.356:53): avc: denied { read } for comm="Binder:557_2" name="wakeup55" dev="sysfs" ino=60556 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2135,35877664,-;type=1400 audit(1614200570.356:54): avc: denied { read } for comm="Binder:557_2" name="wakeup17" dev="sysfs" ino=37477 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2136,35877751,-;type=1400 audit(1614200570.356:55): avc: denied { read } for comm="Binder:557_2" name="wakeup45" dev="sysfs" ino=60184 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
4,2137,35888126,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b04
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
36,2138,35890295,-;type=1400 audit(1614200570.376:56): avc: denied { read } for comm="Binder:557_2" name="wakeup53" dev="sysfs" ino=60484 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2139,35890782,-;type=1400 audit(1614200570.376:57): avc: denied { read } for comm="Binder:557_2" name="wakeup15" dev="sysfs" ino=37210 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2140,35895661,-;type=1400 audit(1614200570.376:58): avc: denied { read } for comm="Binder:557_2" name="wakeup43" dev="sysfs" ino=60112 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2141,35896360,-;type=1400 audit(1614200570.376:59): avc: denied { read } for comm="Binder:557_2" name="wakeup23" dev="sysfs" ino=43611 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
4,2142,35922627,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b05
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2143,35958499,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b06
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2144,35995062,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b07
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2145,36018019,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b08
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2146,36079022,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b09
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2147,36112595,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b10
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2148,36231796,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b12
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2149,36305253,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b14
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2150,36338949,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b15
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2151,36427056,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b16
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2152,36567084,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b18
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2153,36611264,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b19
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2154,36669629,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b20
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2155,36773083,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b21
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2156,36831121,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b22
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
3,2157,36833761,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2158,36846581,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
4,2159,36881033,-;subsys-pil-tz 6080000.qcom,mss: Falling back to syfs fallback for: modem.b23
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
4,2160,36889197,-;------------[ cut here ]------------
4,2161,36889203,-;Unbalanced enable for IRQ 304
4,2162,36889222,-;WARNING: CPU: 6 PID: 81 at kernel/irq/manage.c:621 enable_irq+0x98/0xf0
6,2163,36889223,-;Modules linked in: wlan(O) tas2563_dlkm(O) machine_dlkm(O) rouleur_slave_dlkm(O) rouleur_dlkm(O) pm2250_spmi_dlkm(O) wcd937x_slave_dlkm(O) wcd937x_dlkm(O) mbhc_dlkm(O) tx_macro_dlkm(O) rx_macro_dlkm(O) va_macro_dlkm(O) bolero_cdc_dlkm(O) wsa881x_analog_dlkm(O) wcd9xxx_dlkm(O) wcd_core_dlkm(O) stub_dlkm(O) swr_ctrl_dlkm(O) swr_dlkm(O) pinctrl_lpi_dlkm(O) usf_dlkm(O) native_dlkm(O) platform_dlkm(O) q6_dlkm(O) adsp_loader_dlkm(O) apr_dlkm(O) snd_event_dlkm(O) q6_notifier_dlkm(O) q6_pdr_dlkm(O)
6,2164,36889254,-;CPU: 6 PID: 81 Comm: kworker/6:1 Tainted: G        W  O      4.19.152+ #1
6,2165,36889256,-;Hardware name: Qualcomm Technologies, Inc. Honeywell CT45 (DT)
6,2166,36889264,-;Workqueue: pm pm_runtime_work
6,2167,36889267,-;pstate: 60400085 (nZCv daIf +PAN -UAO)
6,2168,36889271,-;pc : enable_irq+0x98/0xf0
6,2169,36889273,-;lr : enable_irq+0x98/0xf0
6,2170,36889275,-;sp : ffffff800d7e3b90
6,2171,36889276,-;x29: ffffff800d7e3ba0 x28: 0000000000000002 
6,2172,36889279,-;x27: 0000000000000000 x26: ffffffc0a386f535 
6,2173,36889282,-;x25: 0000000000000000 x24: 0000000000000064 
6,2174,36889285,-;x23: 00000000000001f4 x22: 0000000000000014 
6,2175,36889287,-;x21: ffffffc09e138a90 x20: 0000000000000130 
6,2176,36889289,-;x19: ffffffc09512cc80 x18: 0000000000000030 
6,2177,36889291,-;x17: ffffff800a846000 x16: 00000000fffc8ac8 
6,2178,36889294,-;x15: 00000000000c8ac8 x14: 0000000000000086 
6,2179,36889296,-;x13: 0000000000000030 x12: 0000000000000004 
6,2180,36889299,-;x11: 0000000000000001 x10: 0000000000000007 
6,2181,36889301,-;x9 : 7094533e5961e000 x8 : 7094533e5961e000 
6,2182,36889303,-;x7 : 0000000000000000 x6 : ffffffc0fb26f565 
6,2183,36889306,-;x5 : 0000000000000000 x4 : 000000000000000e 
6,2184,36889308,-;x3 : 0000000000000034 x2 : fffffffffffff78f 
6,2185,36889310,-;x1 : ffffff8009e71eda x0 : 000000000000001d 
6,2186,36889313,-;Call trace:
6,2187,36889317,-; enable_irq+0x98/0xf0
6,2188,36889328,-; swrm_runtime_suspend+0x46c/0x5f8 [swr_ctrl_dlkm]
6,2189,36889330,-; pm_generic_runtime_suspend+0x34/0x48
6,2190,36889333,-; __rpm_callback+0x164/0x270
6,2191,36889335,-; rpm_suspend+0x468/0x828
6,2192,36889337,-; pm_runtime_work+0x94/0xa8
6,2193,36889342,-; process_one_work+0x27c/0x470
6,2194,36889345,-; worker_thread+0x23c/0x4c8
6,2195,36889347,-; kthread+0x14c/0x160
6,2196,36889351,-; ret_from_fork+0x10/0x1c
4,2197,36889353,-;---[ end trace e3272503f35f0d76 ]---
6,2198,36978558,-;memshare soc:qcom,memshare: memshare: notifier_cb processed for code: 4
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
6,2199,37131966,-;subsys-pil-tz 6080000.qcom,mss: modem: Brought out of reset
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
6,2200,37149783,-;subsys-pil-tz 6080000.qcom,mss: Subsystem error monitoring/handling services are up
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
6,2201,37152893,-;subsys-pil-tz 6080000.qcom,mss: modem: Power/Clock ready interrupt received
 SUBSYSTEM=platform
 DEVICE=+platform:6080000.qcom,mss
6,2202,37153739,-;memshare soc:qcom,memshare: memshare: notifier_cb processed for code: 8
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
3,2203,37168644,-;166200771:Entered
4,2204,37173004,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
6,2205,37174373,-;memshare soc:qcom,memshare: memshare: SUBSYS_AFTER_POWERUP: Modem has booted up
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
6,2206,37174394,-;memshare soc:qcom,memshare: memshare: notifier_cb processed for code: 3
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare
6,2207,37174441,-;adsprpc: fastrpc_restart_notifier_cb: modem subsystem is up
3,2208,37182541,-;166200771:SMD QRTR driver probed
14,2209,37193246,-;rmt_storage:INFO:rmt_storage_open_cb: Processing: Open Request (req_h 0x1) for /boot/modem_fs1!
6,2210,37194937,-;service-notifier: service_notifier_new_server: Connection established between QMI handle and 180 service
14,2211,37195245,-;rmt_storage:INFO:rmt_storage_open_cb: Processing: Open Request (req_h 0x2) for /boot/modem_fs2!
6,2212,37197585,-;sysmon-qmi: ssctl_new_server: Connection established between QMI handle and modem's SSCTL service
6,2213,37199737,-;read descriptors
6,2214,37199900,-;read strings
14,2215,37201453,-;rmt_storage:INFO:rmt_storage_alloc_buff_cb: Received req_size: 1572864! avail: 2097152
14,2216,37205592,-;rmt_storage:INFO:rmt_storage_rw_iovec_cb: Read iovec request (req_h 0x4 wr_count 0) received for /boot/modem_fs1
4,2217,37221909,-;irq: type mismatch, failed to map hwirq-80 for pinctrl@400000!
14,2218,37235272,-;rmt_storage:INFO:rmt_storage_client_thread: Calling Read [offset=512, size=512, req_h 0x4, wr_count 0] for /boot/modem_fs1!
14,2219,37238111,-;rmt_storage:INFO:rmt_storage_client_thread: Done Read (bytes = 512, req_h 0x4, wr_count 0) for /boot/modem_fs1!
14,2220,37239551,-;rmt_storage:INFO:rmt_storage_rw_iovec_cb: Read iovec request (req_h 0x5 wr_count 0) received for /boot/modem_fs2
14,2221,37241332,-;rmt_storage:INFO:rmt_storage_client_thread: Calling Read [offset=512, size=512, req_h 0x5, wr_count 0] for /boot/modem_fs2!
6,2222,37306861,-;coresight-remote-etm soc:modem_etm0: Connection established between QMI handle and 2 service
 SUBSYSTEM=platform
 DEVICE=+platform:soc:modem_etm0
6,2223,37320657,-;memshare_child soc:qcom,memshare:qcom,client_3: memshare_query: client_id : 1, query_resp.size :5242880, query_resp.resp.result :0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare:qcom,client_3
6,2224,37321382,-;memshare_child soc:qcom,memshare:qcom,client_3: memshare_alloc: memory alloc request received for client id: 1, proc_id: 0, request size: 5242880
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare:qcom,client_3
6,2225,37408768,-;alloc_contig_range: [fe200, fe700) PFNs busy
6,2226,37468223,-;memshare_child soc:qcom,memshare:qcom,client_3: memshare_alloc: client_id: 1, alloc_resp.num_bytes: 5242880, alloc_resp.resp.result: 0
 SUBSYSTEM=platform
 DEVICE=+platform:soc:qcom,memshare:qcom,client_3
3,2227,37470083,-;diag: In diag_send_peripheral_buffering_mode, buffering flag not set for 0
6,2228,38009593,-;service-notifier: root_service_service_ind_cb: Indication received from msm/modem/wlan_pd, state: 0x1fffffff, trans-id: 1
6,2229,38010237,-;service-notifier: send_ind_ack: Indication ACKed for transid 1, service msm/modem/wlan_pd, instance 180!
6,2230,38024800,-;icnss_qmi: QMI Server Connected: state: 0x980
3,2231,38026850,-;icnss: hyperviser disabled
3,2232,38026861,-;icnss: hyperviser disabled
3,2233,38032383,-;icnss_qmi: Invalid Hang Data details, Offset:0x0, Length:0x0
3,2234,38278913,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2235,38308118,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2236,38315806,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2237,38322188,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2238,38327883,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2239,38334894,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2240,38348176,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2241,38354327,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,2242,38386956,-;cnss-daemon Failed to init genl between daemon and platform, continue
3,2243,38388760,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2244,38394455,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2245,38434629,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2246,38443480,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2247,38478312,-;diag: In diag_ioctl_set_buffering_mode, peripheral 3 doesn't support buffering
3,2248,38495295,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2249,38502801,-;android_work: did not send uevent (0 0 0000000000000000)
3,2250,38518283,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2251,38526862,-;healthd: battery l=51 v=3705 t=30.8 h=2 st=2 c=-959473 fc=3812000 cc=0 chg=a
3,2252,38533941,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2253,38548147,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2254,38553353,-;msm_qti_pp_get_rms_value_control, back not active to query rms be_idx:3
6,2255,38562633,-;read descriptors
6,2256,38562787,-;read strings
3,2257,38565393,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2258,38571889,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,2259,38596346,-;cnss-daemon wlfw_start: Starting
6,2260,38702656,-;android_work: did not send uevent (0 0 0000000000000000)
6,2261,38737216,-;core_get_license_status: cmdrsp_license_result.result = 0x15 for module 0x131ff
6,2262,38750717,-;tas2563 0-004c: tas2563_digital_left_tlv_get = 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2263,38751773,-;tas2563 0-004c: tas2563_digital_right_tlv_get = 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2264,38752856,-;tas2563 0-004c: tas2563_program_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2265,38753923,-;tas2563 0-004c: tas2563_program_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2266,38755081,-;tas2563 0-004c: tas2563_program_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2267,38756227,-;tas2563 0-004c: tas2563_configuration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2268,38757303,-;tas2563 0-004c: tas2563_configuration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2269,38758710,-;tas2563 0-004c: tas2563_configuration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2270,38760042,-;tas2563 0-004c: tas2563_calibration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2271,38762169,-;tas2563 0-004c: tas2563_calibration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2272,38763652,-;tas2563 0-004c: tas2563_calibration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2273,38772653,-;tas2563 0-004c: tas2563_get_left_speaker_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2274,38774493,-;tas2563 0-004c: tas2563_get_right_speaker_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2275,38776841,-;tas2563 0-004c: tas2563_get_left_channel_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2276,38779482,-;tas2563 0-004c: tas2563_get_right_channel_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2277,38781170,-;tas2563 0-004c: tas2563_left_180_shift_get, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2278,38782915,-;tas2563 0-004c: tas2563_right_180_shift_get, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,2279,38825440,-;cnss-daemon wlfw_service_request: Start the pthread: 0x0K
6,2280,38852277,-;coresight-tmc 8048000.tmc: TMC-ETR enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8048000.tmc
6,2281,38852395,-;coresight-dynamic-funnel 8045000.funnel: FUNNEL inport 0 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8045000.funnel
6,2282,38852430,-;coresight-dynamic-funnel 8041000.funnel: FUNNEL inport 7 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8041000.funnel
6,2283,38852725,-;coresight-stm 8002000.stm: STM tracing enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8002000.stm
14,2284,38855700,-;cnss-daemon Hardware does not support external modem
6,2285,38865583,-;android_work: did not send uevent (0 0 0000000000000000)
6,2286,38906181,-;capability: warning: `msm_irqbalance' uses 32-bit capabilities (legacy support in use)
14,2287,38949599,-;cnss-daemon Target does not have external modem
14,2288,38952272,-;cnss-daemon wlfw_send_bdf_download_req: BDF file : regdb.bin
14,2289,38996933,-;cnss-daemon wlfw_send_bdf_download_req: Failed to find BDF file regdb.bin
3,2290,39088316,-;msm_pcm_volume_ctl_get substream not found
14,2291,39101597,-;cnss-daemon Failed to Download the REGDB File
6,2292,39124583,-;coresight-tmc 8048000.tmc: TMC-ETR enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8048000.tmc
6,2293,39124620,-;coresight-dynamic-funnel 8045000.funnel: FUNNEL inport 1 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8045000.funnel
6,2294,39124649,-;coresight-dynamic-funnel 8042000.funnel: FUNNEL inport 6 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8042000.funnel
6,2295,39124695,-;coresight-dynamic-funnel 9810000.funnel: FUNNEL inport 4 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:9810000.funnel
6,2296,39124761,-;coresight-tpda 9862000.tpda: TPDA inport 0 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:9862000.tpda
6,2297,39125358,-;coresight-tpdm 9860000.tpdm: TPDM tracing enabled
 SUBSYSTEM=amba
 DEVICE=+amba:9860000.tpdm
6,2298,39152068,-;android_work: sent uevent USB_STATE=CONNECTED
6,2299,39199442,-;coresight-tmc 8048000.tmc: TMC-ETR enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8048000.tmc
6,2300,39199489,-;coresight-dynamic-funnel 8041000.funnel: FUNNEL inport 6 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8041000.funnel
6,2301,39199516,-;coresight-dynamic-funnel 8005000.funnel: FUNNEL inport 0 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8005000.funnel
6,2302,39199552,-;coresight-tpda 8004000.tpda: TPDA inport 0 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8004000.tpda
6,2303,39200152,-;coresight-tpdm 8b58000.tpdm: TPDM tracing enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8b58000.tpdm
14,2304,39203157,-;cnss-daemon wlfw_send_bdf_download_req: BDF file : bdwlan.bin
6,2305,39262016,-;read descriptors
6,2306,39262331,-;read strings
3,2307,39298004,-;msm-dcc 1be2000.dcc_v2: DCC is not ready Disabling DCC...
 SUBSYSTEM=platform
 DEVICE=+platform:1be2000.dcc_v2
6,2308,39383686,-;android_work: sent uevent USB_STATE=DISCONNECTED
6,2309,39526874,-;msm_vidc:   high: 00000001: ....e: Opening video instance: ffffffc086058000, 0
6,2310,39529555,-;msm_vidc_v4l2 5a00000.qcom,vidc: Linked as a consumer to regulator.5
 SUBSYSTEM=platform
 DEVICE=+platform:5a00000.qcom,vidc
6,2311,39530048,-;msm_vidc_v4l2 5a00000.qcom,vidc: Linked as a consumer to regulator.4
 SUBSYSTEM=platform
 DEVICE=+platform:5a00000.qcom,vidc
6,2312,39537064,-;subsys-restart: __subsystem_get(): Changing subsys fw_name to venus
4,2313,39541829,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.mdt
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
14,2314,39572216,-;ueventd: firmware: loading 'venus.mdt' for '/devices/platform/soc/5ab0000.qcom,venus/firmware/venus.mdt'
6,2315,39578405,-;subsys-pil-tz 5ab0000.qcom,venus: venus: loading from 0x0000000051400000 to 0x0000000051900000
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
14,2316,39579488,-;ueventd: loading /devices/platform/soc/5ab0000.qcom,venus/firmware/venus.mdt took 7ms
6,2317,39580094,-;coresight-tmc 8048000.tmc: TMC-ETR enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8048000.tmc
6,2318,39580155,-;coresight-tpda 8004000.tpda: TPDA inport 8 enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8004000.tpda
6,2319,39581292,-;coresight-tpdm 8870000.tpdm: TPDM tracing enabled
 SUBSYSTEM=amba
 DEVICE=+amba:8870000.tpdm
6,2320,39582203,-;android_work: did not send uevent (0 0 0000000000000000)
4,2321,39593036,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b02
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2322,39593219,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b03
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2323,39593254,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b04
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2324,39594887,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b05
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2325,39594962,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b06
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2326,39596076,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b07
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2327,39597586,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b08
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2328,39597615,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b09
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2329,39598992,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b10
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
4,2330,39600431,-;subsys-pil-tz 5ab0000.qcom,venus: Falling back to syfs fallback for: venus.b19
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
14,2331,39607536,-;ueventd: firmware: loading 'venus.b02' for '/devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b02'
14,2332,39616703,-;ueventd: loading /devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b02 took 9ms
14,2333,39624013,-;ueventd: firmware: loading 'venus.b04' for '/devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b04'
14,2334,39630371,-;ueventd: loading /devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b04 took 7ms
14,2335,39642064,-;ueventd: firmware: loading 'venus.b03' for '/devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b03'
14,2336,39648526,-;ueventd: loading /devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b03 took 7ms
11,2337,39650195,-;MAIN_MGR: hvdcp_opti Version: 3:0:0
14,2338,39662126,-;ueventd: firmware: loading 'venus.b05' for '/devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b05'
6,2339,39671211,-;android_work: sent uevent USB_STATE=CONNECTED
14,2340,39672200,-;ueventd: loading /devices/platform/soc/5ab0000.qcom,venus/firmware/venus.b05 took 10ms
11,2341,39690638,-;MAIN_MGR: set keepcaps failed!
11,2342,39691096,-;CHG_POLICY_PATH: Using power-supply path for chg-policy
11,2343,39719565,-;THERM-BALANCE: Parallel PSY entry not found.
6,2344,39732569,-;configfs-gadget gadget: high-speed config #1: b
11,2345,39732571,-;HVDCP2: HVDCP THERMAL_INOV disabled
11,2346,39732848,-;STD-PD: Registered STD_PD
11,2347,39738330,-;CTM: CTM disabled, exiting
11,2348,39739532,-;hvdcpd: HVDCP Thermal INOV disabled
6,2349,39741855,-;android_work: sent uevent USB_STATE=CONFIGURED
11,2350,39742353,-;PPS: Registered PPS
11,2351,39745142,-;CP: charge_pump missing
6,2352,39752994,-;ueventd (1469) used greatest stack depth: 10656 bytes left
3,2353,39774725,-;msm-dcc 1be2000.dcc_v2: DCC list passed 2
 SUBSYSTEM=platform
 DEVICE=+platform:1be2000.dcc_v2
6,2354,39780963,-;msm-dcc 1be2000.dcc_v2: All values written to enable.
 SUBSYSTEM=platform
 DEVICE=+platform:1be2000.dcc_v2
3,2355,39781181,-;msm-dcc 1be2000.dcc_v2: DCC list passed 3
 SUBSYSTEM=platform
 DEVICE=+platform:1be2000.dcc_v2
6,2356,39789912,-;msm-dcc 1be2000.dcc_v2: All values written to enable.
 SUBSYSTEM=platform
 DEVICE=+platform:1be2000.dcc_v2
3,2357,39796669,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2358,39802751,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2359,39825194,-;subsys-pil-tz 5ab0000.qcom,venus: venus: Brought out of reset
 SUBSYSTEM=platform
 DEVICE=+platform:5ab0000.qcom,venus
3,2360,39830026,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2361,39835729,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2362,39853687,-;msm_vidc:   err : 00000001: ....e: msm_vidc_comm_update_ctrl: failed: control name Video B Frames, min 0, max 0, step 0, default_value 0
6,2363,39878923,-;msm_vidc:   high: 00000001: h265e: Closed video instance: ffffffc086058000
6,2364,39930808,-;msm_vidc:   high: 00000001: ....d: Opening video instance: ffffffc08a2d8000, 1
6,2365,39947271,-;msm_vidc:   high: 00000001: h264d: Closed video instance: ffffffc08a2d8000
6,2366,39982981,-;msm_vidc:   high: 00000001: ....d: Opening video instance: ffffffc085b70000, 1
6,2367,39999563,-;msm_vidc:   high: 00000001: h264d: Closed video instance: ffffffc085b70000
3,2368,40070228,-;msm_qti_pp_get_rms_value_control, back not active to query rms be_idx:3
6,2369,40088513,-;msm_vidc:   high: 00000001: ....d: Opening video instance: ffffffc0822b4000, 1
6,2370,40102612,-;msm_vidc:   high: 00000001: h265d: Closed video instance: ffffffc0822b4000
6,2371,40127040,-;msm_vidc:   high: 00000001: ....d: Opening video instance: ffffffc0871f0000, 1
6,2372,40144548,-;msm_vidc:   high: 00000001: h265d: Closed video instance: ffffffc0871f0000
6,2373,40158391,-;core_get_license_status: cmdrsp_license_result.result = 0x15 for module 0x131ff
6,2374,40163565,-;tas2563 0-004c: tas2563_digital_left_tlv_get = 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2375,40164420,-;tas2563 0-004c: tas2563_digital_right_tlv_get = 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2376,40165283,-;tas2563 0-004c: tas2563_program_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2377,40166166,-;tas2563 0-004c: tas2563_program_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2378,40167098,-;tas2563 0-004c: tas2563_program_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2379,40167998,-;tas2563 0-004c: tas2563_configuration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2380,40169116,-;tas2563 0-004c: tas2563_configuration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2381,40170024,-;tas2563 0-004c: tas2563_configuration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2382,40170946,-;tas2563 0-004c: tas2563_calibration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2383,40171868,-;tas2563 0-004c: tas2563_calibration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2384,40172820,-;tas2563 0-004c: tas2563_calibration_get = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2385,40177231,-;tas2563 0-004c: tas2563_get_left_speaker_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2386,40178851,-;tas2563 0-004c: tas2563_get_right_speaker_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2387,40180550,-;tas2563 0-004c: tas2563_get_left_channel_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2388,40182404,-;tas2563 0-004c: tas2563_get_right_channel_switch, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2389,40184028,-;tas2563 0-004c: tas2563_left_180_shift_get, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2390,40185505,-;tas2563 0-004c: tas2563_right_180_shift_get, p_u_control = 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2391,40266617,-;msm_vidc:   high: 00000001: ....d: Opening video instance: ffffffc087178000, 1
6,2392,40284636,-;msm_vidc:   high: 00000001:  vp9d: Closed video instance: ffffffc087178000
6,2393,40304069,-;msm_vidc:   high: 00000001: ....d: Opening video instance: ffffffc087178000, 1
6,2394,40320469,-;msm_vidc:   high: 00000001:  vp9d: Closed video instance: ffffffc087178000
6,2395,40364404,-;msm_vidc:   high: 00000001: ....e: Opening video instance: ffffffc087178000, 0
6,2396,40366210,-;msm_vidc:   err : 00000001: ....e: msm_vidc_comm_update_ctrl: failed: control name Video B Frames, min 0, max 0, step 0, default_value 0
6,2397,40380819,-;msm_vidc:   high: 00000001: h264e: Closed video instance: ffffffc087178000
3,2398,40470423,-;msm_pcm_volume_ctl_get substream not found
6,2399,40483242,-;msm_vidc:   high: 00000001: ....e: Opening video instance: ffffffc087330000, 0
6,2400,40485071,-;msm_vidc:   err : 00000001: ....e: msm_vidc_comm_update_ctrl: failed: control name Video B Frames, min 0, max 0, step 0, default_value 0
6,2401,40496819,-;msm_vidc:   high: 00000001: h265e: Closed video instance: ffffffc087330000
6,2402,40526004,-;msm_vidc:   high: 00000001: ....e: Opening video instance: ffffffc08715c000, 0
6,2403,40527795,-;msm_vidc:   err : 00000001: ....e: msm_vidc_comm_update_ctrl: failed: control name Video B Frames, min 0, max 0, step 0, default_value 0
6,2404,40542741,-;msm_vidc:   high: 00000001: h265e: Closed video instance: ffffffc08715c000
14,2405,40957619,-;init: Control message: Processed ctl.start for 'idmap2d' from pid: 957 (system_server)
3,2406,40986831,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2407,40993653,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2408,41008615,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2409,41014411,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2410,41265998,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2411,41271751,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2412,41292316,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2413,41298256,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2414,41310349,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2415,41316052,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2416,41329481,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2417,41338252,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2418,41346607,-;healthd: battery l=51 v=3710 t=30.8 h=2 st=2 c=-839234 fc=3812000 cc=0 chg=a
3,2419,41347922,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2420,41353852,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2421,41365073,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2422,41371130,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
36,2423,41371599,-;type=1400 audit(1614200575.856:68): avc: denied { read } for comm="Binder:557_2" name="wakeup48" dev="sysfs" ino=60292 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2424,41377434,-;type=1400 audit(1614200575.856:69): avc: denied { read } for comm="Binder:557_2" name="wakeup4" dev="sysfs" ino=36664 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2425,41387508,-;type=1400 audit(1614200575.866:70): avc: denied { read } for comm="Binder:557_2" name="wakeup28" dev="sysfs" ino=48113 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2426,41395885,-;type=1400 audit(1614200575.876:71): avc: denied { read } for comm="Binder:557_2" name="wakeup18" dev="sysfs" ino=37631 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2427,41396602,-;type=1400 audit(1614200575.876:72): avc: denied { read } for comm="Binder:557_2" name="wakeup46" dev="sysfs" ino=60220 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2428,41397258,-;type=1400 audit(1614200575.876:73): avc: denied { read } for comm="Binder:557_2" name="wakeup2" dev="sysfs" ino=36628 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2429,41407493,-;type=1400 audit(1614200575.886:74): avc: denied { read } for comm="Binder:557_2" name="wakeup64" dev="sysfs" ino=63936 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2430,41412103,-;type=1400 audit(1614200575.896:75): avc: denied { read } for comm="Binder:557_2" name="wakeup26" dev="sysfs" ino=47722 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2431,41414423,-;type=1400 audit(1614200575.896:76): avc: denied { read } for comm="Binder:557_2" name="wakeup54" dev="sysfs" ino=60520 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2432,41418152,-;type=1400 audit(1614200575.896:77): avc: denied { read } for comm="Binder:557_2" name="wakeup44" dev="sysfs" ino=60148 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
11,2433,41421003,-;init: Control message: Could not find 'android.frameworks.sensorservice@1.0::ISensorManager/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2434,41438522,-;init: Control message: Could not find 'android.frameworks.sensorservice@1.0::ISensorManager/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2435,41453939,-;max1720x 0-0036: case 5 === SN=TWMX2049505588
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,2436,41456367,-;init: Control message: Could not find 'android.frameworks.sensorservice@1.0::ISensorManager/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2437,41467919,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,2438,41474143,-;init: Control message: Could not find 'android.frameworks.sensorservice@1.0::ISensorManager/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2439,41479311,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2440,41532865,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2441,41538650,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2442,41577518,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2443,41591717,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2444,41609729,-;healthd: battery l=51 v=3721 t=31.1 h=2 st=2 c=-879212 fc=3812000 cc=0 chg=a
3,2445,41612269,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2446,41617969,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2447,41636282,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2448,41645071,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2449,41834679,-;wcdcal_hwdep_ioctl_shared: codec didn't set this 0!!
3,2450,41842772,-;wcdcal_hwdep_ioctl_shared: codec didn't set this 3!!
6,2451,41854960,-;icnss: WLAN FW is ready: 0xd87
4,2452,41861635,-;(NULL device *): Falling back to syfs fallback for: wlan/qca_cld/WCNSS_qcom_cfg.ini
3,2453,41948314,-;ipa_uc_reg_rdyCB:2154 IPA HW is not supported
4,2454,41957059,-;[kworke][0x444ca34d][21:02:56.450490] wlan: [241:W:HIF] hif_snoc_enable_bus: device_init_wakeup already done
6,2455,41957084,-;[kworke][0x444ca5e9][21:02:56.450525] wlan: [241:I:HIF] Up_linkstate_vote 1
3,2456,41957117,-;[kworke][0x444ca85d][21:02:56.450557] wlan: [241:E:TXRX] hif_print_hal_shadow_register_cfg: CONFIG_SHADOW_V2 not defined
14,2457,41991444,-;init: processing action (sys.sysctl.extra_free_kbytes=*) from (/system/etc/init/hw/init.rc:1025)
3,2458,42076282,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2459,42083827,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2460,42094707,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2461,42100575,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2462,42116260,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2463,42122229,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2464,42226914,-;[kworke][0x449bb284][21:02:56.720346] wlan: [241:I:HIF] hif_snoc_bus_configure: 187: expecting wake from ce 2, irq 36
3,2465,42227084,-;[kworke][0x449bbfbf][21:02:56.720522] wlan: [241:E:IPA] ipa_component_config_update: 639: g_ipa_config is NULL
3,2466,42238417,-;[kworke][0x449f11ab][21:02:56.731855] wlan: [241:E:WMI] WMI handle is NULL
3,2467,42246982,-;[kworke][0x44a19440][21:02:56.740422] wlan: [241:E:QDF] cds_get_context: 1365: Module ID 66 context is Null
3,2468,42324775,-;[kworke][0x44b85e6b][21:02:56.818211] wlan: [241:E:QDF] cds_get_context: 1365: Module ID 66 context is Null
1,2469,42355838,-;[kworke][0x44c17810][21:02:56.849274] wlan: [241:F:WMA] WMA --> wmi_unified_attach - success
3,2470,42499221,-;[kworke][0x44eb79ea][21:02:56.992658] wlan: [241:E:QDF] htc_wait_target: 625: Target Ready! TX resource : 2 size:2184, MaxMsgsPerHTCBundle = 1
3,2471,42513155,-;[kworke][0x44ef8f27][21:02:57.006595] wlan: [241:E:QDF] htc_setup_target_buffer_assignments: 517: SVS Index : 1 TX : 0x100 : alloc:2
6,2472,42536068,-;[kworke][0x44f645be][21:02:57.029509] wlan: [82:I:WMA] wma_rx_service_ready_event: Firmware build version : 337e81a6
6,2473,42536087,-;[kworke][0x44f6476d][21:02:57.029531] wlan: [82:I:WMA] wma_rx_service_ready_event: Board id: 0, Board version: 1a 0 0 0 6
6,2474,42536100,-;[kworke][0x44f64874][21:02:57.029545] wlan: [82:I:TXRX] ol_tx_set_desc_global_pool_size: 125: Global pool size: 3600\x0a
3,2475,42536472,-;[kworke][0x44f66425][21:02:57.029914] wlan: [82:E:WMA] wma_update_supported_bands: wrong supported band
3,2476,42550413,-;[kworke][0x44fa792e][21:02:57.043848] wlan: [82:E:QDF] copy_fw_abi_version_tlv: 6747: copy_fw_abi_version_tlv: INIT_CMD version: 1, 0, 0x5f414351, 0x4c4d, 0x0, 0x0
3,2477,42582686,-;[kworke][0x4503edb2][21:02:57.076122] wlan: [82:E:QDF] ready_extract_init_status_tlv: 8517: ready_extract_init_status_tlv:0
6,2478,42601824,-;[kworke][0x45098960][21:02:57.095264] wlan: [82:I:dfs] WLAN_DEBUG_DFS_ALWAYS : wlan_dfs_pdev_obj_create_notification: 389: dfs_offload 0
14,2479,42607374,-;init: starting service 'qspmhal'...
3,2480,42609442,-;[kworke][0x450bc4a7][21:02:57.102881] wlan: [82:E:dfs] WLAN_DEBUG_DFS_ALWAYS : dfs_init_radar_filters: 252: Unknown dfs domain 0
6,2481,42622547,-;[kworke][0x450f9bba][21:02:57.115989] wlan: [82:I:SPECTRAL] null_get_capability: 1553: SPECTRAL : get_capability not registered\x0a
6,2482,42622561,-;[kworke][0x450f9cf8][21:02:57.116005] wlan: [82:I:SPECTRAL] target_if_pdev_spectral_init: 1978: HAL_CAP_PHYDIAG : Capable
6,2483,42622573,-;[kworke][0x450f9ddb][21:02:57.116017] wlan: [82:I:SPECTRAL] null_get_capability: 1553: SPECTRAL : get_capability not registered\x0a
6,2484,42622583,-;[kworke][0x450f9eb0][21:02:57.116028] wlan: [82:I:SPECTRAL] target_if_pdev_spectral_init: 1982: HAL_CAP_RADAR   : Capable
6,2485,42622595,-;[kworke][0x450f9f82][21:02:57.116039] wlan: [82:I:SPECTRAL] null_get_capability: 1553: SPECTRAL : get_capability not registered\x0a
6,2486,42623219,-;[kworke][0x450fa059][21:02:57.116050] wlan: [82:I:SPECTRAL] target_if_pdev_spectral_init: 1987: HAL_CAP_SPECTRAL_SCAN : Capable
6,2487,42623241,-;[kworke][0x450fcfdb][21:02:57.116684] wlan: [82:I:SPECTRAL] null_get_tsf64: 1541: SPECTRAL : get_tsf64 not registered\x0a
6,2488,42623280,-;[kworke][0x450fd2de][21:02:57.116724] wlan: [82:I:GREEN_AP] wlan_green_ap_pdev_obj_create_notification: 106: Green AP creation successful, green ap ctx: ffffffc0880c1ce8, pdev: ffffffc07b3feee8
6,2489,42623350,-;[kworke][0x450fd821][21:02:57.116794] wlan: [82:I:OBJMGR] wlan_objmgr_pdev_obj_create: 175: Created pdev 0
6,2490,42625325,-;[kworke][0x45106c05][21:02:57.118766] wlan: [82:I:REGULATORY] reg_set_band: 392: same band 0
6,2491,42625339,-;[kworke][0x45106d62][21:02:57.118784] wlan: [82:I:HDD] hdd_update_tgt_cfg: 2128: hw_mac is zero
6,2492,42625606,-;[kworke][0x45108155][21:02:57.119050] wlan: [82:I:GREEN_AP] target_if_green_ap_register_egap_event_handler: 131: Set the Enhance Green AP event handler
6,2493,42625749,-;[kworke][0x45108c02][21:02:57.119192] wlan: [82:I:QDF] host_diag_log_submit: Unloading/Loading in Progress. Ignore!!!
6,2494,42626643,-;[kworke][0x4510cecc][21:02:57.120083] wlan: [241:I:WMA] wma_wait_for_ready_event: 7310: FW ready event received
6,2495,42652299,-;[kworke][0x451852bf][21:02:57.145736] wlan: [241:I:HTT] max pool size 64 pool filled 64
3,2496,42879768,-;[kworke][0x455af744][21:02:57.373209] wlan: [241:E:WMI] send_action_oui_cmd_tlv: 220: Invalid action id
3,2497,42891430,-;[kworke][0x455e61ea][21:02:57.384871] wlan: [241:E:action_oui] ucfg_action_oui_send: 160: Failed to send: 7
3,2498,42914310,-;cnss_utils: WLAN MAC address is not set, type 0
4,2499,42920296,-;icnss c800000.qcom,icnss: Falling back to syfs fallback for: wlan/qca_cld/wlan_mac.bin
 SUBSYSTEM=platform
 DEVICE=+platform:c800000.qcom,icnss
6,2500,42939812,-;[kworke][0x456c8e74][21:02:57.433252] wlan: [241:I:HDD] hdd_initialize_mac_address: 11585: using default MAC address
14,2501,42946229,-;init: Service 'qspmhal' (pid 1676) received signal 6
14,2502,42946279,-;init: Sending signal 9 to service 'qspmhal' (pid 1676) process group...
14,2503,42969474,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 1676 in 22ms
6,2504,43404331,-;acc_open
6,2505,43404365,-;acc_release
6,2506,43727092,-;Wifi Turning On from UI
6,2507,43744974,-;[wifi@1][0x46586f4d][21:02:58.238383] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_create: 211: VDEV SM lock is disabled!!!
6,2508,43744990,-;[wifi@1][0x4658731b][21:02:58.238434] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_create: 231: VDEV CMD lock is disabled!!!
6,2509,43745207,-;[wifi@1][0x46588373][21:02:58.238652] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_create: 269: Created vdev 0
6,2510,43754135,-;IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
3,2511,45928890,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2512,45934792,-;PM8008: pm8008_read: failed to read 0x0950
3,2513,45940398,-;PM8008: pm8008_enable_regulator_is_enabled: qcom,pm8008-chip-en: failed to get chip state rc=-107
6,2514,45950428,-;pm8008-chip-en: disabling
11,2515,46149251,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2516,46172623,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2517,46219468,-;bt_ioctl: BT_CMD_PWR_CTRL pwr_cntrl:0
3,2518,46224326,-;bt_ioctl: BT state already:0 no change done\x0a
3,2519,46231934,-;bt_ioctl: BT_CMD_PWR_CTRL pwr_cntrl:1
6,2520,46237671,-;bt_power soc:bt_wcn3990: Linked as a consumer to regulator.30
 SUBSYSTEM=platform
 DEVICE=+platform:soc:bt_wcn3990
3,2521,46237711,-;bt_vreg_enable: vreg_en successful for : qca,bt-vdd-io
6,2522,46244872,-;bt_power soc:bt_wcn3990: Linked as a consumer to regulator.37
 SUBSYSTEM=platform
 DEVICE=+platform:soc:bt_wcn3990
3,2523,46244909,-;bt_vreg_enable: vreg_en successful for : qca,bt-vdd-xtal
6,2524,46252609,-;bt_power soc:bt_wcn3990: Linked as a consumer to regulator.38
 SUBSYSTEM=platform
 DEVICE=+platform:soc:bt_wcn3990
3,2525,46252645,-;bt_vreg_enable: vreg_en successful for : qca,bt-vdd-core
6,2526,46260406,-;bt_power soc:bt_wcn3990: Linked as a consumer to regulator.44
 SUBSYSTEM=platform
 DEVICE=+platform:soc:bt_wcn3990
3,2527,46260445,-;bt_vreg_enable: vreg_en successful for : qca,bt-vdd-pa
6,2528,46263389,-;[wifi@1][0x493a4026][21:03:00.756795] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_delete: 341: Logically deleting vdev 0
6,2529,46266871,-;[wifi@1][0x493b47b2][21:03:00.760308] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_destroy: 237: VDEV CMD lock is disabled!!!
6,2530,46266892,-;[wifi@1][0x493b4984][21:03:00.760333] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_destroy: 217: VDEV SM lock is disabled!!!
6,2531,46277709,-;[wifi@1][0x493e5233][21:03:00.770688] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_create: 211: VDEV SM lock is disabled!!!
6,2532,46277738,-;[wifi@1][0x493e76c5][21:03:00.771176] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_create: 231: VDEV CMD lock is disabled!!!
6,2533,46278249,-;[wifi@1][0x493e9d14][21:03:00.771687] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_create: 269: Created vdev 0
11,2534,46405908,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2535,46426187,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2536,46443916,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2537,46451452,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2538,46469575,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2539,46475262,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2540,46484344,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2541,46490209,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2542,46496938,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2543,46502834,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2544,46509562,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2545,46515234,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2546,46519973,-;bt_ioctl: BT_CMD_CHECK_SW_CTRL
6,2547,46521696,-;bt_ioctl: bt-sw-ctrl-gpio(1254) value(1)
36,2548,46523134,-;type=1400 audit(1614200581.006:179): avc: denied { read } for comm="Binder:557_2" name="wakeup48" dev="sysfs" ino=60292 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2549,46525566,-;type=1400 audit(1614200581.006:180): avc: denied { read } for comm="Binder:557_2" name="wakeup4" dev="sysfs" ino=36664 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
3,2550,46531514,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
36,2551,46535266,-;type=1400 audit(1614200581.016:181): avc: denied { read } for comm="Binder:557_2" name="wakeup28" dev="sysfs" ino=48113 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
3,2552,46535619,-;bt_ioctl: unified Current SOC Version : 40020150
3,2553,46537447,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
36,2554,46546473,-;type=1400 audit(1614200581.026:182): avc: denied { read } for comm="Binder:557_2" name="wakeup18" dev="sysfs" ino=37631 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2555,46556101,-;type=1400 audit(1614200581.026:183): avc: denied { read } for comm="Binder:557_2" name="wakeup46" dev="sysfs" ino=60220 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2556,46556356,-;type=1400 audit(1614200581.026:184): avc: denied { read } for comm="Binder:557_2" name="wakeup2" dev="sysfs" ino=36628 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2557,46556545,-;type=1400 audit(1614200581.036:185): avc: denied { read } for comm="Binder:557_2" name="wakeup64" dev="sysfs" ino=63936 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
6,2558,46559249,-;[wpa_su][0x4990f055][21:03:01.052690] wlan: [1756:I:CMN_MLME] mlme_vdev_sm_spinlock_create: 211: VDEV SM lock is disabled!!!
6,2559,46559265,-;[wpa_su][0x4990f1be][21:03:01.052709] wlan: [1756:I:CMN_MLME] mlme_vdev_cmd_mutex_create: 231: VDEV CMD lock is disabled!!!
6,2560,46559459,-;[wpa_su][0x4991004f][21:03:01.052903] wlan: [1756:I:OBJMGR] wlan_objmgr_vdev_obj_create: 269: Created vdev 1
36,2561,46559675,-;type=1400 audit(1614200581.036:186): avc: denied { read } for comm="Binder:557_2" name="wakeup26" dev="sysfs" ino=47722 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2562,46560092,-;type=1400 audit(1614200581.036:187): avc: denied { read } for comm="Binder:557_2" name="wakeup54" dev="sysfs" ino=60520 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2563,46564519,-;type=1400 audit(1614200581.046:188): avc: denied { read } for comm="Binder:557_2" name="wakeup44" dev="sysfs" ino=60148 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
6,2564,46565831,-;IPv6: ADDRCONF(NETDEV_UP): p2p0: link is not ready
3,2565,46585440,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2566,46592132,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2567,46594065,-;[schedu][0x499b2381][21:03:01.087506] wlan: [1653:I:TXRX] ol_txrx_peer_detach_sync: 3303: ol_txrx_peer_detach_sync peer ffffffc063766ce8, peer->ref_cnt 7
12,2568,46603072,-;healthd: battery l=51 v=3720 t=31.0 h=2 st=2 c=-878754 fc=3812000 cc=0 chg=a
6,2569,46606045,-;[soft_i][0x499ea5e2][21:03:01.099484] wlan: [0:I:TXRX] ol_txrx_peer_release_ref: 3074: [9][0]: Deleting peer ffffffc063766ce8 ref_cnt -> 0 
3,2570,46606904,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2571,46613195,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2572,46616950,-;[wpa_su][0x49a1d7a5][21:03:01.110388] wlan: [1756:I:OBJMGR] wlan_objmgr_vdev_obj_delete: 341: Logically deleting vdev 1
6,2573,46621332,-;[wpa_su][0x49a32095][21:03:01.114774] wlan: [1756:I:CMN_MLME] mlme_vdev_cmd_mutex_destroy: 237: VDEV CMD lock is disabled!!!
6,2574,46621346,-;[wpa_su][0x49a321de][21:03:01.114791] wlan: [1756:I:CMN_MLME] mlme_vdev_sm_spinlock_destroy: 217: VDEV SM lock is disabled!!!
3,2575,46625865,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2576,46627944,-;[wpa_su][0x49a51021][21:03:01.121381] wlan: [1756:I:CMN_MLME] mlme_vdev_sm_spinlock_create: 211: VDEV SM lock is disabled!!!
3,2577,46631646,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2578,46638488,-;[wpa_su][0x49a826b4][21:03:01.131923] wlan: [1756:I:CMN_MLME] mlme_vdev_cmd_mutex_create: 231: VDEV CMD lock is disabled!!!
6,2579,46639401,-;[wpa_su][0x49a86b58][21:03:01.132837] wlan: [1756:I:OBJMGR] wlan_objmgr_vdev_obj_create: 269: Created vdev 1
6,2580,46643942,-;IPv6: ADDRCONF(NETDEV_UP): p2p0: link is not ready
11,2581,47154215,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2582,47285523,-;init: Control message: Could not find 'vendor.qti.qspmhal@1.0::IQspmhal/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2583,47408345,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2584,47623644,-;init: starting service 'qspmhal'...
14,2585,47905494,-;init: Untracked pid 2335 exited with status 0
14,2586,47909007,-;init: Service 'qspmhal' (pid 2319) received signal 6
6,2587,48525971,-;[wifi@1][0x4bd1206e][21:03:03.019411] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_create: 211: VDEV SM lock is disabled!!!
6,2588,48527288,-;[wifi@1][0x4bd121c9][21:03:03.019430] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_create: 231: VDEV CMD lock is disabled!!!
6,2589,48527460,-;[wifi@1][0x4bd19069][21:03:03.020904] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_create: 269: Created vdev 2
3,2590,48529650,-;[wifi@1][0x4bd23408][21:03:03.023086] wlan: [764:E:PMO] pmo_register_wow_wakeup_events: 88: Skipping wake event configuration for vdev_opmode 16
3,2591,48544789,-;[wifi@1][0x4bd6a387][21:03:03.038226] wlan: [764:E:SME] sme_get_nss_chain_shift: 4154: Device mode 16 invalid
3,2592,48557012,-;[wifi@1][0x4bda34c2][21:03:03.050403] wlan: [764:E:SME] sme_get_nss_chain_shift: 4154: Device mode 16 invalid
6,2593,48573027,-;IPv6: ADDRCONF(NETDEV_UP): wifi-aware0: link is not ready
6,2594,48598809,-;[schedu][0x4be67736][21:03:03.092249] wlan: [1653:I:TXRX] ol_txrx_peer_detach_sync: 3303: ol_txrx_peer_detach_sync peer ffffffc063766ce8, peer->ref_cnt 7
6,2595,48606024,-;[soft_i][0x4be8943c][21:03:03.099462] wlan: [0:I:TXRX] ol_txrx_peer_release_ref: 3074: [9][0]: Deleting peer ffffffc063766ce8 ref_cnt -> 0 
6,2596,48618862,-;[wpa_su][0x4bec56c7][21:03:03.112296] wlan: [1756:I:OBJMGR] wlan_objmgr_vdev_obj_delete: 341: Logically deleting vdev 1
6,2597,48619191,-;[wpa_su][0x4bec6fc4][21:03:03.112629] wlan: [1756:I:CMN_MLME] mlme_vdev_cmd_mutex_destroy: 237: VDEV CMD lock is disabled!!!
6,2598,48619212,-;[wpa_su][0x4bec7182][21:03:03.112653] wlan: [1756:I:CMN_MLME] mlme_vdev_sm_spinlock_destroy: 217: VDEV SM lock is disabled!!!
14,2599,48627276,-;Boot completed 
6,2600,48689883,-;[wifi@1][0x4c01252e][21:03:03.183315] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_delete: 341: Logically deleting vdev 2
6,2601,48690081,-;[wifi@1][0x4c013492][21:03:03.183520] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_destroy: 237: VDEV CMD lock is disabled!!!
6,2602,48690101,-;[wifi@1][0x4c01362d][21:03:03.183542] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_destroy: 217: VDEV SM lock is disabled!!!
6,2603,49509998,-;tas2563 0-004c: tas2563_hw_params, format: 2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2604,49510009,-;tas2563 0-004c: tas2563_set_bitwidth 1565
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,2605,49510395,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,2606,49538887,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:8, mask: 0xc, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2607,49538898,-;tas2563 0-004c: mnCh_size: 16
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2608,49538906,-;tas2563 0-004c: blr_clk_ratio: 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2609,49539277,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2610,49540116,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x44
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2611,49540133,-;tas2563 0-004c: tas2563_hw_params, sample rate: 48000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2612,49540627,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:6, mask: 0x20, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2613,49540998,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:6, mask: 0xe, val: 0x8
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2614,49542857,-;__afe_port_start: port id: 0x1002
6,2615,49542884,-;afe_find_cal_topo_id_by_port: port id: 0x1002, dev_acdb_id: 0
6,2616,49542898,-;afe_find_cal_topo_id_by_port: top_id:112fc acdb_id:15 afe_port:0x1002
6,2617,49542912,-;afe_get_cal_topology_id: port_id = 0x1002 acdb_id = 15 topology_id = 0x112fc cal_type_index=8 ret=0
6,2618,49543198,-;afe_send_port_topology_id: AFE set topology id 0x112fc  enable for port 0x1002 ret 0
6,2619,49543208,-;send_afe_cal_type: cal_index is 0
6,2620,49543215,-;send_afe_cal_type: dev_acdb_id[36] is 0
6,2621,49543224,-;send_afe_cal_type: Sending cal_index cal 0
3,2622,49543233,-;send_afe_cal_type: No cal sent for cal_index 0, port_id = 0x1002! ret -22
6,2623,49551920,-;afe_send_hw_delay: port_id 0x1002 rate 48000 delay_usec 474 status 0
6,2624,49562583,-;tas2563 0-004c: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2625,49562595,-;tas2563 0-004c: unmute: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2626,49562603,-;tas2563 0-004c: set power state: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2627,49562611,-;tas2563 0-004c: tas2563_set_power_state, state: 0, mbPowerup 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,2628,49562620,-;tas2563 0-004c: tas2563_set_calibration start 
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2629,49568303,-;tas2563 0-004c: tas2563_load_calibration:
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2630,49599440,-;zram0: detected capacity change from 0 to 2147483648
6,2631,49607883,-;tas2563 0-004c: TAS2563 calibration file = /mnt/vendor/persist/audio/tas2563_cal.bin, handle = -1752696512
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,2632,49609219,-;tas2563 0-004c: Calibration 0 doesn't exist
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,2633,49614525,-;tas2563 0-004c: tas2563_set_calibration finish 
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2634,49620822,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:2, mask: 0xf, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2635,49620833,-;tas2563 0-004c: tas2563_set_power_state  channel is 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2636,49621416,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:48, mask: 0x4, val: 0x4
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2637,49718210,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2638,49718484,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2639,49718850,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2640,49719211,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2641,49728671,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2642,49731798,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2643,49732563,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2644,49736553,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2645,49737645,-;Adding 2097148k swap on /dev/block/zram0.  Priority:32758 extents:1 across:2097148k SS
6,2646,50553085,-;sdcardfs version 2.0
6,2647,50553096,-;sdcardfs: dev_name -> /data/media
6,2648,50553104,-;sdcardfs: options -> fsuid=1023,fsgid=1023,multiuser,derive_gid,default_normal,unshared_obb,mask=6,userid=0,gid=1015
6,2649,50553112,-;sdcardfs: mnt -> ffffffc060aabae0
6,2650,50553374,-;sdcardfs: mounted on top of /data/media type f2fs
6,2651,50562220,-;Remount options were mask=23,gid=9997 for vfsmnt ffffffc060aaeee0.
6,2652,50562259,-;sdcardfs : options - debug:1
6,2653,50562266,-;sdcardfs : options - gid:9997
6,2654,50562273,-;sdcardfs : options - mask:23
6,2655,50573936,-;Remount options were mask=7,gid=9997 for vfsmnt ffffffc05db078a0.
6,2656,50573979,-;sdcardfs : options - debug:1
6,2657,50573987,-;sdcardfs : options - gid:9997
6,2658,50573994,-;sdcardfs : options - mask:7
6,2659,50581976,-;Remount options were mask=7,gid=9997 for vfsmnt ffffffc05db03120.
6,2660,50582031,-;sdcardfs : options - debug:1
6,2661,50582038,-;sdcardfs : options - gid:9997
6,2662,50582045,-;sdcardfs : options - mask:7
11,2663,51171743,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2664,51252961,-;init: Sending signal 9 to service 'idmap2d' (pid 1097) process group...
14,2665,51268401,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 1097 in 13ms
14,2666,51271027,-;init: Control message: Processed ctl.stop for 'idmap2d' from pid: 957 (system_server)
14,2667,51272418,-;init: Service 'idmap2d' (pid 1097) received signal 9
11,2668,51427905,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2669,52072668,-;[wifi@1][0x4fe0325e][21:03:06.566104] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_delete: 341: Logically deleting vdev 0
6,2670,52072756,-;[wifi@1][0x4fe0397e][21:03:06.566199] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_destroy: 237: VDEV CMD lock is disabled!!!
6,2671,52072767,-;[wifi@1][0x4fe03a77][21:03:06.566212] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_destroy: 217: VDEV SM lock is disabled!!!
6,2672,52079992,-;[wifi@1][0x4fe25805][21:03:06.573433] wlan: [764:I:CMN_MLME] mlme_vdev_sm_spinlock_create: 211: VDEV SM lock is disabled!!!
6,2673,52080007,-;[wifi@1][0x4fe25969][21:03:06.573451] wlan: [764:I:CMN_MLME] mlme_vdev_cmd_mutex_create: 231: VDEV CMD lock is disabled!!!
6,2674,52089719,-;[wifi@1][0x4fe5317b][21:03:06.583159] wlan: [764:I:OBJMGR] wlan_objmgr_vdev_obj_create: 269: Created vdev 0
3,2675,52178512,-;[wpa_su][0x4fff3500][21:03:06.671952] wlan: [1756:E:crypto] wlan_get_crypto_params_from_wpa_ie: 3829: WPA IE NULL
3,2676,52194100,-;[wpa_su][0x5003c613][21:03:06.687540] wlan: [1756:E:SER] wlan_serialization_peek_head_pending_cmd_using_psoc: 204: Empty Queue
11,2677,52196807,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2678,52209560,-;[wpa_su][0x50084d97][21:03:06.703000] wlan: [1756:I:SME] vdev-0: Connecting to sc31RFLab f0:7f:06:cc:c0:4f rssi: -66 channel: 132 akm 9 cipher: uc 6 mc 6, CC: 
6,2679,52224860,-;[schedu][0x500cc910][21:03:06.718300] wlan: [1653:I:WMA] wma_set_channel: 4223: vht_capable: 1, dot11_mode: 7
6,2680,52224952,-;[schedu][0x500cd027][21:03:06.718394] wlan: [1653:I:WMI] send_vdev_start_cmd_tlv: vdev_id 0 freq 5660 chanmode 8 ch_info: 0x8 is_dfs 0 beacon interval 100 dtim 1 center_chan 5660 center_freq2 0 reg_info_1: 0x180000 reg_info_2: 0x1800, req->max_txpow: 0x18 Tx SS 1, Rx SS 1, ldpc_rx: 0, cac 0, regd 0, HE ops: 0req->dis_hw_ack: 1 
6,2681,52312447,-;[schedu][0x502671be][21:03:06.805882] wlan: [1653:I:PE] Auth TX: seq 1 seq num 2049 status 0 WEP 0 to f0:7f:06:cc:c0:4f
6,2682,52314843,-;[schedu][0x50272590][21:03:06.808280] wlan: [1653:I:PE] Auth TX: success
6,2683,52315294,-;[schedu][0x5027474b][21:03:06.808730] wlan: [1653:I:PE] Auth RX: vdev 0 sys role 3 lim_state 5 from f0:7f:06:cc:c0:4f rssi -64 auth_alg 0 seq 2304
6,2684,52316036,-;[schedu][0x50277f0e][21:03:06.809473] wlan: [1653:I:PE] Assoc req TX: vdev 0 to f0:7f:06:cc:c0:4f seq num 2050
6,2685,52319174,-;[schedu][0x50286a4e][21:03:06.812610] wlan: [1653:I:PE] Assoc req TX: success
6,2686,52323848,-;[soft_i][0x5029c88c][21:03:06.817280] wlan: [0:I:TXRX] ol_txrx_enqueue_rx_frames: 4635: Data on the peer before it is registered bufq->curr 0 bufq->drops 0
6,2687,52325262,-;[schedu][0x502a31ef][21:03:06.818685] wlan: [1653:I:PE] Assoc rsp RX: subtype 0 vdev 0 sys role 3 lim state 10 rssi 64 from f0:7f:06:cc:c0:4f
6,2688,52339191,-;[schedu][0x502e47e3][21:03:06.832631] wlan: [1653:I:HDD] wlan0(vdevid-0): 3e:fd:55:14:24:bf connected to f0:7f:06:cc:c0:4f
6,2689,52354878,-;[schedu][0x5032e06b][21:03:06.848318] wlan: [1653:I:QDF] EAPOL-1 RX: SA:f0:7f:06:cc:c0:4f DA:3e:fd:55:14:24:bf
6,2690,52361377,-;[soft_i][0x5034c788][21:03:06.854813] wlan: [0:I:QDF] EAPOL-2 TX: SA:3e:fd:55:14:24:bf DA:f0:7f:06:cc:c0:4f msdu_id:1199 status: succ
6,2691,52362640,-;[cds_ol][0x5035261b][21:03:06.856074] wlan: [1659:I:QDF] EAPOL-3 RX: SA:f0:7f:06:cc:c0:4f DA:3e:fd:55:14:24:bf
6,2692,52376536,-;[soft_i][0x50393573][21:03:06.869932] wlan: [0:I:QDF] EAPOL-4 TX: SA:3e:fd:55:14:24:bf DA:f0:7f:06:cc:c0:4f msdu_id:1199 status: succ
3,2693,52388470,-;[schedu][0x503cb7a3][21:03:06.881908] wlan: [1653:E:QDF] qdf_mc_timer_start: Cannot start timer in state = 21 sme_auto_ps_entry_timer_expired [wlan]
6,2694,52417367,-;[schedu][0x50452f1b][21:03:06.910807] wlan: [1653:I:WMI] LFR3:OKC enabled
6,2695,52417382,-;[schedu][0x50453088][21:03:06.910826] wlan: [1653:I:WMI] LFR3:PMKSA caching enabled
3,2696,52428972,-;[schedu][0x50489562][21:03:06.922411] wlan: [1653:E:QDF] qdf_mc_timer_start: Cannot start timer in state = 21 sme_auto_ps_entry_timer_expired [wlan]
11,2697,52432394,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2698,52580532,-;[wifi@1][0x5074fc7e][21:03:07.073972] wlan: [764:E:HDD] hdd_enable_ns_offload: 438: Failed to cache ns request; status:4
14,2699,52640885,-;init: starting service 'qspmhal'...
6,2700,52736183,-;[soft_i][0x50a295c7][21:03:07.229616] wlan: [0:I:QDF] DHCP-R TX: SA:3e:fd:55:14:24:bf DA:ff:ff:ff:ff:ff:ff msdu_id:1199 status: succ
6,2701,52738800,-;[cds_ol][0x50a35a0d][21:03:07.232233] wlan: [1659:I:QDF] DHCP-A RX: SA:f0:7f:06:cc:c0:40 DA:3e:fd:55:14:24:bf
36,2702,53047711,-;type=1400 audit(1614200587.526:252): avc: denied { read } for comm="Binder:557_2" name="wakeup48" dev="sysfs" ino=60292 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
4,2703,53109837,-;audit: audit_lost=1 audit_rate_limit=5 audit_backlog_limit=64
3,2704,53109849,-;audit: rate limit exceeded
31,2705,53117178,-;logd: logdr: UID=1000 GID=1000 PID=3028 n tail=50 logMask=8 pid=2991 start=0ns timeout=0ns
36,2706,53158364,-;type=1400 audit(1614200587.536:253): avc: denied { read } for comm="Binder:557_2" name="wakeup4" dev="sysfs" ino=36664 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2707,53158711,-;type=1400 audit(1614200587.566:254): avc: denied { read } for comm="Binder:557_2" name="wakeup28" dev="sysfs" ino=48113 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2708,53158914,-;type=1400 audit(1614200587.566:255): avc: denied { read } for comm="Binder:557_2" name="wakeup18" dev="sysfs" ino=37631 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2709,53159101,-;type=1400 audit(1614200587.576:256): avc: denied { read } for comm="Binder:557_2" name="wakeup46" dev="sysfs" ino=60220 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2710,53159342,-;type=1400 audit(1614200587.576:257): avc: denied { read } for comm="Binder:557_2" name="wakeup2" dev="sysfs" ino=36628 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2711,53159524,-;type=1400 audit(1614200587.586:258): avc: denied { read } for comm="Binder:557_2" name="wakeup64" dev="sysfs" ino=63936 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,2712,53159701,-;type=1400 audit(1614200587.586:259): avc: denied { read } for comm="Binder:557_2" name="wakeup26" dev="sysfs" ino=47722 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
31,2713,53160414,-;logd: logdr: UID=1000 GID=1000 PID=3028 n tail=50 logMask=1 pid=2991 start=0ns timeout=0ns
11,2714,53182382,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2715,53749345,-;[schedu][0x51cb6993][21:03:08.242787] wlan: [1653:I:WMI] LFR3:OKC enabled
6,2716,53749360,-;[schedu][0x51cb6aea][21:03:08.242805] wlan: [1653:I:WMI] LFR3:PMKSA caching enabled
6,2717,53750055,-;[schedu][0x51cb9ec6][21:03:08.243496] wlan: [1653:I:WMI] LFR3:OKC enabled
6,2718,53750067,-;[schedu][0x51cb9ffa][21:03:08.243512] wlan: [1653:I:WMI] LFR3:PMKSA caching enabled
3,2719,53774327,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2720,53780473,-;nq-nci 0-0028: nfc_write: failed to write -107
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
3,2721,53799403,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2722,53804153,-;nq-nci 0-0028: nfc_write: failed to write -107
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
3,2723,53823323,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2724,53828123,-;nq-nci 0-0028: nfc_write: failed to write -107
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
3,2725,53846332,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2726,53851282,-;nq-nci 0-0028: nfc_write: failed to write -107
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
6,2727,53868967,-;IRQ 6: no longer affine to CPU7
3,2728,53873444,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2729,53880475,-;nq-nci 0-0028: nfc_write: failed to write -107
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
3,2730,53898852,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
3,2731,53905470,-;nq-nci 0-0028: nfc_write: failed to write -107
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0028
6,2732,54589439,-;sdcardfs version 2.0
6,2733,54589450,-;sdcardfs: dev_name -> /ipsm/media
6,2734,54589457,-;sdcardfs: options -> fsuid=1023,fsgid=1023,mask=6,userid=0,gid=1015
6,2735,54589464,-;sdcardfs: mnt -> ffffffc04ae161e0
6,2736,54589659,-;sdcardfs: mounted on top of /ipsm/media type ext4
6,2737,54599921,-;Remount options were mask=18,gid=9997 for vfsmnt ffffffc04adc3460.
6,2738,54599948,-;sdcardfs : options - debug:1
6,2739,54599955,-;sdcardfs : options - gid:9997
6,2740,54599962,-;sdcardfs : options - mask:18
6,2741,54609484,-;Remount options were mask=18,gid=9997 for vfsmnt ffffffc04aec6860.
6,2742,54609510,-;sdcardfs : options - debug:1
6,2743,54609517,-;sdcardfs : options - gid:9997
6,2744,54609524,-;sdcardfs : options - mask:18
3,2745,54610180,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2746,54615897,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2747,54618250,-;Remount options were mask=7,gid=9997 for vfsmnt ffffffc04aecade0.
6,2748,54622054,-;sdcardfs : options - debug:1
6,2749,54622061,-;sdcardfs : options - gid:9997
6,2750,54622068,-;sdcardfs : options - mask:7
3,2751,54626971,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2752,54633619,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2753,54640506,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2754,54646292,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2755,54657601,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2756,54663526,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2757,54670740,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2758,54676651,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2759,54710328,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2760,54720486,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2761,54773094,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2762,54780474,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2763,54793278,-;healthd: battery l=51 v=3785 t=30.9 h=2 st=2 c=-474853 fc=3812000 cc=0 chg=a
3,2764,54795514,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2765,54801450,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2766,54817930,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2767,54823791,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,2768,54878399,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2769,54878790,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2770,54879126,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2771,54881191,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2772,54889424,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2773,54891078,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2774,54891552,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2775,54892107,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
11,2776,56200542,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2777,56453989,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2778,57204820,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2779,57437239,-;tas2563 0-004c: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2780,57437369,-;tas2563 0-004c: mute: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2781,57437408,-;tas2563 0-004c: set power state: 2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,2782,57437449,-;tas2563 0-004c: tas2563_set_power_state, state: 2, mbPowerup 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,2783,57439093,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:2, mask: 0x3, val: 0x2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
11,2784,57462097,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2785,57490922,-;afe_close: port_id = 0x1002
14,2786,57664685,-;init: starting service 'qspmhal'...
31,2787,58051980,-;logd: logdr: UID=1000 GID=1000 PID=3242 n tail=0 logMask=8 pid=3239 start=0ns timeout=0ns
31,2788,58065258,-;logd: logdr: UID=1000 GID=1000 PID=3242 n tail=0 logMask=1 pid=3239 start=0ns timeout=0ns
14,2789,58090261,-;init: Service 'qspmhal' (pid 3239) received signal 6
14,2790,58090435,-;init: Sending signal 9 to service 'qspmhal' (pid 3239) process group...
14,2791,58111532,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3239 in 20ms
14,2792,58116806,-;init: Untracked pid 3242 exited with status 0
14,2793,58117281,-;init: Untracked pid 3244 received signal 9
11,2794,61232485,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2795,61481969,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2796,62239258,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2797,62491227,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2798,62693377,-;init: starting service 'qspmhal'...
3,2799,62777135,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2800,62784873,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2801,62798926,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2802,62805303,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2803,62812532,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2804,62818676,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2805,62826184,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2806,62832362,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2807,62848723,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2808,62855816,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2809,62889468,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2810,62896746,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2811,62965086,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2812,62971591,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2813,62987397,-;healthd: battery l=51 v=3790 t=30.9 h=2 st=2 c=-357971 fc=3812000 cc=0 chg=a
3,2814,62992181,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2815,62997886,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2816,63009032,-;logd: logdr: UID=1000 GID=1000 PID=3265 n tail=50 logMask=8 pid=3262 start=0ns timeout=0ns
3,2817,63015568,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2818,63016643,-;logd: logdr: UID=1000 GID=1000 PID=3265 n tail=50 logMask=1 pid=3262 start=0ns timeout=0ns
3,2819,63021479,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2820,63040068,-;logd: logdr: UID=1000 GID=1000 PID=3265 n tail=0 logMask=8 pid=3262 start=0ns timeout=0ns
31,2821,63051114,-;logd: logdr: UID=1000 GID=1000 PID=3265 n tail=0 logMask=1 pid=3262 start=0ns timeout=0ns
14,2822,63067740,-;init: Service 'qspmhal' (pid 3262) received signal 6
14,2823,63067854,-;init: Sending signal 9 to service 'qspmhal' (pid 3262) process group...
14,2824,63094557,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3262 in 25ms
14,2825,63101885,-;init: Untracked pid 3265 exited with status 0
14,2826,63103147,-;init: Untracked pid 3267 received signal 9
11,2827,66271407,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2828,66516340,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2829,66823818,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2830,66842971,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2831,66918531,-;init: Service 'adbd' (pid 1022) exited with status 1
14,2832,66918606,-;init: Sending signal 9 to service 'adbd' (pid 1022) process group...
14,2833,66919760,-;libprocessgroup: Successfully killed process cgroup uid 0 pid 1022 in 0ms
14,2834,66924948,-;init: starting service 'adbd'...
14,2835,66928264,-;init: Created socket '/dev/socket/adbd', mode 660, user 1000, group 1000
6,2836,67044387,-;read descriptors
6,2837,67045263,-;read strings
14,2838,67053556,-;init: processing action (sys.usb.config=diag,adb && sys.usb.configfs=1 && sys.usb.ffs.ready=1) from (/vendor/etc/init/hw/init.qcom.usb.rc:192)
6,2839,67153014,-;android_work: sent uevent USB_STATE=DISCONNECTED
6,2840,67346994,-;android_work: did not send uevent (0 0 0000000000000000)
6,2841,67436949,-;android_work: sent uevent USB_STATE=CONNECTED
6,2842,67513068,-;configfs-gadget gadget: high-speed config #1: b
6,2843,67515979,-;android_work: sent uevent USB_STATE=CONFIGURED
31,2844,68083794,-;logd: logdr: UID=1000 GID=1000 PID=3344 n tail=50 logMask=8 pid=3340 start=0ns timeout=0ns
31,2845,68092888,-;logd: logdr: UID=1000 GID=1000 PID=3344 n tail=50 logMask=1 pid=3340 start=0ns timeout=0ns
31,2846,68104940,-;logd: logdr: UID=1000 GID=1000 PID=3344 n tail=0 logMask=8 pid=3340 start=0ns timeout=0ns
31,2847,68118774,-;logd: logdr: UID=1000 GID=1000 PID=3344 n tail=0 logMask=1 pid=3340 start=0ns timeout=0ns
3,2848,70947451,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2849,70962815,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2850,70984131,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2851,70990354,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2852,70999578,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2853,71005594,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2854,71016468,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2855,71022501,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2856,71029892,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2857,71036171,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2858,71060120,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2859,71068806,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2860,71111725,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2861,71119853,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2862,71132959,-;healthd: battery l=51 v=3790 t=30.9 h=2 st=2 c=-303497 fc=3812000 cc=0 chg=a
3,2863,71136044,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2864,71141912,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2865,71170462,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2866,71176214,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,2867,71554776,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2868,71860536,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2869,72560795,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2870,72785897,-;init: starting service 'qspmhal'...
11,2871,72865402,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,2872,73144993,-;logd: logdr: UID=1000 GID=1000 PID=3367 n tail=50 logMask=8 pid=3363 start=0ns timeout=0ns
31,2873,73156556,-;logd: logdr: UID=1000 GID=1000 PID=3367 n tail=50 logMask=1 pid=3363 start=0ns timeout=0ns
31,2874,73175588,-;logd: logdr: UID=1000 GID=1000 PID=3367 n tail=0 logMask=8 pid=3363 start=0ns timeout=0ns
31,2875,73185647,-;logd: logdr: UID=1000 GID=1000 PID=3367 n tail=0 logMask=1 pid=3363 start=0ns timeout=0ns
14,2876,73204314,-;init: Service 'qspmhal' (pid 3363) received signal 6
14,2877,73204407,-;init: Sending signal 9 to service 'qspmhal' (pid 3363) process group...
14,2878,73225998,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3363 in 21ms
14,2879,73232926,-;init: Untracked pid 3367 exited with status 0
14,2880,73233570,-;init: Untracked pid 3369 received signal 9
11,2881,76588599,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2882,76889705,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2883,77594772,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2884,77832780,-;init: starting service 'qspmhal'...
11,2885,77893362,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2886,77973570,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2887,77985242,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2888,78001768,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2889,78007472,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2890,78015580,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2891,78025077,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2892,78027046,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2893,78037314,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2894,78040050,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2895,78049284,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2896,78056677,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2897,78062607,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2898,78068974,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2899,78074654,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2900,78082004,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2901,78087924,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2902,78093285,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2903,78099812,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2904,78108530,-;healthd: battery l=51 v=3744 t=31.1 h=2 st=2 c=-558777 fc=3812000 cc=0 chg=a
3,2905,78110575,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2906,78116266,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2907,78166018,-;logd: logdr: UID=1000 GID=1000 PID=3406 n tail=50 logMask=8 pid=3398 start=0ns timeout=0ns
3,2908,78167830,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2909,78173077,-;logd: logdr: UID=1000 GID=1000 PID=3406 n tail=50 logMask=1 pid=3398 start=0ns timeout=0ns
3,2910,78173585,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2911,78183268,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2912,78185568,-;logd: logdr: UID=1000 GID=1000 PID=3406 n tail=0 logMask=8 pid=3398 start=0ns timeout=0ns
3,2913,78189026,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2914,78197683,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2915,78203470,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,2916,78205571,-;logd: logdr: UID=1000 GID=1000 PID=3406 n tail=0 logMask=1 pid=3398 start=0ns timeout=0ns
12,2917,78211526,-;healthd: battery l=51 v=3763 t=30.9 h=2 st=2 c=-691681 fc=3812000 cc=0 chg=a
3,2918,78212729,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2919,78218468,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,2920,78223237,-;init: Untracked pid 3406 exited with status 0
14,2921,78226012,-;init: Service 'qspmhal' (pid 3398) received signal 6
14,2922,78226080,-;init: Sending signal 9 to service 'qspmhal' (pid 3398) process group...
14,2923,78238679,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3398 in 12ms
3,2924,78239309,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,2925,78242571,-;init: Untracked pid 3408 exited with status 0
3,2926,78244998,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
38,2927,78429986,-;type=1400 audit(1614200612.916:290): avc: denied { getattr } for comm="remount" name="/" dev="sde4" ino=1 scontext=u:r:su:s0 tcontext=u:object_r:firmware_file:s0 tclass=filesystem permissive=1
38,2928,78434412,-;type=1400 audit(1614200612.916:291): avc: denied { getattr } for comm="remount" name="/" dev="sde5" ino=1 scontext=u:r:su:s0 tcontext=u:object_r:bt_firmware_file:s0 tclass=filesystem permissive=1
38,2929,78464216,-;type=1400 audit(1614200612.946:292): avc: denied { getattr } for comm="remount" name="/" dev="sde4" ino=1 scontext=u:r:su:s0 tcontext=u:object_r:firmware_file:s0 tclass=filesystem permissive=1
3,2930,78821938,-;msm_rpm_flush_requests: Error: more than 24 requests are buffered
3,2931,79106856,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2932,79113723,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2933,79126697,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2934,79133147,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2935,79141923,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2936,79147648,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2937,79155654,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2938,79161988,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2939,79171555,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2940,79177278,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2941,79195864,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2942,79201728,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2943,79242641,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2944,79248454,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2945,79258221,-;healthd: battery l=51 v=3819 t=30.9 h=2 st=2 c=-244751 fc=3812000 cc=0 chg=a
3,2946,79261293,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2947,79267023,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2948,79286345,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2949,79292184,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,2950,81624562,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2951,81933595,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,2952,82436705,-;[schedu][0x729fe741][21:03:36.930116] wlan: [1653:I:WMA] [21:03:36.926000] [NEIGH_RPT_REQ] VDEV[0]
6,2953,82436775,-;[schedu][0x729fed67][21:03:36.930198] wlan: [1653:I:WMA] [21:03:36.928000] [NEIGH_RPT_RSP] VDEV[0] { 2412 5680 }
11,2954,82633724,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2955,82869580,-;init: starting service 'qspmhal'...
11,2956,82940056,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,2957,83236857,-;logd: logdr: UID=1000 GID=1000 PID=3435 n tail=50 logMask=8 pid=3431 start=0ns timeout=0ns
31,2958,83251273,-;logd: logdr: UID=1000 GID=1000 PID=3435 n tail=50 logMask=1 pid=3431 start=0ns timeout=0ns
31,2959,83273703,-;logd: logdr: UID=1000 GID=1000 PID=3435 n tail=0 logMask=8 pid=3431 start=0ns timeout=0ns
31,2960,83287004,-;logd: logdr: UID=1000 GID=1000 PID=3435 n tail=0 logMask=1 pid=3431 start=0ns timeout=0ns
14,2961,83306962,-;init: Service 'qspmhal' (pid 3431) received signal 6
14,2962,83307048,-;init: Sending signal 9 to service 'qspmhal' (pid 3431) process group...
14,2963,83333466,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3431 in 25ms
14,2964,83345705,-;init: Untracked pid 3435 exited with status 0
14,2965,83346477,-;init: Untracked pid 3437 received signal 9
11,2966,86666638,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2967,86969274,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,2968,87267503,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2969,87273347,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2970,87281957,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2971,87288655,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2972,87295409,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2973,87301466,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2974,87308863,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2975,87314558,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2976,87321693,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2977,87327795,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2978,87354937,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2979,87360700,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2980,87388746,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2981,87394440,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,2982,87402618,-;healthd: battery l=51 v=3759 t=31.1 h=2 st=2 c=-603180 fc=3812000 cc=0 chg=a
3,2983,87405433,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2984,87411369,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2985,87424064,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,2986,87429839,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,2987,87502715,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2988,87521196,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,2989,87669745,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,2990,87914929,-;init: starting service 'qspmhal'...
31,2991,88273395,-;logd: logdr: UID=1000 GID=1000 PID=3484 n tail=50 logMask=8 pid=3481 start=0ns timeout=0ns
31,2992,88282828,-;logd: logdr: UID=1000 GID=1000 PID=3484 n tail=50 logMask=1 pid=3481 start=0ns timeout=0ns
31,2993,88302029,-;logd: logdr: UID=1000 GID=1000 PID=3484 n tail=0 logMask=8 pid=3481 start=0ns timeout=0ns
31,2994,88314934,-;logd: logdr: UID=1000 GID=1000 PID=3484 n tail=0 logMask=1 pid=3481 start=0ns timeout=0ns
14,2995,88338527,-;init: Service 'qspmhal' (pid 3481) received signal 6
14,2996,88338764,-;init: Sending signal 9 to service 'qspmhal' (pid 3481) process group...
14,2997,88374372,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3481 in 34ms
14,2998,88384545,-;init: Untracked pid 3484 exited with status 0
3,2999,91301663,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3000,91307374,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3001,91323053,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3002,91328836,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3003,91338346,-;healthd: battery l=51 v=3814 t=30.7 h=2 st=2 c=-225982 fc=3812000 cc=0 chg=a
3,3004,91340897,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3005,91346596,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3006,91359351,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3007,91365051,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3008,91706730,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3009,92547657,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3010,92716360,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3011,92944516,-;init: starting service 'qspmhal'...
31,3012,93305331,-;logd: logdr: UID=1000 GID=1000 PID=3505 n tail=50 logMask=8 pid=3502 start=0ns timeout=0ns
31,3013,93317674,-;logd: logdr: UID=1000 GID=1000 PID=3505 n tail=50 logMask=1 pid=3502 start=0ns timeout=0ns
31,3014,93340684,-;logd: logdr: UID=1000 GID=1000 PID=3505 n tail=0 logMask=8 pid=3502 start=0ns timeout=0ns
31,3015,93356089,-;logd: logdr: UID=1000 GID=1000 PID=3505 n tail=0 logMask=1 pid=3502 start=0ns timeout=0ns
14,3016,93379213,-;init: Service 'qspmhal' (pid 3502) received signal 6
14,3017,93379447,-;init: Sending signal 9 to service 'qspmhal' (pid 3502) process group...
14,3018,93410502,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3502 in 30ms
14,3019,93415171,-;init: Untracked pid 3505 exited with status 0
14,3020,93415593,-;init: Untracked pid 3507 received signal 9
11,3021,93557670,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3022,95431190,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3023,95436937,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3024,95466843,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3025,95473034,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3026,95479938,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3027,95485647,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3028,95494060,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3029,95500076,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3030,95507694,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3031,95513810,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3032,95543101,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3033,95548914,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3034,95618690,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3035,95624416,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3036,95635307,-;healthd: battery l=51 v=3822 t=30.7 h=2 st=2 c=-254821 fc=3812000 cc=0 chg=a
3,3037,95638013,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3038,95644063,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3039,95660035,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3040,95665736,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3041,96751337,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3042,97591341,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3043,97759513,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3044,97994521,-;init: starting service 'qspmhal'...
31,3045,98373477,-;logd: logdr: UID=1000 GID=1000 PID=3527 n tail=50 logMask=8 pid=3524 start=0ns timeout=0ns
31,3046,98384706,-;logd: logdr: UID=1000 GID=1000 PID=3527 n tail=50 logMask=1 pid=3524 start=0ns timeout=0ns
31,3047,98405852,-;logd: logdr: UID=1000 GID=1000 PID=3527 n tail=0 logMask=8 pid=3524 start=0ns timeout=0ns
31,3048,98421161,-;logd: logdr: UID=1000 GID=1000 PID=3527 n tail=0 logMask=1 pid=3524 start=0ns timeout=0ns
14,3049,98446911,-;init: Untracked pid 3527 exited with status 0
14,3050,98466096,-;init: Service 'qspmhal' (pid 3524) received signal 6
14,3051,98466353,-;init: Sending signal 9 to service 'qspmhal' (pid 3524) process group...
14,3052,98476058,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3524 in 9ms
14,3053,98482433,-;init: Untracked pid 3529 exited with status 0
11,3054,98597557,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3055,100411816,-;boot log copy done
11,3056,101795851,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3057,102631555,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3058,102805110,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3059,103047098,-;init: starting service 'qspmhal'...
31,3060,103400604,-;logd: logdr: UID=1000 GID=1000 PID=3550 n tail=50 logMask=8 pid=3547 start=0ns timeout=0ns
31,3061,103410980,-;logd: logdr: UID=1000 GID=1000 PID=3550 n tail=50 logMask=1 pid=3547 start=0ns timeout=0ns
31,3062,103432859,-;logd: logdr: UID=1000 GID=1000 PID=3550 n tail=0 logMask=8 pid=3547 start=0ns timeout=0ns
31,3063,103447035,-;logd: logdr: UID=1000 GID=1000 PID=3550 n tail=0 logMask=1 pid=3547 start=0ns timeout=0ns
14,3064,103470843,-;init: Service 'qspmhal' (pid 3547) received signal 6
14,3065,103471077,-;init: Sending signal 9 to service 'qspmhal' (pid 3547) process group...
14,3066,103511544,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3547 in 39ms
14,3067,103517455,-;init: Untracked pid 3550 exited with status 0
14,3068,103518451,-;init: Untracked pid 3552 exited with status 0
3,3069,103591260,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3070,103596985,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3071,103605580,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3072,103611539,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3073,103618201,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3074,103623912,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3075,103631208,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3076,103633756,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3077,103636918,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3078,103661346,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3079,103667153,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3080,103684229,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3081,103691089,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3082,103724393,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3083,103730883,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3084,103741907,-;healthd: battery l=51 v=3778 t=30.8 h=2 st=2 c=-365295 fc=3812000 cc=0 chg=a
3,3085,103745322,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3086,103751157,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3087,103766904,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3088,103772911,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3089,106832036,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3090,107665213,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3091,107832797,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3092,108096097,-;init: starting service 'qspmhal'...
11,3093,108166443,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3094,108185767,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3095,108429739,-;logd: logdr: UID=1000 GID=1000 PID=3599 n tail=50 logMask=8 pid=3594 start=0ns timeout=0ns
31,3096,108440944,-;logd: logdr: UID=1000 GID=1000 PID=3599 n tail=50 logMask=1 pid=3594 start=0ns timeout=0ns
31,3097,108463212,-;logd: logdr: UID=1000 GID=1000 PID=3599 n tail=0 logMask=8 pid=3594 start=0ns timeout=0ns
31,3098,108477806,-;logd: logdr: UID=1000 GID=1000 PID=3599 n tail=0 logMask=1 pid=3594 start=0ns timeout=0ns
14,3099,108501121,-;init: Service 'qspmhal' (pid 3594) received signal 6
14,3100,108501192,-;init: Sending signal 9 to service 'qspmhal' (pid 3594) process group...
14,3101,108530695,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3594 in 29ms
14,3102,108535579,-;init: Untracked pid 3599 exited with status 0
3,3103,111751199,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3104,111756916,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3105,111767467,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3106,111778400,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3107,111785365,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3108,111791393,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3109,111798394,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3110,111804457,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3111,111812553,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3112,111818610,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3113,111834477,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3114,111840463,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3115,111886451,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3116,111892221,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3117,111902481,-;healthd: battery l=51 v=3757 t=30.7 h=2 st=2 c=-602570 fc=3812000 cc=0 chg=a
3,3118,111904071,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3119,111909848,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3120,111922842,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3121,111928600,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3122,112104928,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3123,112189942,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3124,112475904,-;init: Control message: Could not find 'vendor.qti.qspmhal@1.0::IQspmhal/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3125,112869172,-;IRQ 6: no longer affine to CPU4
11,3126,113096420,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3127,113135916,-;init: starting service 'qspmhal'...
11,3128,113193339,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3129,113408868,-;IRQ 6: no longer affine to CPU4
31,3130,113479426,-;logd: logdr: UID=1000 GID=1000 PID=3931 n tail=50 logMask=8 pid=3909 start=0ns timeout=0ns
31,3131,113492559,-;logd: logdr: UID=1000 GID=1000 PID=3931 n tail=50 logMask=1 pid=3909 start=0ns timeout=0ns
31,3132,113508813,-;logd: logdr: UID=1000 GID=1000 PID=3931 n tail=0 logMask=8 pid=3909 start=0ns timeout=0ns
31,3133,113518953,-;logd: logdr: UID=1000 GID=1000 PID=3931 n tail=0 logMask=1 pid=3909 start=0ns timeout=0ns
14,3134,113534614,-;init: Service 'qspmhal' (pid 3909) received signal 6
14,3135,113534709,-;init: Sending signal 9 to service 'qspmhal' (pid 3909) process group...
14,3136,113554408,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 3909 in 19ms
14,3137,113559442,-;init: Untracked pid 3935 received signal 9
6,3138,115188580,-;IRQ 6: no longer affine to CPU7
6,3139,115528685,-;IRQ 6: no longer affine to CPU6
6,3140,116328658,-;IRQ 6: no longer affine to CPU7
11,3141,117125552,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3142,117205755,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3143,118121317,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3144,118163317,-;init: starting service 'qspmhal'...
11,3145,118210816,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3146,118517493,-;logd: logdr: UID=1000 GID=1000 PID=4465 n tail=50 logMask=8 pid=4459 start=0ns timeout=0ns
31,3147,118523211,-;logd: logdr: UID=1000 GID=1000 PID=4465 n tail=50 logMask=1 pid=4459 start=0ns timeout=0ns
31,3148,118535282,-;logd: logdr: UID=1000 GID=1000 PID=4465 n tail=0 logMask=8 pid=4459 start=0ns timeout=0ns
31,3149,118541643,-;logd: logdr: UID=1000 GID=1000 PID=4465 n tail=0 logMask=1 pid=4459 start=0ns timeout=0ns
14,3150,118556832,-;init: Service 'qspmhal' (pid 4459) received signal 6
14,3151,118556930,-;init: Sending signal 9 to service 'qspmhal' (pid 4459) process group...
14,3152,118570531,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 4459 in 13ms
14,3153,118574029,-;init: Untracked pid 4465 exited with status 0
14,3154,118574333,-;init: Untracked pid 4473 received signal 9
3,3155,119913491,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3156,119919299,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3157,119928810,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3158,119934546,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3159,119941543,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3160,119947806,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3161,119956465,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3162,119962435,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3163,119969482,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3164,119975941,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3165,120027358,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3166,120033445,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3167,120071973,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3168,120078137,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3169,120090077,-;healthd: battery l=51 v=3744 t=30.8 h=2 st=2 c=-621338 fc=3812000 cc=0 chg=a
3,3170,120091966,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3171,120097653,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3172,120109020,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3173,120114709,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3174,122132658,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3175,122225026,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3176,123136233,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3177,123182239,-;init: starting service 'qspmhal'...
11,3178,123233458,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3179,123478427,-;logd: logdr: UID=1000 GID=1000 PID=4876 n tail=50 logMask=8 pid=4852 start=0ns timeout=0ns
31,3180,123498266,-;logd: logdr: UID=1000 GID=1000 PID=4876 n tail=50 logMask=1 pid=4852 start=0ns timeout=0ns
31,3181,123514998,-;logd: logdr: UID=1000 GID=1000 PID=4876 n tail=0 logMask=8 pid=4852 start=0ns timeout=0ns
31,3182,123526318,-;logd: logdr: UID=1000 GID=1000 PID=4876 n tail=0 logMask=1 pid=4852 start=0ns timeout=0ns
14,3183,123544607,-;init: Service 'qspmhal' (pid 4852) received signal 6
14,3184,123544681,-;init: Sending signal 9 to service 'qspmhal' (pid 4852) process group...
14,3185,123562811,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 4852 in 17ms
14,3186,123567188,-;init: Untracked pid 4876 exited with status 0
14,3187,123567596,-;init: Untracked pid 4879 received signal 9
11,3188,127149654,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3189,127245177,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3190,128075453,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3191,128082689,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3192,128091141,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3193,128097003,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3194,128103692,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3195,128109771,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3196,128117466,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3197,128123837,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3198,128131478,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3199,128137190,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3200,128155673,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3201,128159310,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3202,128175883,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,3203,128207695,-;init: starting service 'qspmhal'...
3,3204,128207910,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3205,128213690,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3206,128221977,-;healthd: battery l=51 v=3738 t=30.9 h=2 st=2 c=-692291 fc=3812000 cc=0 chg=a
3,3207,128223885,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3208,128229811,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3209,128248457,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3210,128254220,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3211,128270138,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,3212,128470199,-;logd: logdr: UID=1000 GID=1000 PID=5274 n tail=50 logMask=8 pid=5268 start=0ns timeout=0ns
31,3213,128477833,-;logd: logdr: UID=1000 GID=1000 PID=5274 n tail=50 logMask=1 pid=5268 start=0ns timeout=0ns
31,3214,128507565,-;logd: logdr: UID=1000 GID=1000 PID=5274 n tail=0 logMask=8 pid=5268 start=0ns timeout=0ns
31,3215,128513270,-;logd: logdr: UID=1000 GID=1000 PID=5274 n tail=0 logMask=1 pid=5268 start=0ns timeout=0ns
14,3216,128526106,-;init: Service 'qspmhal' (pid 5268) received signal 6
14,3217,128526145,-;init: Sending signal 9 to service 'qspmhal' (pid 5268) process group...
14,3218,128538993,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 5268 in 12ms
14,3219,128542421,-;init: Untracked pid 5274 exited with status 0
14,3220,128542822,-;init: Untracked pid 5276 received signal 9
6,3221,128848302,-;IRQ 6: no longer affine to CPU5
14,3222,129146153,-;rmt_storage:INFO:rmt_storage_rw_iovec_cb: Write iovec request (req_h 0x7 wr_count 1) received for /boot/modem_fs1
14,3223,129153127,-;rmt_storage:INFO:rmt_storage_client_thread: Calling Write [offset=0, size=1572864, req_h 0x7, wr_count 1] for /boot/modem_fs1!
14,3224,129190275,-;rmt_storage:INFO:rmt_storage_client_thread: Done Write (bytes = 1572864, req_h 0x7, wr_count 1) for /boot/modem_fs1!
11,3225,132174803,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3226,132904296,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3227,133184335,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3228,133227104,-;init: starting service 'qspmhal'...
3,3229,133416574,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
31,3230,133525881,-;logd: logdr: UID=1000 GID=1000 PID=5644 n tail=50 logMask=8 pid=5637 start=0ns timeout=0ns
31,3231,133536399,-;logd: logdr: UID=1000 GID=1000 PID=5644 n tail=50 logMask=1 pid=5637 start=0ns timeout=0ns
31,3232,133554891,-;logd: logdr: UID=1000 GID=1000 PID=5644 n tail=0 logMask=8 pid=5637 start=0ns timeout=0ns
31,3233,133565049,-;logd: logdr: UID=1000 GID=1000 PID=5644 n tail=0 logMask=1 pid=5637 start=0ns timeout=0ns
14,3234,133584081,-;init: Untracked pid 5644 exited with status 0
14,3235,133587880,-;init: Service 'qspmhal' (pid 5637) received signal 6
14,3236,133589614,-;init: Sending signal 9 to service 'qspmhal' (pid 5637) process group...
14,3237,133614437,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 5637 in 23ms
14,3238,133620904,-;init: Untracked pid 5646 exited with status 0
11,3239,133907974,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3240,136238006,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3241,136244244,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3242,136253362,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3243,136261232,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3244,136266943,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3245,136273377,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3246,136280008,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3247,136285727,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3248,136293765,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3249,136299671,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3250,136313959,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3251,136319697,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3252,136367521,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3253,136373292,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3254,136381408,-;healthd: battery l=51 v=3761 t=30.7 h=2 st=2 c=-430145 fc=3812000 cc=0 chg=a
3,3255,136383319,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3256,136389059,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3257,136401881,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3258,136407570,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3259,137207664,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3260,137930450,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3261,138214171,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3262,138273926,-;init: starting service 'qspmhal'...
31,3263,138583803,-;logd: logdr: UID=1000 GID=1000 PID=5967 n tail=50 logMask=8 pid=5962 start=0ns timeout=0ns
31,3264,138590521,-;logd: logdr: UID=1000 GID=1000 PID=5967 n tail=50 logMask=1 pid=5962 start=0ns timeout=0ns
31,3265,138610220,-;logd: logdr: UID=1000 GID=1000 PID=5967 n tail=0 logMask=8 pid=5962 start=0ns timeout=0ns
31,3266,138622010,-;logd: logdr: UID=1000 GID=1000 PID=5967 n tail=0 logMask=1 pid=5962 start=0ns timeout=0ns
14,3267,138641290,-;init: Untracked pid 5967 exited with status 0
14,3268,138651240,-;init: Service 'qspmhal' (pid 5962) received signal 6
14,3269,138651412,-;init: Sending signal 9 to service 'qspmhal' (pid 5962) process group...
14,3270,138666859,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 5962 in 14ms
14,3271,138673732,-;init: Untracked pid 5969 exited with status 0
11,3272,138945158,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3273,141876014,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3274,141882820,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3275,142232754,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3276,142970141,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3277,143239747,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3278,143322251,-;init: starting service 'qspmhal'...
31,3279,143658458,-;logd: logdr: UID=1000 GID=1000 PID=6276 n tail=50 logMask=8 pid=6261 start=0ns timeout=0ns
31,3280,143666967,-;logd: logdr: UID=1000 GID=1000 PID=6276 n tail=50 logMask=1 pid=6261 start=0ns timeout=0ns
31,3281,143680879,-;logd: logdr: UID=1000 GID=1000 PID=6276 n tail=0 logMask=8 pid=6261 start=0ns timeout=0ns
31,3282,143689426,-;logd: logdr: UID=1000 GID=1000 PID=6276 n tail=0 logMask=1 pid=6261 start=0ns timeout=0ns
14,3283,143708874,-;init: Service 'qspmhal' (pid 6261) received signal 6
14,3284,143709000,-;init: Sending signal 9 to service 'qspmhal' (pid 6261) process group...
14,3285,143728604,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 6261 in 19ms
14,3286,143733993,-;init: Untracked pid 6287 received signal 9
14,3287,143734425,-;init: Untracked pid 6276 exited with status 0
11,3288,143981571,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3289,144403449,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3290,144410036,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3291,144419620,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3292,144426127,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3293,144433046,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3294,144439262,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3295,144446384,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3296,144452371,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3297,144459762,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3298,144465515,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3299,144483618,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3300,144489575,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3301,144533129,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3302,144538893,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3303,144547380,-;healthd: battery l=51 v=3802 t=30.7 h=2 st=2 c=-321350 fc=3812000 cc=0 chg=a
3,3304,144548933,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3305,144554623,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3306,144566537,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3307,144572304,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3308,147257108,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3309,148009616,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3310,148265273,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3311,148348548,-;init: starting service 'qspmhal'...
31,3312,148665040,-;logd: logdr: UID=1000 GID=1000 PID=6599 n tail=50 logMask=8 pid=6590 start=0ns timeout=0ns
31,3313,148675824,-;logd: logdr: UID=1000 GID=1000 PID=6599 n tail=50 logMask=1 pid=6590 start=0ns timeout=0ns
31,3314,148695368,-;logd: logdr: UID=1000 GID=1000 PID=6599 n tail=0 logMask=8 pid=6590 start=0ns timeout=0ns
31,3315,148705315,-;logd: logdr: UID=1000 GID=1000 PID=6599 n tail=0 logMask=1 pid=6590 start=0ns timeout=0ns
14,3316,148725265,-;init: Service 'qspmhal' (pid 6590) received signal 6
14,3317,148725379,-;init: Sending signal 9 to service 'qspmhal' (pid 6590) process group...
14,3318,148745635,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 6590 in 19ms
14,3319,148751621,-;init: Untracked pid 6599 exited with status 0
14,3320,148752153,-;init: Untracked pid 6615 received signal 9
11,3321,149010634,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3322,151300191,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3323,151305904,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3324,151319365,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3325,151325070,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3326,151333763,-;healthd: battery l=51 v=3802 t=30.6 h=2 st=2 c=-379486 fc=3812000 cc=0 chg=a
3,3327,151337139,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3328,151343017,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3329,151356106,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3330,151361959,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3331,152262952,-;init: Control message: Could not find 'vendor.qti.qspmhal@1.0::IQspmhal/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3332,152299772,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3333,152333258,-;tas2563 0-004c: tas2563_hw_params, format: 2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3334,152333270,-;tas2563 0-004c: tas2563_set_bitwidth 1565
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,3335,152333721,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
11,3336,152357451,-;init: Control message: Could not find 'vendor.qti.qspmhal@1.0::IQspmhal/default' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
7,3337,152372417,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:8, mask: 0xc, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3338,152372428,-;tas2563 0-004c: mnCh_size: 16
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3339,152372436,-;tas2563 0-004c: blr_clk_ratio: 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3340,152373144,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3341,152373775,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x44
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3342,152373787,-;tas2563 0-004c: tas2563_hw_params, sample rate: 48000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3343,152374186,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:6, mask: 0x20, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3344,152374593,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:6, mask: 0xe, val: 0x8
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3345,152375946,-;__afe_port_start: port id: 0x1002
6,3346,152375965,-;afe_find_cal_topo_id_by_port: port id: 0x1002, dev_acdb_id: 0
6,3347,152375973,-;afe_find_cal_topo_id_by_port: top_id:112fc acdb_id:15 afe_port:0x1002
6,3348,152375981,-;afe_get_cal_topology_id: port_id = 0x1002 acdb_id = 15 topology_id = 0x112fc cal_type_index=8 ret=0
6,3349,152376362,-;afe_send_port_topology_id: AFE set topology id 0x112fc  enable for port 0x1002 ret 0
6,3350,152376370,-;send_afe_cal_type: cal_index is 0
6,3351,152376378,-;send_afe_cal_type: dev_acdb_id[36] is 0
6,3352,152376386,-;send_afe_cal_type: Sending cal_index cal 0
3,3353,152376394,-;send_afe_cal_type: No cal sent for cal_index 0, port_id = 0x1002! ret -22
6,3354,152384809,-;afe_send_hw_delay: port_id 0x1002 rate 48000 delay_usec 474 status 0
6,3355,152389198,-;tas2563 0-004c: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3356,152389209,-;tas2563 0-004c: unmute: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3357,152389217,-;tas2563 0-004c: set power state: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3358,152389225,-;tas2563 0-004c: tas2563_set_power_state, state: 0, mbPowerup 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3359,152390051,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:2, mask: 0xf, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3360,152390061,-;tas2563 0-004c: tas2563_set_power_state  channel is 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3361,152390639,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:48, mask: 0x4, val: 0x4
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3362,152488177,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3363,152488451,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3364,152488723,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3365,152489068,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3366,152498165,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3367,152498422,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3368,152498709,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3369,152498990,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,3370,152562662,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3371,152563172,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3372,152569286,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3373,152593092,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3374,152599737,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3375,152607816,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3376,152614080,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3377,152626425,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3378,152633952,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3379,152640872,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3380,152647520,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3381,152665088,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3382,152673201,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3383,152720072,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3384,152725766,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3385,152734021,-;healthd: battery l=51 v=3705 t=30.8 h=2 st=2 c=-903473 fc=3812000 cc=0 chg=a
3,3386,152735173,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3387,152740983,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3388,152752389,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3389,152758126,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3390,153307936,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3391,153373972,-;init: starting service 'qspmhal'...
11,3392,153562830,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3393,153610047,-;logd: logdr: UID=1000 GID=1000 PID=7003 n tail=50 logMask=8 pid=6991 start=0ns timeout=0ns
31,3394,153617484,-;logd: logdr: UID=1000 GID=1000 PID=7003 n tail=50 logMask=1 pid=6991 start=0ns timeout=0ns
31,3395,153635955,-;logd: logdr: UID=1000 GID=1000 PID=7003 n tail=0 logMask=8 pid=6991 start=0ns timeout=0ns
31,3396,153643888,-;logd: logdr: UID=1000 GID=1000 PID=7003 n tail=0 logMask=1 pid=6991 start=0ns timeout=0ns
14,3397,153659054,-;init: Service 'qspmhal' (pid 6991) received signal 6
14,3398,153659096,-;init: Sending signal 9 to service 'qspmhal' (pid 6991) process group...
14,3399,153677523,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 6991 in 18ms
6,3400,155735134,-;tas2563 0-004c: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3401,155735153,-;tas2563 0-004c: mute: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3402,155735169,-;tas2563 0-004c: set power state: 2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3403,155735183,-;tas2563 0-004c: tas2563_set_power_state, state: 2, mbPowerup 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,3404,155736894,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,3405,155770699,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:2, mask: 0x3, val: 0x2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3406,155810108,-;afe_close: port_id = 0x1002
6,3407,156154137,-;tas2563 0-004c: tas2563_hw_params, format: 2
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3408,156154152,-;tas2563 0-004c: tas2563_set_bitwidth 1565
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,3409,156156357,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,3410,156189035,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:8, mask: 0xc, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3411,156189047,-;tas2563 0-004c: mnCh_size: 16
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3412,156189056,-;tas2563 0-004c: blr_clk_ratio: 32
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3413,156189700,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x40
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3414,156190360,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:12, mask: 0xff, val: 0x44
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3415,156190383,-;tas2563 0-004c: tas2563_hw_params, sample rate: 48000
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3416,156190902,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:6, mask: 0x20, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3417,156191649,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:6, mask: 0xe, val: 0x8
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3418,156194091,-;__afe_port_start: port id: 0x1002
6,3419,156194124,-;afe_find_cal_topo_id_by_port: port id: 0x1002, dev_acdb_id: 0
6,3420,156194143,-;afe_find_cal_topo_id_by_port: top_id:112fc acdb_id:15 afe_port:0x1002
6,3421,156194162,-;afe_get_cal_topology_id: port_id = 0x1002 acdb_id = 15 topology_id = 0x112fc cal_type_index=8 ret=0
6,3422,156194571,-;afe_send_port_topology_id: AFE set topology id 0x112fc  enable for port 0x1002 ret 0
6,3423,156194597,-;send_afe_cal_type: cal_index is 0
6,3424,156194616,-;send_afe_cal_type: dev_acdb_id[36] is 0
6,3425,156194634,-;send_afe_cal_type: Sending cal_index cal 0
3,3426,156194652,-;send_afe_cal_type: No cal sent for cal_index 0, port_id = 0x1002! ret -22
6,3427,156203243,-;afe_send_hw_delay: port_id 0x1002 rate 48000 delay_usec 474 status 0
6,3428,156208235,-;tas2563 0-004c: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3429,156208254,-;tas2563 0-004c: unmute: tas2563_mute
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3430,156208270,-;tas2563 0-004c: set power state: 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3431,156208285,-;tas2563 0-004c: tas2563_set_power_state, state: 0, mbPowerup 0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3432,156208971,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:2, mask: 0xf, val: 0x0
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3433,156208982,-;tas2563 0-004c: tas2563_set_power_state  channel is 1
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3434,156209666,-;tas2563 0-004c: tas2563_dev_update_bits: chn4c:BOOK:PAGE:REG 0:0:48, mask: 0x4, val: 0x4
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3435,156308719,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3436,156309069,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3437,156309575,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3438,156310464,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3439,156319233,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3440,156319528,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3441,156319809,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3442,156320115,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3443,156588663,-;IRQ 6: no longer affine to CPU7
11,3444,157323846,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3445,157429025,-;IRQ 6: no longer affine to CPU7
11,3446,157583541,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3447,158328428,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3448,158391701,-;init: starting service 'qspmhal'...
11,3449,158591376,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3450,158721883,-;logd: logdr: UID=1000 GID=1000 PID=7363 n tail=50 logMask=8 pid=7342 start=0ns timeout=0ns
31,3451,158729130,-;logd: logdr: UID=1000 GID=1000 PID=7363 n tail=50 logMask=1 pid=7342 start=0ns timeout=0ns
31,3452,158744263,-;logd: logdr: UID=1000 GID=1000 PID=7363 n tail=0 logMask=8 pid=7342 start=0ns timeout=0ns
31,3453,158759854,-;logd: logdr: UID=1000 GID=1000 PID=7363 n tail=0 logMask=1 pid=7342 start=0ns timeout=0ns
14,3454,158779326,-;init: Untracked pid 7363 exited with status 0
14,3455,158779965,-;init: Service 'qspmhal' (pid 7342) received signal 6
14,3456,158780031,-;init: Sending signal 9 to service 'qspmhal' (pid 7342) process group...
14,3457,158806280,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 7342 in 25ms
14,3458,158811032,-;init: Untracked pid 7368 exited with status 0
3,3459,160726222,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3460,160732312,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3461,160742963,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3462,160749256,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3463,160757127,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3464,160763731,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3465,160771265,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3466,160777049,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3467,160784508,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3468,160790956,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3469,160815781,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3470,160821586,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3471,160859303,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3472,160864993,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3473,160873261,-;healthd: battery l=51 v=3730 t=31.1 h=2 st=2 c=-783386 fc=3812000 cc=0 chg=a
3,3474,160874464,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3475,160880220,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3476,160900282,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3477,160905979,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3478,162353741,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3479,162607348,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3480,163355311,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3481,163420472,-;init: starting service 'qspmhal'...
11,3482,163612729,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3483,163758462,-;logd: logdr: UID=1000 GID=1000 PID=7687 n tail=50 logMask=8 pid=7661 start=0ns timeout=0ns
31,3484,163770560,-;logd: logdr: UID=1000 GID=1000 PID=7687 n tail=50 logMask=1 pid=7661 start=0ns timeout=0ns
31,3485,163789817,-;logd: logdr: UID=1000 GID=1000 PID=7687 n tail=0 logMask=8 pid=7661 start=0ns timeout=0ns
31,3486,163800567,-;logd: logdr: UID=1000 GID=1000 PID=7687 n tail=0 logMask=1 pid=7661 start=0ns timeout=0ns
14,3487,163816987,-;init: Service 'qspmhal' (pid 7661) received signal 6
14,3488,163817065,-;init: Sending signal 9 to service 'qspmhal' (pid 7661) process group...
14,3489,163832818,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 7661 in 12ms
14,3490,163836535,-;init: Untracked pid 7687 exited with status 0
14,3491,163836953,-;init: Untracked pid 7691 received signal 9
11,3492,167381548,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3493,167635584,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3494,168383316,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3495,168446024,-;init: starting service 'qspmhal'...
11,3496,168641330,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3497,168797202,-;logd: logdr: UID=1000 GID=1000 PID=8021 n tail=50 logMask=8 pid=7996 start=0ns timeout=0ns
31,3498,168816908,-;logd: logdr: UID=1000 GID=1000 PID=8021 n tail=50 logMask=1 pid=7996 start=0ns timeout=0ns
31,3499,168844371,-;logd: logdr: UID=1000 GID=1000 PID=8021 n tail=0 logMask=8 pid=7996 start=0ns timeout=0ns
31,3500,168855027,-;logd: logdr: UID=1000 GID=1000 PID=8021 n tail=0 logMask=1 pid=7996 start=0ns timeout=0ns
14,3501,168896784,-;init: Service 'qspmhal' (pid 7996) received signal 6
14,3502,168896935,-;init: Sending signal 9 to service 'qspmhal' (pid 7996) process group...
3,3503,168898230,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,3504,168904517,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 7996 in 7ms
3,3505,168905875,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,3506,168908676,-;init: Untracked pid 8021 exited with status 0
14,3507,168912639,-;init: Untracked pid 8025 exited with status 0
3,3508,168914825,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3509,168920893,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3510,168927508,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3511,168934387,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3512,168941357,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3513,168947104,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3514,168954550,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3515,168960666,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3516,168992521,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3517,168998744,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3518,169043853,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3519,169050355,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3520,169063353,-;healthd: battery l=51 v=3687 t=31.2 h=2 st=2 c=-1210480 fc=3812000 cc=0 chg=a
3,3521,169065751,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3522,169071651,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3523,169088571,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3524,169094683,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,3525,172229047,-;IRQ 6: no longer affine to CPU7
11,3526,172405887,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3527,173221571,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3528,173416892,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3529,173482044,-;init: starting service 'qspmhal'...
31,3530,173819475,-;logd: logdr: UID=1000 GID=1000 PID=8369 n tail=50 logMask=8 pid=8366 start=0ns timeout=0ns
31,3531,173830542,-;logd: logdr: UID=1000 GID=1000 PID=8369 n tail=50 logMask=1 pid=8366 start=0ns timeout=0ns
31,3532,173849777,-;logd: logdr: UID=1000 GID=1000 PID=8369 n tail=0 logMask=8 pid=8366 start=0ns timeout=0ns
31,3533,173867322,-;logd: logdr: UID=1000 GID=1000 PID=8369 n tail=0 logMask=1 pid=8366 start=0ns timeout=0ns
14,3534,173886513,-;init: Service 'qspmhal' (pid 8366) received signal 6
14,3535,173886589,-;init: Sending signal 9 to service 'qspmhal' (pid 8366) process group...
14,3536,173916972,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 8366 in 30ms
14,3537,173923174,-;init: Untracked pid 8369 exited with status 0
14,3538,173923694,-;init: Untracked pid 8377 received signal 9
11,3539,174228452,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3540,175815326,-;perf: interrupt took too long (2509 > 2500), lowering kernel.perf_event_max_sample_rate to 79700
3,3541,177052279,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3542,177058002,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3543,177069881,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3544,177075946,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3545,177082718,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3546,177088692,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3547,177095811,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3548,177102944,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3549,177110735,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3550,177116536,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3551,177136604,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3552,177148733,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3553,177205713,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3554,177211479,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3555,177219703,-;healthd: battery l=51 v=3694 t=31.5 h=2 st=2 c=-920258 fc=3812000 cc=0 chg=a
3,3556,177221101,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3557,177226837,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3558,177238901,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3559,177244602,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3560,177445861,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3561,178249762,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3562,178458283,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3563,178520159,-;init: starting service 'qspmhal'...
6,3564,178828486,-;IRQ 6: no longer affine to CPU7
31,3565,178845716,-;logd: logdr: UID=1000 GID=1000 PID=8734 n tail=50 logMask=8 pid=8720 start=0ns timeout=0ns
31,3566,178873091,-;logd: logdr: UID=1000 GID=1000 PID=8734 n tail=50 logMask=1 pid=8720 start=0ns timeout=0ns
31,3567,178886157,-;logd: logdr: UID=1000 GID=1000 PID=8734 n tail=0 logMask=8 pid=8720 start=0ns timeout=0ns
31,3568,178901577,-;logd: logdr: UID=1000 GID=1000 PID=8734 n tail=0 logMask=1 pid=8720 start=0ns timeout=0ns
14,3569,178915382,-;init: Service 'qspmhal' (pid 8720) received signal 6
14,3570,178915441,-;init: Sending signal 9 to service 'qspmhal' (pid 8720) process group...
14,3571,178932963,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 8720 in 17ms
14,3572,178935077,-;init: Untracked pid 8734 exited with status 0
14,3573,178935233,-;init: Untracked pid 8750 received signal 9
11,3574,179256602,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3575,179428939,-;IRQ 6: no longer affine to CPU7
6,3576,181968284,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,3577,181968996,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,3578,181998870,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3579,181999180,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3580,181999452,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3581,182008347,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3582,182008809,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3583,182009671,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3584,182011395,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3585,182029639,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3586,182030151,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3587,182030778,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3588,182031226,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3589,182269040,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3590,182269858,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3591,182271238,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3592,182271683,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3593,182283157,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3594,182284044,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3595,182284848,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3596,182285591,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
11,3597,183271703,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3598,183401711,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3599,183558164,-;init: starting service 'qspmhal'...
31,3600,183943556,-;logd: logdr: UID=1000 GID=1000 PID=9113 n tail=50 logMask=8 pid=9104 start=0ns timeout=0ns
31,3601,183968796,-;logd: logdr: UID=1000 GID=1000 PID=9113 n tail=50 logMask=1 pid=9104 start=0ns timeout=0ns
31,3602,183983205,-;logd: logdr: UID=1000 GID=1000 PID=9113 n tail=0 logMask=8 pid=9104 start=0ns timeout=0ns
31,3603,183991263,-;logd: logdr: UID=1000 GID=1000 PID=9113 n tail=0 logMask=1 pid=9104 start=0ns timeout=0ns
14,3604,184008674,-;init: Service 'qspmhal' (pid 9104) received signal 6
14,3605,184008787,-;init: Sending signal 9 to service 'qspmhal' (pid 9104) process group...
14,3606,184036383,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 9104 in 27ms
14,3607,184039714,-;init: Untracked pid 9127 received signal 9
14,3608,184040122,-;init: Untracked pid 9113 exited with status 0
11,3609,184276670,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3610,184403432,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3611,185217878,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3612,185227879,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3613,185239637,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3614,185245691,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3615,185254318,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3616,185260543,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3617,185270833,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3618,185276622,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3619,185284176,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3620,185290204,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3621,185309511,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3622,185315226,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3623,185326359,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3624,185332112,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3625,185340330,-;healthd: battery l=51 v=3723 t=31.4 h=2 st=2 c=-854492 fc=3812000 cc=0 chg=a
3,3626,185341416,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3627,185347095,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3628,185387421,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3629,185393184,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3630,188298917,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3631,188440176,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3632,188599205,-;init: starting service 'qspmhal'...
31,3633,188925720,-;logd: logdr: UID=1000 GID=1000 PID=9442 n tail=50 logMask=8 pid=9439 start=0ns timeout=0ns
31,3634,188937646,-;logd: logdr: UID=1000 GID=1000 PID=9442 n tail=50 logMask=1 pid=9439 start=0ns timeout=0ns
31,3635,188951727,-;logd: logdr: UID=1000 GID=1000 PID=9442 n tail=0 logMask=8 pid=9439 start=0ns timeout=0ns
31,3636,188961051,-;logd: logdr: UID=1000 GID=1000 PID=9442 n tail=0 logMask=1 pid=9439 start=0ns timeout=0ns
14,3637,188981534,-;init: Service 'qspmhal' (pid 9439) received signal 6
14,3638,188981642,-;init: Sending signal 9 to service 'qspmhal' (pid 9439) process group...
14,3639,188995546,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 9439 in 13ms
14,3640,188999950,-;init: Untracked pid 9442 exited with status 0
14,3641,189002062,-;init: Untracked pid 9444 received signal 9
11,3642,189304715,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3643,189449127,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3644,190429118,-;IRQ 6: no longer affine to CPU7
3,3645,193383182,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3646,193389563,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3647,193401588,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3648,193408880,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3649,193415754,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3650,193421751,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3651,193429933,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3652,193435737,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3653,193445136,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3654,193450975,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3655,193470128,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3656,193481618,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3657,193492214,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3658,193535156,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3659,193541772,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3660,193554552,-;healthd: battery l=51 v=3689 t=31.6 h=2 st=2 c=-900574 fc=3812000 cc=0 chg=a
3,3661,193559173,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3662,193565005,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3663,193579832,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3664,193585556,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,3665,193634585,-;init: starting service 'qspmhal'...
11,3666,193884894,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3667,193947774,-;logd: logdr: UID=1000 GID=1000 PID=9788 n tail=50 logMask=8 pid=9784 start=0ns timeout=0ns
31,3668,193962143,-;logd: logdr: UID=1000 GID=1000 PID=9788 n tail=50 logMask=1 pid=9784 start=0ns timeout=0ns
31,3669,193986742,-;logd: logdr: UID=1000 GID=1000 PID=9788 n tail=0 logMask=8 pid=9784 start=0ns timeout=0ns
31,3670,193999268,-;logd: logdr: UID=1000 GID=1000 PID=9788 n tail=0 logMask=1 pid=9784 start=0ns timeout=0ns
14,3671,194022965,-;init: Untracked pid 9788 exited with status 0
14,3672,194029726,-;init: Service 'qspmhal' (pid 9784) received signal 6
14,3673,194029824,-;init: Sending signal 9 to service 'qspmhal' (pid 9784) process group...
14,3674,194042696,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 9784 in 12ms
14,3675,194046942,-;init: Untracked pid 9790 exited with status 0
11,3676,194474205,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3677,194731767,-;init: starting service 'qvrd'...
11,3678,198510048,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,3679,198588982,-;IRQ 6: no longer affine to CPU7
14,3680,198669412,-;init: starting service 'qspmhal'...
11,3681,198906441,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3682,198986370,-;logd: logdr: UID=1000 GID=1000 PID=10124 n tail=50 logMask=8 pid=10121 start=0ns timeout=0ns
31,3683,198999803,-;logd: logdr: UID=1000 GID=1000 PID=10124 n tail=50 logMask=1 pid=10121 start=0ns timeout=0ns
31,3684,199012482,-;logd: logdr: UID=1000 GID=1000 PID=10124 n tail=0 logMask=8 pid=10121 start=0ns timeout=0ns
31,3685,199019068,-;logd: logdr: UID=1000 GID=1000 PID=10124 n tail=0 logMask=1 pid=10121 start=0ns timeout=0ns
14,3686,199036004,-;init: Service 'qspmhal' (pid 10121) received signal 6
14,3687,199036048,-;init: Sending signal 9 to service 'qspmhal' (pid 10121) process group...
14,3688,199047872,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 10121 in 11ms
14,3689,199050639,-;init: Untracked pid 10124 exited with status 0
14,3690,199050788,-;init: Untracked pid 10126 received signal 9
11,3691,199513105,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3692,199765868,-;init: starting service 'qvrd'...
3,3693,201548336,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3694,201554093,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3695,201567942,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3696,201574742,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3697,201581666,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3698,201587486,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3699,201595072,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3700,201601055,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3701,201608243,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3702,201614065,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3703,201645715,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3704,201651477,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3705,201666642,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3706,201672705,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3707,201681077,-;healthd: battery l=51 v=3736 t=31.4 h=2 st=2 c=-517731 fc=3812000 cc=0 chg=a
3,3708,201682268,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3709,201687952,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3710,201698571,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3711,201704265,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,3712,202901700,-;[soft_i][0xfc7c63a2][21:05:37.395134] wlan: [0:I:QDF] DHCP-R TX: SA:3e:fd:55:14:24:bf DA:94:de:80:a9:0e:ae msdu_id:1197 status: succ
6,3713,202904252,-;[cds_ol][0xfc7d22b3][21:05:37.397682] wlan: [1659:I:QDF] DHCP-A RX: SA:f0:7f:06:cc:c0:40 DA:3e:fd:55:14:24:bf
11,3714,203534642,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3715,203701905,-;init: starting service 'qspmhal'...
11,3716,203936182,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3717,204031731,-;logd: logdr: UID=1000 GID=1000 PID=10463 n tail=50 logMask=8 pid=10439 start=0ns timeout=0ns
31,3718,204038415,-;logd: logdr: UID=1000 GID=1000 PID=10463 n tail=50 logMask=1 pid=10439 start=0ns timeout=0ns
31,3719,204054622,-;logd: logdr: UID=1000 GID=1000 PID=10463 n tail=0 logMask=8 pid=10439 start=0ns timeout=0ns
31,3720,204064697,-;logd: logdr: UID=1000 GID=1000 PID=10463 n tail=0 logMask=1 pid=10439 start=0ns timeout=0ns
14,3721,204082835,-;init: Service 'qspmhal' (pid 10439) received signal 6
14,3722,204082902,-;init: Sending signal 9 to service 'qspmhal' (pid 10439) process group...
14,3723,204106728,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 10439 in 23ms
14,3724,204113990,-;init: Untracked pid 10463 exited with status 0
14,3725,204114596,-;init: Untracked pid 10465 received signal 9
11,3726,204542709,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3727,204822872,-;init: starting service 'qvrd'...
6,3728,205008905,-;IRQ 6: no longer affine to CPU7
3,3729,205780110,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3730,205786936,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3731,205808950,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3732,205814815,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3733,205823076,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3734,205829071,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3735,205837533,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3736,205845741,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3737,205851861,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3738,205860344,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3739,205864387,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3740,205866046,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3741,205882166,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3742,205887873,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3743,205894619,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3744,205900854,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3745,205901755,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3746,205906701,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3747,205925833,-;healthd: battery l=51 v=3747 t=31.4 h=2 st=2 c=-651550 fc=3812000 cc=0 chg=a
3,3748,205927672,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3749,205933801,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3750,205967948,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,3751,205968705,-;IRQ 6: no longer affine to CPU5
3,3752,205973763,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3753,205986445,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3754,205992603,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3755,206007120,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3756,206012893,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3757,206021539,-;healthd: battery l=51 v=3743 t=31.3 h=2 st=2 c=-718384 fc=3812000 cc=0 chg=a
3,3758,206023466,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3759,206029258,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3760,206041639,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3761,206047328,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3762,207115333,-;q6asm_callback: cmd = 0x10bce returned error = 0xa
3,3763,207121568,-;__q6asm_cmd: DSP returned error[ADSP_ENOTREADY] opcode 68558
11,3764,208560387,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3765,208743180,-;init: starting service 'qspmhal'...
11,3766,208971221,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3767,209105248,-;logd: logdr: UID=1000 GID=1000 PID=10805 n tail=50 logMask=8 pid=10786 start=0ns timeout=0ns
31,3768,209115703,-;logd: logdr: UID=1000 GID=1000 PID=10805 n tail=50 logMask=1 pid=10786 start=0ns timeout=0ns
31,3769,209128608,-;logd: logdr: UID=1000 GID=1000 PID=10805 n tail=0 logMask=8 pid=10786 start=0ns timeout=0ns
31,3770,209136315,-;logd: logdr: UID=1000 GID=1000 PID=10805 n tail=0 logMask=1 pid=10786 start=0ns timeout=0ns
14,3771,209152052,-;init: Service 'qspmhal' (pid 10786) received signal 6
14,3772,209152118,-;init: Sending signal 9 to service 'qspmhal' (pid 10786) process group...
14,3773,209176427,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 10786 in 23ms
14,3774,209181704,-;init: Untracked pid 10805 exited with status 0
14,3775,209182105,-;init: Untracked pid 10809 received signal 9
11,3776,209569236,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3777,209711734,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3778,209717879,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3779,209727153,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3780,209735280,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3781,209742854,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3782,209749374,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3783,209757765,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3784,209764161,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3785,209770850,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3786,209776918,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3787,209796300,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3788,209804271,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3789,209841826,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3790,209847514,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3791,209857013,-;healthd: battery l=51 v=3754 t=31.3 h=2 st=2 c=-616760 fc=3812000 cc=0 chg=a
3,3792,209858933,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,3793,209860409,-;init: starting service 'qvrd'...
3,3794,209864644,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3795,209878136,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3796,209883831,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3797,211298546,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3798,211304237,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3799,211316365,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3800,211325983,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3801,211334238,-;healthd: battery l=51 v=3676 t=31.7 h=2 st=2 c=-1109772 fc=3812000 cc=0 chg=a
3,3802,211336785,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3803,211342614,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3804,211353455,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3805,211359206,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3806,213586545,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3807,213799599,-;init: starting service 'qspmhal'...
31,3808,214106168,-;logd: logdr: UID=1000 GID=1000 PID=11154 n tail=50 logMask=8 pid=11149 start=0ns timeout=0ns
31,3809,214122334,-;logd: logdr: UID=1000 GID=1000 PID=11154 n tail=50 logMask=1 pid=11149 start=0ns timeout=0ns
31,3810,214152189,-;logd: logdr: UID=1000 GID=1000 PID=11154 n tail=0 logMask=8 pid=11149 start=0ns timeout=0ns
31,3811,214165344,-;logd: logdr: UID=1000 GID=1000 PID=11154 n tail=0 logMask=1 pid=11149 start=0ns timeout=0ns
14,3812,214184326,-;init: Service 'qspmhal' (pid 11149) received signal 6
14,3813,214184405,-;init: Sending signal 9 to service 'qspmhal' (pid 11149) process group...
14,3814,214202701,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 11149 in 17ms
14,3815,214207018,-;init: Untracked pid 11154 exited with status 0
14,3816,214207543,-;init: Untracked pid 11156 received signal 9
11,3817,214539276,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3818,214593233,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3819,214902742,-;init: starting service 'qvrd'...
3,3820,217877796,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3821,217884214,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3822,217893572,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3823,217901450,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3824,217901602,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3825,217914936,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3826,217922047,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3827,217927817,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3828,217936685,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3829,217944727,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3830,217957494,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3831,217963277,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3832,217999643,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3833,218005338,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3834,218014919,-;healthd: battery l=51 v=3703 t=31.5 h=2 st=2 c=-850983 fc=3812000 cc=0 chg=a
3,3835,218016364,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3836,218022230,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3837,218044994,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3838,218050785,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,3839,218129349,-;IRQ 6: no longer affine to CPU7
11,3840,218619117,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3841,218842319,-;init: starting service 'qspmhal'...
31,3842,219146536,-;logd: logdr: UID=1000 GID=1000 PID=11479 n tail=50 logMask=8 pid=11474 start=0ns timeout=0ns
31,3843,219159277,-;logd: logdr: UID=1000 GID=1000 PID=11479 n tail=50 logMask=1 pid=11474 start=0ns timeout=0ns
31,3844,219178323,-;logd: logdr: UID=1000 GID=1000 PID=11479 n tail=0 logMask=8 pid=11474 start=0ns timeout=0ns
31,3845,219191067,-;logd: logdr: UID=1000 GID=1000 PID=11479 n tail=0 logMask=1 pid=11474 start=0ns timeout=0ns
14,3846,219207580,-;init: Untracked pid 11479 exited with status 0
14,3847,219210295,-;init: Service 'qspmhal' (pid 11474) received signal 6
14,3848,219210395,-;init: Sending signal 9 to service 'qspmhal' (pid 11474) process group...
14,3849,219228311,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 11474 in 17ms
14,3850,219231771,-;init: Untracked pid 11481 exited with status 0
11,3851,219579914,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3852,219616077,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3853,219958302,-;init: starting service 'qvrd'...
11,3854,223637561,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3855,223878547,-;init: starting service 'qspmhal'...
31,3856,224192050,-;logd: logdr: UID=1000 GID=1000 PID=11799 n tail=50 logMask=8 pid=11796 start=0ns timeout=0ns
31,3857,224205949,-;logd: logdr: UID=1000 GID=1000 PID=11799 n tail=50 logMask=1 pid=11796 start=0ns timeout=0ns
6,3858,224208633,-;IRQ 6: no longer affine to CPU7
31,3859,224221729,-;logd: logdr: UID=1000 GID=1000 PID=11799 n tail=0 logMask=8 pid=11796 start=0ns timeout=0ns
31,3860,224228962,-;logd: logdr: UID=1000 GID=1000 PID=11799 n tail=0 logMask=1 pid=11796 start=0ns timeout=0ns
14,3861,224242122,-;init: Service 'qspmhal' (pid 11796) received signal 6
14,3862,224242217,-;init: Sending signal 9 to service 'qspmhal' (pid 11796) process group...
14,3863,224272455,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 11796 in 29ms
14,3864,224276877,-;init: Untracked pid 11799 exited with status 0
14,3865,224277205,-;init: Untracked pid 11803 received signal 9
11,3866,224601495,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3867,224644125,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3868,225002807,-;init: starting service 'qvrd'...
3,3869,226042241,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3870,226048313,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3871,226056681,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3872,226062607,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3873,226069422,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3874,226075116,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3875,226082115,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3876,226087803,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3877,226096251,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3878,226102001,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3879,226123026,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3880,226134959,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3881,226170269,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3882,226177112,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3883,226190518,-;healthd: battery l=51 v=3692 t=31.6 h=2 st=2 c=-973969 fc=3812000 cc=0 chg=a
3,3884,226192542,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3885,226198434,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3886,226215438,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3887,226221248,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,3888,226469036,-;IRQ 6: no longer affine to CPU7
6,3889,228088879,-;IRQ 6: no longer affine to CPU7
11,3890,228663996,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3891,228920123,-;init: starting service 'qspmhal'...
31,3892,229250064,-;logd: logdr: UID=1000 GID=1000 PID=12124 n tail=50 logMask=8 pid=12118 start=0ns timeout=0ns
31,3893,229257093,-;logd: logdr: UID=1000 GID=1000 PID=12124 n tail=50 logMask=1 pid=12118 start=0ns timeout=0ns
31,3894,229280235,-;logd: logdr: UID=1000 GID=1000 PID=12124 n tail=0 logMask=8 pid=12118 start=0ns timeout=0ns
31,3895,229287814,-;logd: logdr: UID=1000 GID=1000 PID=12124 n tail=0 logMask=1 pid=12118 start=0ns timeout=0ns
14,3896,229304140,-;init: Service 'qspmhal' (pid 12118) received signal 6
14,3897,229304235,-;init: Sending signal 9 to service 'qspmhal' (pid 12118) process group...
14,3898,229320211,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 12118 in 15ms
14,3899,229323912,-;init: Untracked pid 12124 exited with status 0
14,3900,229324371,-;init: Untracked pid 12126 received signal 9
11,3901,229635223,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,3902,229667576,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3903,230053322,-;init: starting service 'qvrd'...
6,3904,230228471,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,3905,230230852,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,3906,230260421,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3907,230260933,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3908,230261440,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3909,230269087,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3910,230269477,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3911,230270272,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,3912,230270660,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,3913,230906845,-;perf: interrupt took too long (3152 > 3136), lowering kernel.perf_event_max_sample_rate to 63400
6,3914,232068870,-;IRQ 6: no longer affine to CPU7
11,3915,233689705,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3916,233963187,-;init: starting service 'qspmhal'...
3,3917,234209966,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,3918,234214155,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,3919,234222920,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3920,234241281,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3921,234247208,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3922,234254327,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3923,234260945,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3924,234267798,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3925,234274300,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3926,234282246,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3927,234290370,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3928,234310482,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3929,234316196,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3930,234331073,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,3931,234334476,-;logd: logdr: UID=1000 GID=1000 PID=12468 n tail=50 logMask=8 pid=12443 start=0ns timeout=0ns
3,3932,234336765,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3933,234339039,-;healthd: battery l=51 v=3660 t=31.9 h=2 st=2 c=-889435 fc=3812000 cc=0 chg=a
3,3934,234344250,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3935,234350005,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,3936,234354215,-;logd: logdr: UID=1000 GID=1000 PID=12468 n tail=50 logMask=1 pid=12443 start=0ns timeout=0ns
3,3937,234368365,-;max1720x 0-0036: SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,3938,234371228,-;logd: logdr: UID=1000 GID=1000 PID=12468 n tail=0 logMask=8 pid=12443 start=0ns timeout=0ns
3,3939,234374052,-;max1720x 0-0036: POST SOC routine soc(51) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,3940,234380810,-;logd: logdr: UID=1000 GID=1000 PID=12468 n tail=0 logMask=1 pid=12443 start=0ns timeout=0ns
14,3941,234396183,-;init: Service 'qspmhal' (pid 12443) received signal 6
14,3942,234396229,-;init: Sending signal 9 to service 'qspmhal' (pid 12443) process group...
14,3943,234408710,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 12443 in 12ms
14,3944,234414172,-;init: Untracked pid 12468 exited with status 0
14,3945,234414655,-;init: Untracked pid 12471 received signal 9
11,3946,234697572,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3947,235109486,-;init: starting service 'qvrd'...
6,3948,235128647,-;IRQ 6: no longer affine to CPU7
11,3949,238717622,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,3950,238995412,-;init: starting service 'qspmhal'...
11,3951,239236648,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3952,239320961,-;logd: logdr: UID=1000 GID=1000 PID=12793 n tail=50 logMask=8 pid=12789 start=0ns timeout=0ns
31,3953,239333285,-;logd: logdr: UID=1000 GID=1000 PID=12793 n tail=50 logMask=1 pid=12789 start=0ns timeout=0ns
31,3954,239349453,-;logd: logdr: UID=1000 GID=1000 PID=12793 n tail=0 logMask=8 pid=12789 start=0ns timeout=0ns
31,3955,239358641,-;logd: logdr: UID=1000 GID=1000 PID=12793 n tail=0 logMask=1 pid=12789 start=0ns timeout=0ns
14,3956,239378561,-;init: Service 'qspmhal' (pid 12789) received signal 6
14,3957,239379128,-;init: Sending signal 9 to service 'qspmhal' (pid 12789) process group...
14,3958,239399553,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 12789 in 19ms
14,3959,239406075,-;init: Untracked pid 12793 exited with status 0
14,3960,239406613,-;init: Untracked pid 12795 received signal 9
11,3961,239721739,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
36,3962,240106277,-;type=1400 audit(1614200774.586:293): avc: denied { read } for comm="ywell.defroster" name="u:object_r:hsm_prop:s0" dev="tmpfs" ino=14960 scontext=u:r:system_app:s0 tcontext=u:object_r:hsm_prop:s0 tclass=file permissive=0
14,3963,240144753,-;init: starting service 'qvrd'...
36,3964,241275485,-;type=1400 audit(1614200775.756:294): avc: denied { read } for comm="Binder:2795_3" name="u:object_r:hsm_prop:s0" dev="tmpfs" ino=14960 scontext=u:r:system_app:s0 tcontext=u:object_r:hsm_prop:s0 tclass=file permissive=0
36,3965,242110933,-;type=1400 audit(1614200776.596:295): avc: denied { read } for comm="ell.vdockconfig" name="u:object_r:hsm_prop:s0" dev="tmpfs" ino=14960 scontext=u:r:system_app:s0 tcontext=u:object_r:hsm_prop:s0 tclass=file permissive=0
3,3966,242376454,-;max1720x 0-0036: SOC routine soc(50) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3967,242383887,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(51)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3968,242397621,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3969,242404492,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3970,242411492,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3971,242417764,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3972,242425509,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3973,242432774,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3974,242440522,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3975,242446993,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3976,242465208,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3977,242470971,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3978,242520937,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3979,242526627,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,3980,242534855,-;healthd: battery l=50 v=3681 t=31.8 h=2 st=2 c=-895233 fc=3812000 cc=0 chg=a
3,3981,242536133,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3982,242541900,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3983,242554835,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,3984,242560599,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,3985,242589688,-;IRQ 6: no longer affine to CPU4
36,3986,242687086,-;type=1400 audit(1614200777.166:296): avc: denied { read } for comm="Binder:557_2" name="wakeup48" dev="sysfs" ino=60292 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,3987,242689177,-;type=1400 audit(1614200777.176:297): avc: denied { read } for comm="Binder:557_2" name="wakeup4" dev="sysfs" ino=36664 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,3988,242700239,-;type=1400 audit(1614200777.186:298): avc: denied { read } for comm="Binder:557_2" name="wakeup28" dev="sysfs" ino=48113 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,3989,242707685,-;type=1400 audit(1614200777.186:299): avc: denied { read } for comm="Binder:557_2" name="wakeup18" dev="sysfs" ino=37631 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
36,3990,242713339,-;type=1400 audit(1614200777.196:300): avc: denied { read } for comm="Binder:557_2" name="wakeup46" dev="sysfs" ino=60220 scontext=u:r:system_suspend:s0 tcontext=u:object_r:sysfs:s0 tclass=dir permissive=0
4,3991,242725253,-;audit: audit_lost=29 audit_rate_limit=5 audit_backlog_limit=64
3,3992,242725268,-;audit: rate limit exceeded
14,3993,244039386,-;init: starting service 'qspmhal'...
11,3994,244263566,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,3995,244366676,-;logd: logdr: UID=1000 GID=1000 PID=13262 n tail=50 logMask=8 pid=13254 start=0ns timeout=0ns
31,3996,244376851,-;logd: logdr: UID=1000 GID=1000 PID=13262 n tail=50 logMask=1 pid=13254 start=0ns timeout=0ns
31,3997,244396453,-;logd: logdr: UID=1000 GID=1000 PID=13262 n tail=0 logMask=8 pid=13254 start=0ns timeout=0ns
31,3998,244404937,-;logd: logdr: UID=1000 GID=1000 PID=13262 n tail=0 logMask=1 pid=13254 start=0ns timeout=0ns
14,3999,244419523,-;init: Service 'qspmhal' (pid 13254) received signal 6
14,4000,244419566,-;init: Sending signal 9 to service 'qspmhal' (pid 13254) process group...
14,4001,244458818,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 13254 in 38ms
14,4002,244463526,-;init: Untracked pid 13262 exited with status 0
14,4003,244464039,-;init: Untracked pid 13270 received signal 9
11,4004,244471927,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4005,245176501,-;init: starting service 'qvrd'...
14,4006,245179651,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
14,4007,249093331,-;init: starting service 'qspmhal'...
11,4008,249297290,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4009,249449600,-;logd: logdr: UID=1000 GID=1000 PID=13570 n tail=50 logMask=8 pid=13561 start=0ns timeout=0ns
31,4010,249457532,-;logd: logdr: UID=1000 GID=1000 PID=13570 n tail=50 logMask=1 pid=13561 start=0ns timeout=0ns
31,4011,249477664,-;logd: logdr: UID=1000 GID=1000 PID=13570 n tail=0 logMask=8 pid=13561 start=0ns timeout=0ns
31,4012,249490097,-;logd: logdr: UID=1000 GID=1000 PID=13570 n tail=0 logMask=1 pid=13561 start=0ns timeout=0ns
11,4013,249502972,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4014,249519865,-;init: Service 'qspmhal' (pid 13561) received signal 6
14,4015,249519944,-;init: Sending signal 9 to service 'qspmhal' (pid 13561) process group...
14,4016,249533452,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 13561 in 12ms
14,4017,249538505,-;init: Untracked pid 13570 exited with status 0
14,4018,249539204,-;init: Untracked pid 13587 exited with status 0
14,4019,250207598,-;init: starting service 'qvrd'...
14,4020,250212785,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
3,4021,250538948,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4022,250556010,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4023,250565258,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4024,250571912,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4025,250578761,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4026,250584600,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4027,250592128,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4028,250597912,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4029,250606192,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4030,250612251,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4031,250628244,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4032,250633953,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4033,250684653,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4034,250691558,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4035,250703575,-;healthd: battery l=50 v=3713 t=31.7 h=2 st=2 c=-817261 fc=3812000 cc=0 chg=a
3,4036,250706115,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4037,250712242,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4038,250727835,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4039,250734585,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4040,252033239,-;max1720x 0-0036: case 5 === SN=TWMX2049505588
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4041,252049179,-;IRQ 6: no longer affine to CPU7
3,4042,252053238,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4043,252060915,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4044,252081618,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4045,252087320,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4046,252119675,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4047,252125367,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4048,252133598,-;healthd: battery l=50 v=3715 t=31.9 h=2 st=2 c=-798187 fc=3812000 cc=0 chg=a
3,4049,252134885,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4050,252140757,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4051,252152226,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4052,252157922,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4053,254131210,-;init: starting service 'qspmhal'...
31,4054,254475968,-;logd: logdr: UID=1000 GID=1000 PID=13912 n tail=50 logMask=8 pid=13909 start=0ns timeout=0ns
11,4055,254532683,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4056,254586130,-;logd: logdr: UID=1000 GID=1000 PID=13912 n tail=50 logMask=1 pid=13909 start=0ns timeout=0ns
31,4057,254610362,-;logd: logdr: UID=1000 GID=1000 PID=13912 n tail=0 logMask=8 pid=13909 start=0ns timeout=0ns
31,4058,254683146,-;logd: logdr: UID=1000 GID=1000 PID=13912 n tail=0 logMask=1 pid=13909 start=0ns timeout=0ns
14,4059,254717735,-;init: Untracked pid 13912 exited with status 0
14,4060,254721140,-;init: Service 'qspmhal' (pid 13909) received signal 6
14,4061,254721339,-;init: Sending signal 9 to service 'qspmhal' (pid 13909) process group...
14,4062,254749572,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 13909 in 27ms
14,4063,254754549,-;init: Untracked pid 13920 exited with status 0
11,4064,254887270,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4065,255266579,-;init: starting service 'qvrd'...
14,4066,255273534,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
3,4067,258705350,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4068,258711502,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4069,258723021,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4070,258729271,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4071,258736208,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4072,258742425,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4073,258750318,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4074,258756017,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4075,258763593,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4076,258768541,-;IRQ 6: no longer affine to CPU7
3,4077,258769622,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4078,258800915,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4079,258806615,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4080,258848238,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4081,258853932,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4082,258862060,-;healthd: battery l=50 v=3709 t=31.7 h=2 st=2 c=-882416 fc=3812000 cc=0 chg=a
3,4083,258863308,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4084,258869066,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4085,258892297,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4086,258897984,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4087,259181837,-;init: starting service 'qspmhal'...
31,4088,259529536,-;logd: logdr: UID=1000 GID=1000 PID=14258 n tail=50 logMask=8 pid=14233 start=0ns timeout=0ns
31,4089,259542887,-;logd: logdr: UID=1000 GID=1000 PID=14258 n tail=50 logMask=1 pid=14233 start=0ns timeout=0ns
11,4090,259557450,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4091,259564580,-;logd: logdr: UID=1000 GID=1000 PID=14258 n tail=0 logMask=8 pid=14233 start=0ns timeout=0ns
31,4092,259582100,-;logd: logdr: UID=1000 GID=1000 PID=14258 n tail=0 logMask=1 pid=14233 start=0ns timeout=0ns
14,4093,259595607,-;init: Service 'qspmhal' (pid 14233) received signal 6
14,4094,259595982,-;init: Sending signal 9 to service 'qspmhal' (pid 14233) process group...
14,4095,259614645,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 14233 in 18ms
14,4096,259620508,-;init: Untracked pid 14258 exited with status 0
14,4097,259621021,-;init: Untracked pid 14262 received signal 9
11,4098,259925568,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4099,260315574,-;init: starting service 'qvrd'...
14,4100,260325234,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
14,4101,264229256,-;init: starting service 'qspmhal'...
31,4102,264540217,-;logd: logdr: UID=1000 GID=1000 PID=14571 n tail=50 logMask=8 pid=14554 start=0ns timeout=0ns
31,4103,264548533,-;logd: logdr: UID=1000 GID=1000 PID=14571 n tail=50 logMask=1 pid=14554 start=0ns timeout=0ns
31,4104,264563045,-;logd: logdr: UID=1000 GID=1000 PID=14571 n tail=0 logMask=8 pid=14554 start=0ns timeout=0ns
31,4105,264573471,-;logd: logdr: UID=1000 GID=1000 PID=14571 n tail=0 logMask=1 pid=14554 start=0ns timeout=0ns
14,4106,264593405,-;init: Service 'qspmhal' (pid 14554) received signal 6
14,4107,264593499,-;init: Sending signal 9 to service 'qspmhal' (pid 14554) process group...
14,4108,264617444,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 14554 in 23ms
14,4109,264629071,-;init: Untracked pid 14571 exited with status 0
14,4110,264629576,-;init: Untracked pid 14579 received signal 9
11,4111,264631987,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4112,264946060,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4113,265368517,-;init: starting service 'qvrd'...
14,4114,265373970,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
3,4115,266873061,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4116,266880851,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4117,266894097,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4118,266900350,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4119,266907645,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4120,266913893,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4121,266921428,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4122,266927150,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4123,266934877,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4124,266941158,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4125,266969116,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4126,266974981,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4127,267008547,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4128,267014237,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4129,267023069,-;healthd: battery l=50 v=3719 t=31.8 h=2 st=2 c=-550232 fc=3812000 cc=0 chg=a
3,4130,267024399,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4131,267030157,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4132,267042001,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4133,267047700,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4134,269263179,-;init: starting service 'qspmhal'...
31,4135,269596630,-;logd: logdr: UID=1000 GID=1000 PID=14880 n tail=50 logMask=8 pid=14875 start=0ns timeout=0ns
31,4136,269612851,-;logd: logdr: UID=1000 GID=1000 PID=14880 n tail=50 logMask=1 pid=14875 start=0ns timeout=0ns
11,4137,269621047,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4138,269634425,-;logd: logdr: UID=1000 GID=1000 PID=14880 n tail=0 logMask=8 pid=14875 start=0ns timeout=0ns
31,4139,269647222,-;logd: logdr: UID=1000 GID=1000 PID=14880 n tail=0 logMask=1 pid=14875 start=0ns timeout=0ns
14,4140,269675619,-;init: Service 'qspmhal' (pid 14875) received signal 6
14,4141,269675935,-;init: Sending signal 9 to service 'qspmhal' (pid 14875) process group...
14,4142,269692036,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 14875 in 15ms
14,4143,269702190,-;init: Untracked pid 14880 exited with status 0
14,4144,269702694,-;init: Untracked pid 14888 exited with status 0
3,4145,269704728,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4146,269711503,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4147,269726752,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4148,269732997,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4149,269739879,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4150,269745574,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4151,269753967,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4152,269765656,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4153,269772628,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4154,269778452,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4155,269784873,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4156,269786500,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4157,269790675,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4158,269798256,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4159,269803812,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4160,269814595,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4161,269820206,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4162,269826874,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4163,269839058,-;healthd: battery l=50 v=3728 t=31.8 h=2 st=2 c=-679932 fc=3812000 cc=0 chg=a
3,4164,269841373,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4165,269847174,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4166,269890060,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4167,269896121,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4168,269915841,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4169,269924989,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4170,269941942,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4171,269947673,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4172,269959303,-;healthd: battery l=50 v=3750 t=31.7 h=2 st=2 c=-740356 fc=3812000 cc=0 chg=a
3,4173,269961228,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4174,269967147,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4175,269979373,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,4176,269979915,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,4177,269985075,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4178,270406098,-;init: starting service 'qvrd'...
14,4179,270411608,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
3,4180,271299563,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4181,271305266,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4182,271319960,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4183,271325663,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4184,271335322,-;healthd: battery l=50 v=3761 t=31.6 h=2 st=2 c=-553894 fc=3812000 cc=0 chg=a
3,4185,271337288,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4186,271343123,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4187,271357450,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4188,271363276,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4189,273468367,-;IRQ 6: no longer affine to CPU5
14,4190,274297249,-;init: starting service 'qspmhal'...
31,4191,274614353,-;logd: logdr: UID=1000 GID=1000 PID=15233 n tail=50 logMask=8 pid=15224 start=0ns timeout=0ns
31,4192,274624577,-;logd: logdr: UID=1000 GID=1000 PID=15233 n tail=50 logMask=1 pid=15224 start=0ns timeout=0ns
11,4193,274643175,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4194,274645334,-;logd: logdr: UID=1000 GID=1000 PID=15233 n tail=0 logMask=8 pid=15224 start=0ns timeout=0ns
11,4195,274662004,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4196,274703357,-;logd: logdr: UID=1000 GID=1000 PID=15233 n tail=0 logMask=1 pid=15224 start=0ns timeout=0ns
14,4197,274742184,-;init: Service 'qspmhal' (pid 15224) received signal 6
14,4198,274742258,-;init: Sending signal 9 to service 'qspmhal' (pid 15224) process group...
14,4199,274755309,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 15224 in 12ms
14,4200,274760645,-;init: Untracked pid 15235 received signal 9
14,4201,274761328,-;init: Untracked pid 15233 exited with status 0
3,4202,275036627,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4203,275043636,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4204,275055416,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4205,275063098,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4206,275069967,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4207,275075764,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4208,275084039,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4209,275090276,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4210,275097961,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4211,275103775,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4212,275122481,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4213,275128311,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4214,275179180,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4215,275184900,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4216,275193947,-;healthd: battery l=50 v=3743 t=31.6 h=2 st=2 c=-593567 fc=3812000 cc=0 chg=a
3,4217,275195910,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4218,275201717,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4219,275215796,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4220,275221582,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4221,275472719,-;init: starting service 'qvrd'...
14,4222,275476935,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4223,276188817,-;IRQ 6: no longer affine to CPU7
6,4224,279329003,-;IRQ 6: no longer affine to CPU7
14,4225,279350011,-;init: starting service 'qspmhal'...
31,4226,279650823,-;logd: logdr: UID=1000 GID=1000 PID=15551 n tail=50 logMask=8 pid=15545 start=0ns timeout=0ns
31,4227,279667409,-;logd: logdr: UID=1000 GID=1000 PID=15551 n tail=50 logMask=1 pid=15545 start=0ns timeout=0ns
11,4228,279675847,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4229,279686982,-;logd: logdr: UID=1000 GID=1000 PID=15551 n tail=0 logMask=8 pid=15545 start=0ns timeout=0ns
11,4230,279692315,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4231,279702335,-;logd: logdr: UID=1000 GID=1000 PID=15551 n tail=0 logMask=1 pid=15545 start=0ns timeout=0ns
14,4232,279723766,-;init: Untracked pid 15551 exited with status 0
14,4233,279726852,-;init: Service 'qspmhal' (pid 15545) received signal 6
14,4234,279726893,-;init: Sending signal 9 to service 'qspmhal' (pid 15545) process group...
14,4235,279738952,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 15545 in 11ms
14,4236,279741412,-;init: Untracked pid 15553 exited with status 0
14,4237,280509671,-;init: starting service 'qvrd'...
14,4238,280511634,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
3,4239,283204439,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4240,283211260,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4241,283232244,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4242,283239067,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4243,283246810,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4244,283253206,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4245,283261043,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4246,283267259,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4247,283274685,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4248,283280760,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4249,283298754,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4250,283304445,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4251,283363161,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4252,283369071,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4253,283381526,-;healthd: battery l=50 v=3779 t=31.7 h=2 st=2 c=-469513 fc=3812000 cc=0 chg=a
3,4254,283384326,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4255,283390887,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4256,283404678,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4257,283410485,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4258,284384903,-;init: starting service 'qspmhal'...
11,4259,284704086,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4260,284721603,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4261,284735931,-;logd: logdr: UID=1000 GID=1000 PID=15873 n tail=50 logMask=8 pid=15867 start=0ns timeout=0ns
31,4262,284748885,-;logd: logdr: UID=1000 GID=1000 PID=15873 n tail=50 logMask=1 pid=15867 start=0ns timeout=0ns
31,4263,284762248,-;logd: logdr: UID=1000 GID=1000 PID=15873 n tail=0 logMask=8 pid=15867 start=0ns timeout=0ns
31,4264,284769568,-;logd: logdr: UID=1000 GID=1000 PID=15873 n tail=0 logMask=1 pid=15867 start=0ns timeout=0ns
14,4265,284792033,-;init: Untracked pid 15873 exited with status 0
14,4266,284801832,-;init: Service 'qspmhal' (pid 15867) received signal 6
14,4267,284801920,-;init: Sending signal 9 to service 'qspmhal' (pid 15867) process group...
14,4268,284809595,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 15867 in 7ms
14,4269,284813948,-;init: Untracked pid 15875 exited with status 0
14,4270,285533325,-;init: starting service 'qvrd'...
14,4271,285537255,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
14,4272,289446120,-;init: starting service 'qspmhal'...
11,4273,289751956,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4274,289769929,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4275,289769994,-;logd: logdr: UID=1000 GID=1000 PID=16196 n tail=50 logMask=8 pid=16175 start=0ns timeout=0ns
31,4276,289797559,-;logd: logdr: UID=1000 GID=1000 PID=16196 n tail=50 logMask=1 pid=16175 start=0ns timeout=0ns
31,4277,289811986,-;logd: logdr: UID=1000 GID=1000 PID=16196 n tail=0 logMask=8 pid=16175 start=0ns timeout=0ns
31,4278,289822797,-;logd: logdr: UID=1000 GID=1000 PID=16196 n tail=0 logMask=1 pid=16175 start=0ns timeout=0ns
14,4279,289842331,-;init: Service 'qspmhal' (pid 16175) received signal 6
14,4280,289842444,-;init: Sending signal 9 to service 'qspmhal' (pid 16175) process group...
14,4281,289863306,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 16175 in 20ms
14,4282,289866902,-;init: Untracked pid 16196 exited with status 0
14,4283,289867296,-;init: Untracked pid 16198 received signal 9
14,4284,290580968,-;init: starting service 'qvrd'...
14,4285,290587472,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4286,290948634,-;IRQ 6: no longer affine to CPU7
3,4287,291369636,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4288,291375555,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4289,291387352,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4290,291394119,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4291,291401340,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4292,291407169,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4293,291414955,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4294,291421035,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4295,291433363,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4296,291439402,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4297,291457436,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4298,291464400,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4299,291511083,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4300,291516793,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4301,291527466,-;healthd: battery l=50 v=3783 t=31.5 h=2 st=2 c=-522308 fc=3812000 cc=0 chg=a
3,4302,291530978,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4303,291536675,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4304,291553606,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4305,291559415,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4306,294128916,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
3,4307,294131312,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
7,4308,294161428,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,4309,294161741,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,4310,294165444,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
6,4311,294168694,-;tas2563 0-004c: irq_work_routine
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,4312,294169098,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:26, VAL: 0xfc
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,4313,294169443,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:27, VAL: 0xfb
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
7,4314,294169727,-;tas2563 0-004c: tas2563_dev_write: chn4c:BOOK:PAGE:REG 0:0:28, VAL: 0xdf
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-004c
14,4315,294495994,-;init: starting service 'qspmhal'...
11,4316,294776425,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4317,294849832,-;logd: logdr: UID=1000 GID=1000 PID=16558 n tail=50 logMask=8 pid=16550 start=0ns timeout=0ns
31,4318,294864088,-;logd: logdr: UID=1000 GID=1000 PID=16558 n tail=50 logMask=1 pid=16550 start=0ns timeout=0ns
31,4319,294881469,-;logd: logdr: UID=1000 GID=1000 PID=16558 n tail=0 logMask=8 pid=16550 start=0ns timeout=0ns
31,4320,294890895,-;logd: logdr: UID=1000 GID=1000 PID=16558 n tail=0 logMask=1 pid=16550 start=0ns timeout=0ns
14,4321,294904399,-;init: Service 'qspmhal' (pid 16550) received signal 6
14,4322,294904511,-;init: Sending signal 9 to service 'qspmhal' (pid 16550) process group...
14,4323,294929721,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 16550 in 24ms
14,4324,294933880,-;init: Untracked pid 16558 exited with status 0
14,4325,294934311,-;init: Untracked pid 16560 received signal 9
11,4326,295408623,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4327,295642475,-;init: starting service 'qvrd'...
14,4328,295648935,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4329,296169213,-;IRQ 6: no longer affine to CPU7
3,4330,299531408,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4331,299537264,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4332,299549274,-;init: starting service 'qspmhal'...
3,4333,299553568,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4334,299559755,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4335,299566653,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4336,299572732,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4337,299579680,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4338,299585741,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4339,299592929,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4340,299598992,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4341,299629424,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4342,299635255,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4343,299651770,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4344,299657515,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4345,299665815,-;healthd: battery l=50 v=3745 t=31.6 h=2 st=2 c=-522461 fc=3812000 cc=0 chg=a
3,4346,299667536,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4347,299673314,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4348,299689820,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4349,299695517,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,4350,299811029,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4351,299850867,-;logd: logdr: UID=1000 GID=1000 PID=16880 n tail=50 logMask=8 pid=16864 start=0ns timeout=0ns
31,4352,299862672,-;logd: logdr: UID=1000 GID=1000 PID=16880 n tail=50 logMask=1 pid=16864 start=0ns timeout=0ns
31,4353,299895671,-;logd: logdr: UID=1000 GID=1000 PID=16880 n tail=0 logMask=8 pid=16864 start=0ns timeout=0ns
31,4354,299908435,-;logd: logdr: UID=1000 GID=1000 PID=16880 n tail=0 logMask=1 pid=16864 start=0ns timeout=0ns
14,4355,299927237,-;init: Service 'qspmhal' (pid 16864) received signal 6
14,4356,299927327,-;init: Sending signal 9 to service 'qspmhal' (pid 16864) process group...
14,4357,299947127,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 16864 in 19ms
14,4358,299952285,-;init: Untracked pid 16880 exited with status 0
14,4359,299952810,-;init: Untracked pid 16882 received signal 9
11,4360,300426499,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4361,300705381,-;init: starting service 'qvrd'...
14,4362,300716478,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4363,302048974,-;IRQ 6: no longer affine to CPU7
14,4364,304564546,-;init: starting service 'qspmhal'...
31,4365,304857048,-;logd: logdr: UID=1000 GID=1000 PID=17242 n tail=50 logMask=8 pid=17212 start=0ns timeout=0ns
31,4366,304871860,-;logd: logdr: UID=1000 GID=1000 PID=17242 n tail=50 logMask=1 pid=17212 start=0ns timeout=0ns
31,4367,304888571,-;logd: logdr: UID=1000 GID=1000 PID=17242 n tail=0 logMask=8 pid=17212 start=0ns timeout=0ns
31,4368,304896330,-;logd: logdr: UID=1000 GID=1000 PID=17242 n tail=0 logMask=1 pid=17212 start=0ns timeout=0ns
14,4369,304914144,-;init: Untracked pid 17242 exited with status 0
14,4370,304917730,-;init: Service 'qspmhal' (pid 17212) received signal 6
14,4371,304917802,-;init: Sending signal 9 to service 'qspmhal' (pid 17212) process group...
14,4372,304924357,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 17212 in 6ms
14,4373,304926567,-;init: Untracked pid 17244 exited with status 0
6,4374,304948535,-;IRQ 6: no longer affine to CPU7
11,4375,305008465,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4376,305024285,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,4377,305308597,-;IRQ 6: no longer affine to CPU7
11,4378,305452289,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4379,305767554,-;init: starting service 'qvrd'...
6,4380,307208912,-;IRQ 6: no longer affine to CPU4
6,4381,307468954,-;IRQ 6: no longer affine to CPU7
3,4382,307694661,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4383,307702372,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4384,307711266,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4385,307717629,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4386,307724709,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4387,307730737,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4388,307740924,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4389,307746635,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4390,307754116,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4391,307761847,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4392,307779560,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4393,307786510,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4394,307832594,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4395,307838690,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4396,307850741,-;healthd: battery l=50 v=3708 t=31.6 h=2 st=2 c=-788727 fc=3812000 cc=0 chg=a
3,4397,307852745,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4398,307860944,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4399,307877569,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4400,307883446,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4401,309146313,-;perf: interrupt took too long (4075 > 3940), lowering kernel.perf_event_max_sample_rate to 49000
14,4402,309591277,-;init: starting service 'qspmhal'...
11,4403,310056945,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4404,310174292,-;logd: logdr: UID=1000 GID=1000 PID=17783 n tail=50 logMask=8 pid=17779 start=0ns timeout=0ns
31,4405,310215874,-;logd: logdr: UID=1000 GID=1000 PID=17783 n tail=50 logMask=1 pid=17779 start=0ns timeout=0ns
31,4406,310238017,-;logd: logdr: UID=1000 GID=1000 PID=17783 n tail=0 logMask=8 pid=17779 start=0ns timeout=0ns
31,4407,310252683,-;logd: logdr: UID=1000 GID=1000 PID=17783 n tail=0 logMask=1 pid=17779 start=0ns timeout=0ns
14,4408,310271195,-;init: Service 'qspmhal' (pid 17779) received signal 6
14,4409,310271250,-;init: Sending signal 9 to service 'qspmhal' (pid 17779) process group...
14,4410,310282871,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 17779 in 11ms
14,4411,310285235,-;init: Untracked pid 17785 received signal 9
14,4412,310285422,-;init: Untracked pid 17783 exited with status 0
11,4413,310482040,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4414,310802897,-;init: starting service 'qvrd'...
14,4415,310804517,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
14,4416,314627310,-;init: starting service 'qspmhal'...
11,4417,315118608,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4418,315150518,-;logd: logdr: UID=1000 GID=1000 PID=18159 n tail=50 logMask=8 pid=18131 start=0ns timeout=0ns
31,4419,315181491,-;logd: logdr: UID=1000 GID=1000 PID=18159 n tail=50 logMask=1 pid=18131 start=0ns timeout=0ns
11,4420,315206193,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4421,315223318,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4422,315240897,-;logd: logdr: UID=1000 GID=1000 PID=18159 n tail=0 logMask=8 pid=18131 start=0ns timeout=0ns
31,4423,315271075,-;logd: logdr: UID=1000 GID=1000 PID=18159 n tail=0 logMask=1 pid=18131 start=0ns timeout=0ns
14,4424,315326875,-;init: Service 'qspmhal' (pid 18131) received signal 6
14,4425,315326947,-;init: Sending signal 9 to service 'qspmhal' (pid 18131) process group...
14,4426,315346221,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 18131 in 18ms
14,4427,315352363,-;init: Untracked pid 18174 received signal 9
14,4428,315353367,-;init: Untracked pid 18159 exited with status 0
14,4429,315836388,-;init: starting service 'qvrd'...
3,4430,315863918,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4431,315872613,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4432,315908243,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4433,315915300,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4434,315928411,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4435,315938168,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4436,315947241,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4437,315954424,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4438,315962518,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4439,315972074,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4440,316025486,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4441,316036022,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4442,316087669,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4443,316093467,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4444,316103356,-;healthd: battery l=50 v=3730 t=31.8 h=2 st=2 c=-708923 fc=3812000 cc=0 chg=a
3,4445,316107680,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4446,316113463,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4447,316126587,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4448,316132386,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4449,316228393,-;IRQ 6: no longer affine to CPU7
6,4450,316389129,-;IRQ 6: no longer affine to CPU7
36,4451,318303653,-;type=1400 audit(1614200852.786:332): avc: denied { write } for comm="iptables-restor" name="etc" dev="overlay" ino=66286 scontext=u:r:netd:s0 tcontext=u:object_r:system_file:s0 tclass=dir permissive=0
6,4452,319428941,-;IRQ 6: no longer affine to CPU5
14,4453,319662861,-;init: starting service 'qspmhal'...
6,4454,319669020,-;IRQ 6: no longer affine to CPU7
11,4455,320147554,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4456,320237085,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4457,320274169,-;logd: logdr: UID=1000 GID=1000 PID=18535 n tail=50 logMask=8 pid=18515 start=0ns timeout=0ns
31,4458,320311243,-;logd: logdr: UID=1000 GID=1000 PID=18535 n tail=50 logMask=1 pid=18515 start=0ns timeout=0ns
31,4459,320365125,-;logd: logdr: UID=1000 GID=1000 PID=18535 n tail=0 logMask=8 pid=18515 start=0ns timeout=0ns
31,4460,320407522,-;logd: logdr: UID=1000 GID=1000 PID=18535 n tail=0 logMask=1 pid=18515 start=0ns timeout=0ns
14,4461,320476607,-;init: Service 'qspmhal' (pid 18515) received signal 6
14,4462,320476743,-;init: Sending signal 9 to service 'qspmhal' (pid 18515) process group...
14,4463,320584048,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 18515 in 106ms
14,4464,320596659,-;init: Untracked pid 18535 exited with status 0
14,4465,320597053,-;init: Untracked pid 18538 received signal 9
14,4466,320890700,-;init: starting service 'qvrd'...
14,4467,320897569,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4468,321028534,-;IRQ 6: no longer affine to CPU7
6,4469,321683747,-;LTEBCInitManage (18568) used greatest stack depth: 10528 bytes left
6,4470,323688912,-;IRQ 6: no longer affine to CPU7
3,4471,324027273,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4472,324034766,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4473,324045670,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4474,324053451,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4475,324060165,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4476,324066007,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4477,324073283,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4478,324079361,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4479,324087400,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4480,324093269,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4481,324117861,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4482,324123705,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4483,324158529,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4484,324164217,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4485,324172335,-;healthd: battery l=50 v=3749 t=31.7 h=2 st=2 c=-577545 fc=3812000 cc=0 chg=a
3,4486,324173713,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4487,324179521,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4488,324192204,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4489,324197897,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4490,324716808,-;init: starting service 'qspmhal'...
6,4491,324747395,-;alloc_contig_range: [fa940, fa950) PFNs busy
31,4492,325027395,-;logd: logdr: UID=1000 GID=1000 PID=18883 n tail=50 logMask=8 pid=18880 start=0ns timeout=0ns
31,4493,325041524,-;logd: logdr: UID=1000 GID=1000 PID=18883 n tail=50 logMask=1 pid=18880 start=0ns timeout=0ns
31,4494,325055976,-;logd: logdr: UID=1000 GID=1000 PID=18883 n tail=0 logMask=8 pid=18880 start=0ns timeout=0ns
31,4495,325064480,-;logd: logdr: UID=1000 GID=1000 PID=18883 n tail=0 logMask=1 pid=18880 start=0ns timeout=0ns
14,4496,325083393,-;init: Untracked pid 18883 exited with status 0
14,4497,325086776,-;init: Service 'qspmhal' (pid 18880) received signal 6
14,4498,325086889,-;init: Sending signal 9 to service 'qspmhal' (pid 18880) process group...
14,4499,325099225,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 18880 in 11ms
14,4500,325103462,-;init: Untracked pid 18887 exited with status 0
11,4501,325174954,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4502,325260808,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4503,325944600,-;init: starting service 'qvrd'...
14,4504,325947628,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4505,328908925,-;IRQ 6: no longer affine to CPU7
14,4506,329752228,-;init: starting service 'qspmhal'...
31,4507,330097379,-;logd: logdr: UID=1000 GID=1000 PID=19222 n tail=50 logMask=8 pid=19199 start=0ns timeout=0ns
31,4508,330125895,-;logd: logdr: UID=1000 GID=1000 PID=19222 n tail=50 logMask=1 pid=19199 start=0ns timeout=0ns
31,4509,330150539,-;logd: logdr: UID=1000 GID=1000 PID=19222 n tail=0 logMask=8 pid=19199 start=0ns timeout=0ns
31,4510,330159643,-;logd: logdr: UID=1000 GID=1000 PID=19222 n tail=0 logMask=1 pid=19199 start=0ns timeout=0ns
14,4511,330176516,-;init: Service 'qspmhal' (pid 19199) received signal 6
14,4512,330176578,-;init: Sending signal 9 to service 'qspmhal' (pid 19199) process group...
14,4513,330194269,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 19199 in 17ms
14,4514,330201614,-;init: Untracked pid 19222 exited with status 0
14,4515,330202185,-;init: Untracked pid 19225 received signal 9
11,4516,330203353,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4517,330288582,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4518,330979729,-;init: starting service 'qvrd'...
14,4519,330988532,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
3,4520,331298683,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4521,331304655,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4522,331319468,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4523,331325152,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4524,331333520,-;healthd: battery l=50 v=3779 t=31.6 h=2 st=2 c=-429535 fc=3812000 cc=0 chg=a
3,4525,331336179,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4526,331341923,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4527,331354007,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4528,331359798,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4529,332195568,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4530,332203111,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4531,332212781,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4532,332219358,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4533,332226822,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4534,332233115,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4535,332240385,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4536,332246108,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4537,332253463,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4538,332259342,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4539,332287653,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4540,332293598,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4541,332330464,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4542,332336233,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4543,332351928,-;healthd: battery l=50 v=3744 t=31.8 h=2 st=2 c=-473327 fc=3812000 cc=0 chg=a
3,4544,332354760,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4545,332360537,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4546,332380745,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4547,332386445,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4548,333614163,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4549,333620272,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4550,333635266,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4551,333641434,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4552,333648435,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4553,333654130,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4554,333664064,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4555,333666930,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4556,333669969,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4557,333675544,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4558,333689113,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4559,333694819,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4560,333701780,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4561,333707475,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4562,333714973,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4563,333719886,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4564,333721001,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4565,333726365,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4566,333728526,-;healthd: battery l=50 v=3704 t=31.9 h=2 st=2 c=-467529 fc=3812000 cc=0 chg=a
3,4567,333741999,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4568,333747954,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4569,333802692,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4570,333808442,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4571,333818458,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4572,333824153,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4573,333835408,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4574,333841176,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4575,333849249,-;healthd: battery l=50 v=3740 t=31.8 h=2 st=2 c=-720062 fc=3812000 cc=0 chg=a
3,4576,333850473,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4577,333856165,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4578,333877787,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4579,333883528,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4580,334777557,-;init: starting service 'qspmhal'...
31,4581,335093519,-;logd: logdr: UID=1000 GID=1000 PID=19555 n tail=50 logMask=8 pid=19532 start=0ns timeout=0ns
31,4582,335101490,-;logd: logdr: UID=1000 GID=1000 PID=19555 n tail=50 logMask=1 pid=19532 start=0ns timeout=0ns
31,4583,335114393,-;logd: logdr: UID=1000 GID=1000 PID=19555 n tail=0 logMask=8 pid=19532 start=0ns timeout=0ns
31,4584,335124860,-;logd: logdr: UID=1000 GID=1000 PID=19555 n tail=0 logMask=1 pid=19532 start=0ns timeout=0ns
14,4585,335143070,-;init: Service 'qspmhal' (pid 19532) received signal 6
14,4586,335143129,-;init: Sending signal 9 to service 'qspmhal' (pid 19532) process group...
14,4587,335155065,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 19532 in 11ms
14,4588,335160060,-;init: Untracked pid 19555 exited with status 0
14,4589,335160427,-;init: Untracked pid 19558 received signal 9
11,4590,335232197,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,4591,335368811,-;IRQ 6: no longer affine to CPU5
11,4592,335754752,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4593,335772158,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,4594,335788709,-;IRQ 6: no longer affine to CPU6
14,4595,336025322,-;init: starting service 'qvrd'...
11,4596,339783912,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4597,339807621,-;init: starting service 'qspmhal'...
31,4598,340140537,-;logd: logdr: UID=1000 GID=1000 PID=19904 n tail=50 logMask=8 pid=19879 start=0ns timeout=0ns
31,4599,340151500,-;logd: logdr: UID=1000 GID=1000 PID=19904 n tail=50 logMask=1 pid=19879 start=0ns timeout=0ns
31,4600,340170573,-;logd: logdr: UID=1000 GID=1000 PID=19904 n tail=0 logMask=8 pid=19879 start=0ns timeout=0ns
31,4601,340182587,-;logd: logdr: UID=1000 GID=1000 PID=19904 n tail=0 logMask=1 pid=19879 start=0ns timeout=0ns
14,4602,340204246,-;init: Service 'qspmhal' (pid 19879) received signal 6
14,4603,340204358,-;init: Sending signal 9 to service 'qspmhal' (pid 19879) process group...
14,4604,340223229,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 19879 in 18ms
14,4605,340228759,-;init: Untracked pid 19904 exited with status 0
14,4606,340229213,-;init: Untracked pid 19907 exited with status 0
11,4607,340263934,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,4608,340368632,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4609,340374643,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4610,340384428,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4611,340391209,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4612,340397688,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4613,340404482,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4614,340413079,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4615,340420053,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4616,340427024,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4617,340432945,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4618,340452231,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4619,340457923,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4620,340502781,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4621,340511429,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4622,340522640,-;healthd: battery l=50 v=3762 t=31.6 h=2 st=2 c=-416107 fc=3812000 cc=0 chg=a
3,4623,340525450,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4624,340531495,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4625,340545103,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4626,340550871,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,4627,340786897,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4628,341079690,-;init: starting service 'qvrd'...
11,4629,344803922,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4630,344824635,-;init: starting service 'qspmhal'...
31,4631,345132037,-;logd: logdr: UID=1000 GID=1000 PID=20241 n tail=50 logMask=8 pid=20216 start=0ns timeout=0ns
31,4632,345140908,-;logd: logdr: UID=1000 GID=1000 PID=20241 n tail=50 logMask=1 pid=20216 start=0ns timeout=0ns
31,4633,345154647,-;logd: logdr: UID=1000 GID=1000 PID=20241 n tail=0 logMask=8 pid=20216 start=0ns timeout=0ns
31,4634,345161987,-;logd: logdr: UID=1000 GID=1000 PID=20241 n tail=0 logMask=1 pid=20216 start=0ns timeout=0ns
14,4635,345174508,-;init: Service 'qspmhal' (pid 20216) received signal 6
14,4636,345174596,-;init: Sending signal 9 to service 'qspmhal' (pid 20216) process group...
14,4637,345181186,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 20216 in 6ms
14,4638,345184426,-;init: Untracked pid 20241 exited with status 0
14,4639,345184740,-;init: Untracked pid 20244 exited with status 0
11,4640,345299703,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4641,345812879,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4642,346110267,-;init: starting service 'qvrd'...
3,4643,348524798,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4644,348535772,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4645,348551257,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4646,348557773,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4647,348566149,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4648,348572672,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4649,348580495,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4650,348586314,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4651,348594008,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4652,348600032,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4653,348627122,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4654,348632894,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4655,348683312,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4656,348689606,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4657,348712941,-;healthd: battery l=50 v=3769 t=31.7 h=2 st=2 c=-479278 fc=3812000 cc=0 chg=a
3,4658,348715800,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4659,348721632,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4660,348734057,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4661,348739874,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
11,4662,349834904,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4663,349855616,-;init: starting service 'qspmhal'...
31,4664,350161259,-;logd: logdr: UID=1000 GID=1000 PID=20537 n tail=50 logMask=8 pid=20533 start=0ns timeout=0ns
31,4665,350174019,-;logd: logdr: UID=1000 GID=1000 PID=20537 n tail=50 logMask=1 pid=20533 start=0ns timeout=0ns
31,4666,350189719,-;logd: logdr: UID=1000 GID=1000 PID=20537 n tail=0 logMask=8 pid=20533 start=0ns timeout=0ns
31,4667,350197551,-;logd: logdr: UID=1000 GID=1000 PID=20537 n tail=0 logMask=1 pid=20533 start=0ns timeout=0ns
14,4668,350212433,-;init: Untracked pid 20537 exited with status 0
14,4669,350217410,-;init: Service 'qspmhal' (pid 20533) received signal 6
14,4670,350217508,-;init: Sending signal 9 to service 'qspmhal' (pid 20533) process group...
14,4671,350230965,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 20533 in 13ms
14,4672,350234558,-;init: Untracked pid 20539 exited with status 0
11,4673,350314095,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4674,350839787,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,4675,351110051,-;IRQ 6: no longer affine to CPU7
14,4676,351146179,-;init: starting service 'qvrd'...
6,4677,352982364,-;[soft_i][0x1a83d556c][21:08:07.475798] wlan: [0:I:QDF] DHCP-R TX: SA:3e:fd:55:14:24:bf DA:94:de:80:a9:0e:ae msdu_id:1197 status: succ
6,4678,352984360,-;[cds_ol][0x1a83deaf8][21:08:07.477792] wlan: [1659:I:QDF] DHCP-A RX: SA:f0:7f:06:cc:c0:40 DA:3e:fd:55:14:24:bf
11,4679,354862331,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4680,354884683,-;init: starting service 'qspmhal'...
31,4681,355244883,-;logd: logdr: UID=1000 GID=1000 PID=20878 n tail=50 logMask=8 pid=20869 start=0ns timeout=0ns
31,4682,355277826,-;logd: logdr: UID=1000 GID=1000 PID=20878 n tail=50 logMask=1 pid=20869 start=0ns timeout=0ns
31,4683,355297339,-;logd: logdr: UID=1000 GID=1000 PID=20878 n tail=0 logMask=8 pid=20869 start=0ns timeout=0ns
31,4684,355311593,-;logd: logdr: UID=1000 GID=1000 PID=20878 n tail=0 logMask=1 pid=20869 start=0ns timeout=0ns
14,4685,355332463,-;init: Service 'qspmhal' (pid 20869) received signal 6
14,4686,355332551,-;init: Sending signal 9 to service 'qspmhal' (pid 20869) process group...
14,4687,355351185,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 20869 in 18ms
14,4688,355355613,-;init: Untracked pid 20878 exited with status 0
14,4689,355356009,-;init: Untracked pid 20894 received signal 9
11,4690,355357391,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4691,355873939,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4692,356180138,-;init: starting service 'qvrd'...
3,4693,356688987,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4694,356695029,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4695,356707675,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4696,356714968,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4697,356724682,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4698,356730784,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4699,356737390,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4700,356743928,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4701,356748747,-;IRQ 6: no longer affine to CPU7
3,4702,356752926,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4703,356759954,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4704,356775331,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4705,356781137,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4706,356793186,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4707,356798940,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4708,356807047,-;healthd: battery l=50 v=3779 t=31.9 h=2 st=2 c=-451202 fc=3812000 cc=0 chg=a
3,4709,356809080,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4710,356815016,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4711,356833356,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4712,356839133,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4713,359913945,-;init: starting service 'qspmhal'...
31,4714,360227355,-;logd: logdr: UID=1000 GID=1000 PID=21216 n tail=50 logMask=8 pid=21212 start=0ns timeout=0ns
31,4715,360239801,-;logd: logdr: UID=1000 GID=1000 PID=21216 n tail=50 logMask=1 pid=21212 start=0ns timeout=0ns
31,4716,360267403,-;logd: logdr: UID=1000 GID=1000 PID=21216 n tail=0 logMask=8 pid=21212 start=0ns timeout=0ns
31,4717,360280459,-;logd: logdr: UID=1000 GID=1000 PID=21216 n tail=0 logMask=1 pid=21212 start=0ns timeout=0ns
14,4718,360302737,-;init: Service 'qspmhal' (pid 21212) received signal 6
14,4719,360302864,-;init: Sending signal 9 to service 'qspmhal' (pid 21212) process group...
14,4720,360321200,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 21212 in 17ms
14,4721,360326466,-;init: Untracked pid 21216 exited with status 0
14,4722,360326906,-;init: Untracked pid 21218 received signal 9
11,4723,360390065,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4724,360443008,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4725,361216539,-;init: starting service 'qvrd'...
14,4726,361219548,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4727,362626280,-;[schedu][0x1b346b31e][21:08:17.119714] wlan: [1653:I:PE] Assoc rsp RX: subtype 1 vdev 0 sys role 3 lim state 1 rssi 0 from f0:7f:06:cc:c0:40
6,4728,362627851,-;[schedu][0x1b34728f4][21:08:17.121285] wlan: [1653:I:TXRX] ol_txrx_peer_detach_sync: 3303: ol_txrx_peer_detach_sync peer ffffffc0534192e8, peer->ref_cnt 10
6,4729,362627907,-;[schedu][0x1b3472d82][21:08:17.121346] wlan: [1653:I:TXRX] ol_txrx_peer_detach: 3250: started peer_unmap_timer for peer ffffffc0534192e8
6,4730,362633843,-;[schedu][0x1b348ea7f][21:08:17.127279] wlan: [1653:I:HDD] wlan0(vdevid-0): 3e:fd:55:14:24:bf connected to f0:7f:06:cc:c0:40
6,4731,362637291,-;[schedu][0x1b349ed1c][21:08:17.130727] wlan: [1653:I:WMA] LFR3: Posting WMA_ROAM_OFFLOAD_SYNCH_CNF
6,4732,362639136,-;[schedu][0x1b34a779c][21:08:17.132574] wlan: [1653:I:WMA] [21:08:16.758000] [ROAM_TRIGGER]: VDEV[0] Reason: "DEAUTH RECEIVED" Type: 1 Reason: 1 
6,4733,362639201,-;[schedu][0x1b34a7cbe][21:08:17.132642] wlan: [1653:I:WMA] [21:08:16.758000] [ROAM_SCAN]: VDEV[0] Scan_type: PARTIAL  {2412 5660 5680 }
6,4734,362639230,-;[schedu][0x1b34a7ee1][21:08:17.132671] wlan: [1653:I:WMA]      AP BSSID           TSTAMP       CH   TY  ETP  RSSI/SCR CU%/SCR TOT_SCR
6,4735,362639257,-;[schedu][0x1b34a80d8][21:08:17.132697] wlan: [1653:I:WMA] f0:7f:06:cc:c0:4f [21:08:16.758000] 5660 P_AP    0  64/0     0/0     5436
6,4736,362639278,-;[schedu][0x1b34a8270][21:08:17.132718] wlan: [1653:I:WMA] f0:7f:06:cc:c0:40 [21:08:16.780000] 2412 R_AP   44  53/0    31/0     3886
6,4737,362639297,-;[schedu][0x1b34a83e8][21:08:17.132738] wlan: [1653:I:WMA] 6c:fa:89:54:90:90 [21:08:16.782000] 2412 C_AP   42  80/0    34/0     1009
6,4738,362639351,-;[schedu][0x1b34a87f3][21:08:17.132792] wlan: [1653:I:WMA] [21:08:17.124000] [ROAM_RESULT]: VDEV[0] SUCCESS 
6,4739,362639591,-;[soft_i][0x1b34a99d6][21:08:17.133030] wlan: [0:I:TXRX] ol_txrx_peer_release_ref: 3074: [9][0]: Deleting peer ffffffc0534192e8 ref_cnt -> 0 
6,4740,362640815,-;[schedu][0x1b34af596][21:08:17.134253] wlan: [1653:I:WMI] LFR3:OKC enabled
6,4741,362640832,-;[schedu][0x1b34af717][21:08:17.134273] wlan: [1653:I:WMI] LFR3:PMKSA caching enabled
3,4742,362645630,-;[schedu][0x1b34c5e74][21:08:17.139065] wlan: [1653:E:tdls] tdls_process_reset_all_peers: 488: tdls objects are NULL 
6,4743,362768616,-;IRQ 6: no longer affine to CPU7
3,4744,364854048,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4745,364864706,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4746,364875231,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4747,364881555,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4748,364888707,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4749,364894702,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4750,364901871,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4751,364907713,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4752,364915290,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4753,364921461,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4754,364946315,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4755,364952245,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4756,364961754,-;init: starting service 'qspmhal'...
3,4757,364988396,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4758,364994087,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4759,365002554,-;healthd: battery l=50 v=3745 t=31.9 h=2 st=2 c=-476074 fc=3812000 cc=0 chg=a
3,4760,365003701,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4761,365009486,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4762,365021910,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4763,365027605,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
31,4764,365254818,-;logd: logdr: UID=1000 GID=1000 PID=21572 n tail=50 logMask=8 pid=21548 start=0ns timeout=0ns
31,4765,365264067,-;logd: logdr: UID=1000 GID=1000 PID=21572 n tail=50 logMask=1 pid=21548 start=0ns timeout=0ns
31,4766,365281282,-;logd: logdr: UID=1000 GID=1000 PID=21572 n tail=0 logMask=8 pid=21548 start=0ns timeout=0ns
31,4767,365290238,-;logd: logdr: UID=1000 GID=1000 PID=21572 n tail=0 logMask=1 pid=21548 start=0ns timeout=0ns
14,4768,365303821,-;init: Untracked pid 21572 exited with status 0
14,4769,365307526,-;init: Untracked pid 21576 exited with status 0
14,4770,365311757,-;init: Service 'qspmhal' (pid 21548) received signal 6
14,4771,365311871,-;init: Sending signal 9 to service 'qspmhal' (pid 21548) process group...
14,4772,365312837,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 21548 in 0ms
11,4773,365409082,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4774,365472540,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4775,366254398,-;init: starting service 'qvrd'...
14,4776,366264400,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4777,368548975,-;IRQ 6: no longer affine to CPU7
6,4778,369689283,-;IRQ 6: no longer affine to CPU7
14,4779,369985237,-;init: starting service 'qspmhal'...
31,4780,370306692,-;logd: logdr: UID=1000 GID=1000 PID=21890 n tail=50 logMask=8 pid=21872 start=0ns timeout=0ns
31,4781,370331501,-;logd: logdr: UID=1000 GID=1000 PID=21890 n tail=50 logMask=1 pid=21872 start=0ns timeout=0ns
31,4782,370351781,-;logd: logdr: UID=1000 GID=1000 PID=21890 n tail=0 logMask=8 pid=21872 start=0ns timeout=0ns
31,4783,370366821,-;logd: logdr: UID=1000 GID=1000 PID=21890 n tail=0 logMask=1 pid=21872 start=0ns timeout=0ns
14,4784,370385178,-;init: Service 'qspmhal' (pid 21872) received signal 6
14,4785,370385283,-;init: Sending signal 9 to service 'qspmhal' (pid 21872) process group...
14,4786,370402292,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 21872 in 16ms
14,4787,370406589,-;init: Untracked pid 21890 exited with status 0
14,4788,370407048,-;init: Untracked pid 21894 received signal 9
11,4789,370433139,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4790,370500940,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
6,4791,370828890,-;IRQ 6: no longer affine to CPU7
14,4792,371309915,-;init: starting service 'qvrd'...
14,4793,371315460,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4794,372388890,-;IRQ 6: no longer affine to CPU7
3,4795,373020210,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4796,373025972,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4797,373038275,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4798,373044755,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4799,373054177,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4800,373060154,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4801,373066673,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4802,373072892,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4803,373080341,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4804,373086041,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4805,373100049,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4806,373105750,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4807,373154081,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4808,373159867,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4809,373168686,-;healthd: battery l=50 v=3760 t=31.7 h=2 st=2 c=-410003 fc=3812000 cc=0 chg=a
3,4810,373171046,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4811,373176737,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4812,373189675,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4813,373195380,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4814,373828655,-;IRQ 6: no longer affine to CPU7
14,4815,375023542,-;init: starting service 'qspmhal'...
31,4816,375320310,-;logd: logdr: UID=1000 GID=1000 PID=22226 n tail=50 logMask=8 pid=22223 start=0ns timeout=0ns
31,4817,375335428,-;logd: logdr: UID=1000 GID=1000 PID=22226 n tail=50 logMask=1 pid=22223 start=0ns timeout=0ns
31,4818,375357892,-;logd: logdr: UID=1000 GID=1000 PID=22226 n tail=0 logMask=8 pid=22223 start=0ns timeout=0ns
6,4819,375368547,-;IRQ 6: no longer affine to CPU7
31,4820,375388708,-;logd: logdr: UID=1000 GID=1000 PID=22226 n tail=0 logMask=1 pid=22223 start=0ns timeout=0ns
14,4821,375409954,-;init: Service 'qspmhal' (pid 22223) received signal 6
14,4822,375410086,-;init: Sending signal 9 to service 'qspmhal' (pid 22223) process group...
14,4823,375435563,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 22223 in 24ms
14,4824,375440994,-;init: Untracked pid 22226 exited with status 0
14,4825,375441622,-;init: Untracked pid 22234 received signal 9
11,4826,375460073,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
11,4827,375536253,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,4828,376028198,-;i2c_geni 4a84000.i2c: i2c error :-107
 SUBSYSTEM=platform
 DEVICE=+platform:4a84000.i2c
6,4829,376048765,-;IRQ 6: no longer affine to CPU4
14,4830,376356248,-;init: starting service 'qvrd'...
14,4831,376360365,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
14,4832,380062964,-;init: starting service 'qspmhal'...
6,4833,380288388,-;IRQ 6: no longer affine to CPU4
31,4834,380436109,-;logd: logdr: UID=1000 GID=1000 PID=22597 n tail=50 logMask=8 pid=22573 start=0ns timeout=0ns
31,4835,380444948,-;logd: logdr: UID=1000 GID=1000 PID=22597 n tail=50 logMask=1 pid=22573 start=0ns timeout=0ns
11,4836,380491654,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
31,4837,380497166,-;logd: logdr: UID=1000 GID=1000 PID=22597 n tail=0 logMask=8 pid=22573 start=0ns timeout=0ns
31,4838,380516122,-;logd: logdr: UID=1000 GID=1000 PID=22597 n tail=0 logMask=1 pid=22573 start=0ns timeout=0ns
14,4839,380533072,-;init: Service 'qspmhal' (pid 22573) received signal 6
14,4840,380533169,-;init: Sending signal 9 to service 'qspmhal' (pid 22573) process group...
14,4841,380558898,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 22573 in 25ms
14,4842,380564453,-;init: Untracked pid 22597 exited with status 0
14,4843,380564954,-;init: Untracked pid 22599 received signal 9
11,4844,381030987,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
3,4845,381185626,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4846,381191911,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4847,381205582,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4848,381211731,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4849,381218627,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4850,381224928,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4851,381232156,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4852,381237866,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4853,381244970,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4854,381250963,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4855,381266869,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4856,381272722,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4857,381324321,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4858,381330071,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4859,381338543,-;healthd: battery l=50 v=3748 t=31.9 h=2 st=2 c=-495148 fc=3812000 cc=0 chg=a
3,4860,381340480,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4861,381346179,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
6,4862,381348755,-;IRQ 6: no longer affine to CPU7
3,4863,381361123,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4864,381366810,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4865,381394345,-;init: starting service 'qvrd'...
14,4866,381397936,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4867,383069205,-;IRQ 6: no longer affine to CPU7
14,4868,385096835,-;init: starting service 'qspmhal'...
6,4869,385409366,-;IRQ 6: no longer affine to CPU7
31,4870,385469273,-;logd: logdr: UID=1000 GID=1000 PID=22955 n tail=50 logMask=8 pid=22932 start=0ns timeout=0ns
31,4871,385479818,-;logd: logdr: UID=1000 GID=1000 PID=22955 n tail=50 logMask=1 pid=22932 start=0ns timeout=0ns
31,4872,385499182,-;logd: logdr: UID=1000 GID=1000 PID=22955 n tail=0 logMask=8 pid=22932 start=0ns timeout=0ns
31,4873,385507619,-;logd: logdr: UID=1000 GID=1000 PID=22955 n tail=0 logMask=1 pid=22932 start=0ns timeout=0ns
11,4874,385516927,-;init: Control message: Could not find 'android.hardware.radio@1.4::IRadio/slot1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4875,385533273,-;init: Service 'qspmhal' (pid 22932) received signal 6
14,4876,385533364,-;init: Sending signal 9 to service 'qspmhal' (pid 22932) process group...
14,4877,385540689,-;libprocessgroup: Successfully killed process cgroup uid 1000 pid 22932 in 6ms
14,4878,385544305,-;init: Untracked pid 22955 exited with status 0
14,4879,385544697,-;init: Untracked pid 22959 exited with status 0
11,4880,386068867,-;init: Control message: Could not find 'android.hardware.secure_element@1.2::ISecureElement/SIM1' for ctl.interface_start from pid: 482 (/system/bin/hwservicemanager)
14,4881,386430982,-;init: starting service 'qvrd'...
14,4882,386433993,-;init: Created socket '/dev/socket/qvrservice', mode 666, user 1000, group 1000
6,4883,387049104,-;IRQ 6: no longer affine to CPU6
3,4884,389351168,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4885,389357113,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4886,389366009,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4887,389372414,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4888,389378971,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4889,389384687,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4890,389391962,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4891,389397684,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4892,389406216,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4893,389412448,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4894,389436076,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4895,389441867,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4896,389469817,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4897,389475511,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
12,4898,389483924,-;healthd: battery l=50 v=3767 t=31.8 h=2 st=2 c=-542297 fc=3812000 cc=0 chg=a
3,4899,389485077,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4900,389490865,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4901,389508861,-;max1720x 0-0036: SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
3,4902,389514574,-;max1720x 0-0036: POST SOC routine soc(50) pre_soc(50)
 SUBSYSTEM=i2c
 DEVICE=+i2c:0-0036
14,4903,390133212,-;init: starting service 'qspmhal'...
