##### wpa_supplicant configuration file template #####
#
# This option can be used to allow wpa_supplicant to overwrite configuration
# file whenever configuration is changed (e.g., new network block is added with
# wpa_cli or wpa_gui, or a password is changed). This is required for
# wpa_cli/wpa_gui to be able to store the configuration changes permanently.
# Please note that overwriting configuration file will remove the comments from
# it.
update_config=1
ctrl_interface=/var/run/wpa_supplicant
# IEEE 802.1X/EAPOL version
# wpa_supplicant is implemented based on IEEE Std 802.1X-2004 which defines
# EAPOL version 2. However, there are many APs that do not handle the new
# version number correctly (they seem to drop the frames completely). In order
# to make wpa_supplicant interoperate with these APs, the version number is set
# to 1 by default. This configuration value can be used to set it to the new
# version (2).
eapol_version=1
# AP scanning/selection
# By default, wpa_supplicant requests driver to perform AP scanning and then
# uses the scan results to select a suitable AP. Another alternative is to
# allow the driver to take care of AP scanning and selection and use
# wpa_supplicant just to process EAPOL frames based on IEEE 802.11 association
# information from the driver.
# 1: wpa_supplicant initiates scanning and AP selection; if no APs matching to
#    the currently enabled networks are found, a new network (IBSS or AP mode
#    operation) may be initialized (if configured) (default)
# 0: driver takes care of scanning, AP selection, and IEEE 802.11 association
#    parameters (e.g., WPA IE generation); this mode can also be used with
#    non-WPA drivers when using IEEE 802.1X mode; do not try to associate with
#    APs (i.e., external program needs to control association). This mode must
#    also be used when using wired Ethernet drivers.
# 2: like 0, but associate with APs using security policy and SSID (but not
#    BSSID); this can be used, e.g., with ndiswrapper and NDIS drivers to
#    enable operation with hidden SSIDs and optimized roaming; in this mode,
#    the network blocks in the configuration file are tried one by one until
#    the driver reports successful association; each network block should have
#    explicit security policy (i.e., only one option in the lists) for
#    key_mgmt, pairwise, group, proto variables
# When using IBSS or AP mode, ap_scan=2 mode can force the new network to be
# created immediately regardless of scan results. ap_scan=1 mode will first try
# to scan for existing networks and only if no matches with the enabled
# networks are found, a new IBSS or AP mode network is created.
ap_scan=1
# EAP fast re-authentication
# By default, fast re-authentication is enabled for all EAP methods that
# support it. This variable can be used to disable fast re-authentication.
# Normally, there is no need to disable this.
fast_reauth=1
device_name=Blaze
manufacturer=TI
model_name=Wilink
model_number=wl18xx
serial_number=12345
driver_param=use_multi_chan_concurrent=1 use_p2p_group_interface=1
# Timeout in seconds to detect STA inactivity (default: 300 seconds)
#
# This timeout value is used in P2P GO mode to clean up
# inactive stations.
p2p_go_max_inactivity=60
p2p_go_ht40=1
disassoc_low_ack=1
p2p_disabled=1