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The faling edge of the input clock
and the divided clock are aligned
after a sampling low-to-high
transition on SYSREF.

SYSREF is sampled by this sdge.
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