[IBIS Ver]   5.1
|
[Disclaimer]
             THIS IBIS MODEL HAS BEEN CREATED BY THE ALTERA
             SPICE CONVERSION PROCESS.
             THESE IBIS MODELS ARE PROVIDED "AS IS" WITH NO
             WARRANTY WHATSOEVER AND ALTERA
             SPECIFICALLY DISCLAIMS ANY IMPLIED WARRANTIES OF
             MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE,
             OR AGAINST INFRINGEMENT.
|
[File Name]  a10_rx_5p1_ads.ibs
[Date]       July 6, 2016
[File Rev]   2.0
[Source]     Intel PSG High-Speed Technology Group
|
[Notes]
  This model is distributed in two versions:
   - "a10_rx_5p1.ibs" supports those IBIS-AMI simulators, which are
     compliant to version 5.1 of the IBIS specification.
   - "a10_rx_5p1_ads.ibs" supports Keysight ADS
|
[Component]    Arria10_Rx
|
[Manufacturer] Intel Corporation
|
[Package]
R_pkg        0.001m  NA  NA
L_pkg        0.001nH  NA  NA
C_pkg        0.001pF  NA  NA
|
[Pin] signal_name model_name R_pin L_pin C_pin
  20   a10_rx_1P     a10_rx    NA    NA     NA
  21   a10_rx_1N     a10_rx    NA    NA     NA
  22   a10_rx_2P     a10_rx    NA    NA     NA
  23   a10_rx_2N     a10_rx    NA    NA     NA
  24   a10_rx_3P     a10_rx    NA    NA     NA
  25   a10_rx_3N     a10_rx    NA    NA     NA
|
[Diff Pin] inv_pin  vdiff tdelay_typ tdelay_min tdelay_max
     20       21    0.05      NA         NA         NA
     22       23    0.05      NA         NA         NA
     24       25    0.05      NA         NA         NA
|
[Model Selector] a10_rx
a10_rx_100_ads  100 Ohms differential termination.
a10_rx_85_ads   85 Ohms differential termination.
|
| ------------------------------------
|
|   model   a10_rx_85_ads
|
[Model] a10_rx_85_ads
Model_type Input
C_comp 1.2pF 1.1pF 1.3pF
Vinl = 0.025
Vinh = 0.025
[Temperature Range] 85 100 -40
[Voltage Range] 1.1 1.02 1.13
[Algorithmic Model]
Executable Windows_VisualStudio9.0.21022.8_32 a10gx_ami_rx_x86.dll a10_rx_85_5p1_ads.ami
Executable Windows_VisualStudio9.0.21022.8_64 a10gx_ami_rx_x64.dll a10_rx_85_5p1_ads.ami
Executable Linux_GCC4.8.2_32                  a10gx_ami_rx_x86.so  a10_rx_85_5p1_ads.ami
Executable Linux_GCC4.8.2_64                  a10gx_ami_rx_x64.so  a10_rx_85_5p1_ads.ami
[End Algorithmic Model]
[GND Clamp]
-1.0     -1.0      -1.0      -1.0
-0.5     -0.0282   -0.0264   -0.0300
 2.3      0.0376    0.0352    0.0400
 2.8      1.0       1.0       1.0
|
| ------------------------------------
|
|   model   a10_rx_100_ads
|
[Model] a10_rx_100_ads
Model_type Input
C_comp 1.2pF 1.1pF 1.3pF
Vinl = 0.025
Vinh = 0.025
[Temperature Range] 85 100 -40
[Voltage Range] 1.1 1.02 1.13
[Algorithmic Model]
Executable Windows_VisualStudio9.0.21022.8_32 a10gx_ami_rx_x86.dll a10_rx_5p1_ads.ami
Executable Windows_VisualStudio9.0.21022.8_64 a10gx_ami_rx_x64.dll a10_rx_5p1_ads.ami
Executable Linux_GCC4.8.2_32                  a10gx_ami_rx_x86.so  a10_rx_5p1_ads.ami
Executable Linux_GCC4.8.2_64                  a10gx_ami_rx_x64.so  a10_rx_5p1_ads.ami
[End Algorithmic Model]
[GND Clamp]
-1.0     -1.0      -1.0      -1.0
-0.5     -0.0240   -0.0231   -0.0261
 2.3      0.0320    0.0308    0.0348
 2.8      1.0       1.0       1.0
[End]
