To rule out if the problem is in DAC or ADC, can he use RF sources instead of DAC for his experiment?  
He may also try shorting both channels of ADC (reference and observation channels, I think they channel 1 and 4 for him) so that there is no phase difference

With signals at input of both channels of ADC, then increase input power and test phase difference at ADC’s output?

