

DAC8771

to Hart Out

DAC8742

Or use OPA188

To Hart in

DAC8742

Combined volt and mA output with Hart and FF/PA injection

Actually, idea from Analog Devices (CN-0278)

Would this work with the combination DAC8771 & DAC8742?

Obviously, the voltage output is not used in the loop but saves a jackplug if you need voltage output.

The whole thing should be isolated.