; Top Design: "TI_ADC12QJ1600_lib:ADC12QJ1600_TX_example:schematic"
; Netlisted using Hierarchy Policy: "Standard"

Options ResourceUsage=yes UseNutmegFormat=no EnableOptim=no TopDesignName="TI_ADC12QJ1600_lib:ADC12QJ1600_TX_example:schematic" DcopOutputNodeVoltages=yes DcopOutputPinCurrents=yes DcopOutputAllSweepPoints=no DcopOutputDcopType=0
TX:Tx_AMI1 N__2 N__5  Model="AMITx"  IbisFile="ADC12xJ_17p16.ibs" ComponentName="ADC12xJ_17p16" PinName="2p" InvPinName="2n" ModelName="ADC12xJ_17p16_slow" SetAllData=yes DataTypeSelector=1 UsePkg=yes RpkgType=1 LpkgType=1 CpkgType=1 DiffTimeDelayType=1 CcompType=1 TTgndType=1 TTpowerType=1 RgndType=1 RpowerType=1 RacType=1 CacType=1 PuDataType=1 PdDataType=1 PcDataType=1 GcDataType=1 WaveformType=1 RampType=1 IgnoreWaveforms=no VinhType=1 VinlType=1 OffDelayType=1 DisableRampWaveformSolution=yes InterpMode="linear" BitRate=17.16 Gbps Mode=0 RegisterLength=8 Encoder=0 UseControllerSampleRate=yes AMIvarName[1]="AMI_Version" AMIvarName[2]="Init_Returns_Impulse" AMIvarName[3]="GetWave_Exists" AMIvarName[4]="Max_Init_Aggressors" AMIvarName[5]="AutoInit" AMIvarName[6]="PreEmphasis" AMIvarName[7]="CornerCase" AMIvarName[8]="OutputGain" AMIvarValue[1]="6.0" AMIvarValue[2]=yes AMIvarValue[3]=no AMIvarValue[4]=2147483646 AMIvarValue[5]=1 AMIvarValue[6]=0 AMIvarValue[7]=1 AMIvarValue[8]=1.0 JitterName[1]="Tx_Dj" JitterName[2]="Tx_Rj" JitterName[3]="Tx_Sj" JitterName[4]="Tx_DCD" JitterName[5]="Tx_Sj_Frequency" JitterValue[1]=0.0 JitterValue[2]=0.0 JitterValue[3]=0.0 JitterValue[4]=0.0 JitterValue[5]=0.0 JitterType[1]="UI" JitterType[2]="UI" JitterType[3]="UI" JitterType[4]="UI" JitterType[5]="Float"
ChannelSim:ChannelSim1 Type="FastConvolution"  NumberOfBits=1000 ToleranceMode=1 EnforcePassivity=no MaxImpulseLength=1000 NumberTimePtPerUI=32 BlockSize=1024 StatusLevel=2 AntiAliasingWindow=1
#uselib "ckt" , "S4P"
S4P:SNP1  N__2 N__0 N__5 N__4 0 File="/home/a197185/TI_ADC12QJ1600/ADS/data/TX_slow.s4p" Type="touchstone" InterpMode="linear" InterpDom="" ExtrapMode="constant" Temp=27.0 CheckPassivity=0 
#uselib "ckt" , "S4P"
S4P:SNP2  N__4 N__8 N__0 N__11 0 File="/home/a197185/TI_ADC12QJ1600/ADS/data/D5aav.s4p" Type="touchstone" InterpMode="linear" InterpDom="" ExtrapMode="constant" Temp=27.0 CheckPassivity=0 
#load "python","TDM_Eye"
ComponentWithNodes:"Eye_Probe1"  N__1 Type="ModelExtractor" Module="Eye" \ 
 Save_LevelMean=no Save_HeightAtBER=no Save_Level1=yes Save_JitterRMS=no Save_Density=yes Save_RiseTime=no Save_Height=yes Save_Level0=yes Save_Width=yes Save_CheckMaskViolation=no Save_SNR=no Save_Amplitude=no Save_HeightDB=no Save_FallTime=no Save_WidthAtBER=no Save_JitterPP=no Save_Bathtub=no Save_Waveform=no Save_Contour=no Save_CrossingLevel=no Save_ClockSignal=no Save_DDR4MaskMargin=no LowerBoundary=40 UpperThreshold=80 DataRate=1.0 Gbps LowerThreshold=20 UpperBoundary=60 TimePoints=400 AmplitudeResolution=0.001 V BERWidthHeight=1e-12 TimingBathTub=0.0 V EyeMask="Eye_Probe1" UseEyeMask=0 BERContour=list(1e-12,1e-11,1e-10) ExtrapolateBER=0 VoltageBathTub=0.5 DisableTransientOutput=yes DDR4MaskWidthUI=0.0 DDR4MaskHeight=0.0 V Save_BathtubQPlot=no Save_VSRPAM4=no SetDDR4MaskCenter=0 DDR4MaskCenter=0.0 V SetDDR4MaskGroup=0 DDR4MaskGroup=1 Save_FlexDCAmeasurements=no

RX:Rx_AMI1 N__10 N__7 N__1  Model="AMIRx"  IbisFile="EEsof_Rx_Pass_Through.ibs" ComponentName="EEsof_Rx_Pass_Through" PinName="2p" InvPinName="2n" ModelName="EEsof_Rx_Pass_Through" SetAllData=yes DataTypeSelector=1 UsePkg=yes RpkgType=1 LpkgType=1 CpkgType=1 DiffTimeDelayType=1 CcompType=1 TTgndType=1 TTpowerType=1 RgndType=1 RpowerType=1 RacType=1 CacType=1 PuDataType=1 PdDataType=1 PcDataType=1 GcDataType=1 WaveformType=1 RampType=1 IgnoreWaveforms=no VinhType=1 VinlType=1 OffDelayType=1 DisableRampWaveformSolution=yes InterpMode="linear" UseControllerSampleRate=yes AMIvarName[1]="Init_Returns_Impulse" AMIvarName[2]="GetWave_Exists" AMIvarName[3]="Use_Init_Output" AMIvarName[4]="Max_Init_Aggressors" AMIvarName[5]="Gain" AMIvarValue[1]=yes AMIvarValue[2]=no AMIvarValue[3]=yes AMIvarValue[4]=2147483646 AMIvarValue[5]=1.0 JitterName[1]="Rx_Dj" JitterName[2]="Rx_Rj" JitterName[3]="Rx_Sj" JitterName[4]="Rx_DCD" JitterName[5]="Rx_Noise" JitterValue[1]=0.0 JitterValue[2]=0.0 JitterValue[3]=0.0 JitterValue[4]=0.0 JitterValue[5]=0.0 JitterType[1]="UI" JitterType[2]="UI" JitterType[3]="UI" JitterType[4]="UI" JitterType[5]="Float"
R:R1  N__10 N__7 R=100 Ohm Noise=yes 
#uselib "ckt" , "S4P"
S4P:SNP3  N__11 N__10 N__8 N__7 0 File="/home/a197185/TI_ADC12QJ1600/ADS/data/fr4_100mm.s4p" Type="touchstone" InterpMode="linear" InterpDom="" ExtrapMode="constant" Temp=27.0 CheckPassivity=0 
